Index: DamEngine/trunk/doc/Dam Engine - Functional Design/UseWBIPipingKernel.tex
===================================================================
diff -u -r1557 -r1560
--- DamEngine/trunk/doc/Dam Engine - Functional Design/UseWBIPipingKernel.tex	(.../UseWBIPipingKernel.tex)	(revision 1557)
+++ DamEngine/trunk/doc/Dam Engine - Functional Design/UseWBIPipingKernel.tex	(.../UseWBIPipingKernel.tex)	(revision 1560)
@@ -133,6 +133,8 @@
 \end{align}
 
 In the WBI piping kernel is an assumption made for the distribution ot the piezomeric head in the aquifer at different x locations. This requires a leakage length $\lambda$. This is a user defined parameter (new to DAM).
+Parameter used in DAM is \textit{\textcolor[rgb]{0.65,0.16,0}{SlopeDampingPiezometricHeightPolderSide}. remark Irene (2-5-2018): Perhaps it is an option to calculate the leakage length from this parameter to avoid adding new parameters to DAM. This belongs to the extended version of the WBI-piping connection, as adaption in the UI is needed.
 
+
 \section{Determination of soil parameters}\label{sec:DeterminationSoilParameters}
 The kernel requires
