Index: DamEngine/branches/DamEngine 19.3/doc/Dam Engine - Functional Design/UseStabKernel.tex
===================================================================
diff -u -r3736 -r3737
--- DamEngine/branches/DamEngine 19.3/doc/Dam Engine - Functional Design/UseStabKernel.tex	(.../DamEngine 19.3 wrong/doc/Dam Engine - Functional Design/UseStabKernel.tex)	(revision 3736)
+++ DamEngine/branches/DamEngine 19.3/doc/Dam Engine - Functional Design/UseStabKernel.tex	(.../DamEngine 19.3/doc/Dam Engine - Functional Design/UseStabKernel.tex)	(revision 3737)
@@ -44,20 +44,28 @@
 
 Ad 2 Client defined generation\newline
 The client defines the dimensions; number of gridpoints and distance between the points. The \ProgramName defines the position of the grid depending on the characteristic points:
-For Bishop and for the active grid of LiftVan the left (outside) bottom corner is situated at the surfaceline in the middle of the crest (distance between outer- and innercrest). The right bottom corner of the passive grid of LiftVan is situated above the most right x co-ordinate where uplift occurs. With the restriction that the left bottom corner can not be situated left of the x co-ordinate of the DikeToePolder.	
+For Bishop and for the left grid of LiftVan the left (outside) bottom corner is situated at the surfaceline in the middle of the crest (distance between outer- and innercrest). The right bottom corner of the right (inside) grid of LiftVan is situated above the most right x co-ordinate where uplift occurs. With the restriction that the left bottom corner can not be situated left of the x co-ordinate of the DikeToePolder.	
 	
 \subsection{Tangent lines generation}
 \label{sec:TangentLinesGeneration}
+For the models Bishop and LiftVan a tangent lines must be generated.
 
-For the Bishop model only automatic generation is used.\newline
-The tangent lines are placed from the minimum Z-value of the surface line until 0.5 m below the upper geometry point of the lowest aquifer. The distance between the tangent lines is 0.25 m.
+There are two options:
+\begin{enumerate}
+	\item automatic generation
+	\item client defined generation
+\end{enumerate}
 
-For LiftVan there are two client defined methods\newline
-Distance defined - Naar opgave afstand\newline
+Ad 1 Automatic generation\newline
+Bishop\newline
+-to described-\newline
+Liftvan\newline
+-to described-\newline
+
+Ad 2 Client defined\newline
+For Bishop calcuations the tangent lines can not be defined by the client.\newline
 For LiftVan the client must provide the distance between the tangent lines.
-The lower tangent line is always situated 0.5 m below the boundary of the upper aquifer. The tangent lines are drawn with the given distance until the minimum Z value of the passive grid.\newline
-On boundary - Op laagscheidingen (default)\newline
-On every boundary of the subsoil layer.
+The lower tangentline is always situated 5.0 m below the upper geometry point of the lowest aquifer. The tangentlines are drawn with the given distance until the upper tangent line is situated above the Z DikeToeAtPolder.
 
 \subsection{Calculation area}
 \label{sec:CalculationArea}
