Index: DamEngine/trunk/doc/Dam Engine - Functional Design/UseStabKernel.tex
===================================================================
diff -u -r1279 -r1337
--- DamEngine/trunk/doc/Dam Engine - Functional Design/UseStabKernel.tex	(.../UseStabKernel.tex)	(revision 1279)
+++ DamEngine/trunk/doc/Dam Engine - Functional Design/UseStabKernel.tex	(.../UseStabKernel.tex)	(revision 1337)
@@ -34,13 +34,42 @@
 \label{sec:GridGeneration}
 	
 For the models Bishop and LiftVan a calculation grid must be generated.
+There are two options:
+\begin{enumerate}
+	\item automatic generation
+	\item user defined generation
+\end{enumerate}
+
+Ad 1 Automatic generation\newline
+Bishop\newline
+-to described-\newline
+Liftvan\newline
+-to described-\newline
+
+Ad 2 User defined generation\newline
 The user defines the dimensions; number of gridpoints and distance between the points. The DAM engine defines the position of the grid depending on the characteristic points:
 For Bishop and for the left grid of LiftVan the left bottom corner is situated at the surfaceline in the middle of the crest (distance between outer- and innercrest). The right bottom corner of the right grid of LiftVan is situated above the most right x co-ordinate where uplift occurs. With the restriction that the left bottom corner can not be situated left of the x co-ordinate of the DikeToePolder.	
 	
 \subsection{Tangent lines generation}
 \label{sec:TangentLinesGeneration}
-For Bishop calcuations the tangent lines are always situated at the layer boundaries (automatic). For LiftVan the tangent lines can either be situated automatic or specified. This is user-defined.
-When specified, the user (client of DAM-Engine) must provide the distance between the tangent lines, \textcolor[rgb]{1,0,0}{\textsl{Distance tangent lines (UV) }}.
+For the models Bishop and LiftVan a tangent lines must be generated.
+
+There are two options:
+\begin{enumerate}
+	\item automatic generation
+	\item user defined generation
+\end{enumerate}
+
+Ad 1 Automatic generation\newline
+Bishop\newline
+-to described-\newline
+Liftvan\newline
+-to described-\newline
+
+Ad 2 User defined\newline
+For Bishop calcuations the tangent lines are generated automatic. 
+
+For LiftVan the user (client of DAM-Engine) must provide the distance between the tangent lines, \textcolor[rgb]{1,0,0}{\textsl{Distance tangent lines (UV) }}.
 The lower tangentline is always situated 5.0 m below the upper geometry point of the lowest aquifer. The tangentlines are drawn with the given distance until the upper tangent line is situated above the Z;DikeToeAtPolder.
 
 \subsection{Calculation area}
