{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["segment input","unit descr.","sedimentaire facieseenheden","Global application layer types","Items","GLobal appl layers out","TOut"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"segment input","index":0,"n_rows":12459,"n_cols":36,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[1,0,2,0],[2,17,2,19],[3,17,3,19],[2,27,2,29],[3,27,3,29],[3,9,3,10],[3,12,3,13],[3,15,3,16]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["for use of ScenarioGenerator .exe: create an \"input\" and \"output\" directory in the workspace directorywith this EXCEL workbook",null,null,null,null,null,null,null,null,null,null,null,{"$f":"COLUMN()","v":13}]
["ring","Segment",null,"Global Scenario",null,null,null,"Sedimentary Facies Unit"]
[null,null,null,null,null,null,null,null,"prob","pos","alt","prob","pos","alt",null,null,null,"base"]
[null,null,null,null,null,null,null,null,"0-100","first order",null,"0-100","second order",null,"0-100","third order",null,"m-NAP"]
[null,"Iseg",null,null,null,"P_Gs_zg",null,"SFU","Psfu0","Tsfu0","Csfu0","Psfu1","Tsfu1","Csfu1","Psfu2","Tsfu2","Csfu2","Hsfr","Hsfi","Hsfa",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Remarks"]
[]
[1,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,null,null,null,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,1,2,null,null,null,null,null,null,7.5,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling met klei"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.3,1,3,null,null,null,null,null,null,2.5,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mg_zf",1,2,1,null,null,null,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"P_Om_zf",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combinatie van Eem Formatie en Fm. van Drente en Peelo"]
[]
[2,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,-1.5,-1.75,-1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Duinzand"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,2,1,null,null,null,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"H_Mr_kz",0.05,2,2,null,null,null,null,null,null,4,3.5,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling met klei"]
[null,null,null,null,null,null,null,"H_Mg_zf",1,3,1,null,null,null,null,null,null,22.5,21,23]
[null,null,null,null,null,null,null,"P_Om_k",1,4,1,null,null,null,null,null,null,32,29,36]
[null,null,null,null,null,null,null,"P_Om_zf",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[2,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,null,null,null,null,null,null,2.5,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,1,2,null,null,null,null,null,null,2.5,1.5,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling met klei"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.3,1,3,null,null,null,null,null,null,2.5,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mg_zf",1,2,1,null,null,null,null,null,null,22.5,21,23]
[null,null,null,null,null,null,null,"P_Om_k",1,3,1,null,null,null,null,null,null,32,29,36]
[null,null,null,null,null,null,null,"P_Om_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[2,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,1,null,null,null,null,null,null,5.5,4.5,6.5]
[null,null,null,null,null,null,null,"H_Mr_kz",0.5,1,2,null,null,null,null,null,null,5.5,4.5,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling met klei"]
[null,null,null,null,null,null,null,"H_Mg_zf",1,2,1,null,null,null,null,null,null,22.5,21,23]
[null,null,null,null,null,null,null,"P_Om_k",1,3,1,null,null,null,null,null,null,32,29,36]
[null,null,null,null,null,null,null,"P_Om_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[2,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,1,null,null,null,null,null,null,5.5,4.5,6.5]
[null,null,null,null,null,null,null,"H_Mr_kz",0.2,1,2,null,null,null,null,null,null,5,4.5,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling met klei"]
[null,null,null,null,null,null,null,"H_Mg_zf",1,2,1,null,null,null,null,null,null,22.5,21,23]
[null,null,null,null,null,null,null,"P_Om_k",1,3,1,null,null,null,null,null,null,32,29,36]
[null,null,null,null,null,null,null,"P_Om_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[2,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,null,null,null,null,null,null,2.5,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,1,2,null,null,null,null,null,null,2.5,1.5,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling met klei"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.3,1,3,null,null,null,null,null,null,2.5,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mg_zf",1,2,1,null,null,null,null,null,null,32,30,34]
[null,null,null,null,null,null,null,"P_Om_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[3,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,-0.5,-1,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Duinzand, lokaal dun (dunner dan 50cm dik) duinveen aanwezig"]
[null,null,null,null,null,null,null,"H_Mp_k",1,2,1,null,null,null,null,null,null,1.5,0.5,3.75]
[null,null,null,null,null,null,null,"H_Mg_zf",1,3,1,null,null,null,null,null,null,28,27,30]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,30,29,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keileem, inclusief dunne Urk-klei onder keileem"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[3,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0.25,0,0.5]
[null,null,null,null,null,null,null,"H_Mg_zf",0.6,2,1,1,1,1,null,null,null,28,27,30]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.6,2,1,1,2,1,null,null,null,30,29,31]
[null,null,null,null,null,null,null,"H_Mg_zf",0.4,2,2,null,null,null,null,null,null,32,30,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holoceen zand, beneden ~ 27m-NAP ook Eem-zand"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[3,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mg_zf",1,1,1,null,null,null,null,null,null,34,32,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holoceen zand, beneden ~ 27m-NAP ook Eem-zand"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,40,40,40]
[]
[3,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,1,1,1,1,1,null,null,null,0.5,0,3]
[null,null,null,null,null,null,null,"H_Mg_zf",0.85,1,1,1,2,1,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"H_Mg_zf",0.15,1,2,null,null,null,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,40,40,40]
[]
[3,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,1,1,1,1,null,null,null,1.75,0,3]
[null,null,null,null,null,null,null,"H_Mg_zf",0.9,1,1,1,2,1,null,null,null,27,25,28]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,1,2,1,1,1,null,null,null,9,6.5,12]
[null,null,null,null,null,null,null,"H_Mg_zf",0.1,1,2,1,2,1,null,null,null,27,25,28]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,2,1,null,null,null,null,null,null,30.5,29,32]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[3,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2.5]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,2,1,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Duinzand, lokaal dun (dunner dan 50cm dik) duinveen aanwezig"]
[null,null,null,null,null,null,null,"H_Mp_k",1,2,1,null,null,null,null,null,null,3,2,3.5]
[null,null,null,null,null,null,null,"H_Mg_zf",1,3,1,null,null,null,null,null,null,27,25,28]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,30.5,29,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keileem, inclusief dunne Urk-klei onder keileem"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[4,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2.5]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,5,1,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Duinzand met sandflat zand"]
[null,null,null,null,null,null,null,"H_Mp_k",1,2,1,null,null,null,null,null,null,11,9,12]
[null,null,null,null,null,null,null,"H_Mg_zk",1,3,1,null,null,null,null,null,null,19,18,20]
[null,null,null,null,null,null,null,"H_Ova_zm",1,4,1,null,null,null,null,null,null,21,19,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Erosierelict Drente-Schaarsbergen,Eem,grof Holoceen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,5,1,null,null,null,null,null,null,32,31,33]
[null,null,null,null,null,null,null,"P_Rg_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[4,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2.5]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,5,1,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Duinzand met sandflat zand"]
[null,null,null,null,null,null,null,"H_Mg_zk",1,3,1,null,null,null,null,null,null,19,18,20]
[null,null,null,null,null,null,null,"H_Ova_zm",1,4,1,null,null,null,null,null,null,21,19,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Erosierelict Drente-Schaarsbergen,Eem,grof Holoceen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,5,1,null,null,null,null,null,null,32,31,33]
[null,null,null,null,null,null,null,"P_Rg_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[5,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bij duingebied haven maaiveldhoogtes tot 3 m NAP"]
[null,null,null,null,null,null,null,"H_Ova_zf",0.1,1,1,null,null,null,null,null,null,2.5,1,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S09D00302 voorbeeld van strandzandlaag op fijn zandige getijdeafzettingen (met klei); S09D00299 voorbeeld van matig grove getijdezanden liggend op een Pleistocene ondoorlatende laag op 23 m -NAP"]
[null,null,null,null,null,null,null,"H_Ova_zf",0.9,1,2,null,null,null,null,null,null,0,0,0]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,2,1,1,1,1,null,null,null,4,3.5,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms 1 m klei aan de top."]
[null,null,null,null,null,null,null,"H_Mr_kz",0.8,2,1,1,2,1,null,null,null,6,4,7]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,2,1,1,3,1,null,null,null,23,20,25]
[null,null,null,null,null,null,null,"H_Mg_zf",0.2,2,2,null,null,null,null,null,null,23,20,25]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,3,1,1,1,1,null,null,null,25,23,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Klei nooit dikker dan 4 m."]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,2,null,null,null,null,null,null,40,40,40]
[]
[5,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In oostelijk deel ligt de dijk tegen een duin aan. Sonderingen S09D00251 (schoon zand) en S09D00263 (gelaagde opbouw)"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,null,null,null,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,1,2,null,null,null,null,null,null,6.5,6,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling met klei"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.3,1,3,null,null,null,null,null,null,2.5,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mg_zf",1,2,1,null,null,null,null,null,null,18,16,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"in het westelijk deel schoon zand tot -5m NAP"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[5,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S09D00306"]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,0.85,0.75,1]
[null,null,null,null,null,null,null,"H_Mp_zf",1,2,1,null,null,null,null,null,null,1.25,1,1.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,3,1,1,1,1,null,null,null,2,1.25,2.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,3,1,1,2,1,null,null,null,2.5,1.75,3.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,3,2,null,null,null,null,null,null,2.5,1.75,3.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,4,1,1,1,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.2,4,1,1,2,1,null,null,null,8,6,9]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.8,4,2,null,null,null,null,null,null,8,6,9]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,15,11.75,18.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Drachten, zeer compact zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,24,22,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[5,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S09D00287 (keileem tussen -2m en -25m NAP) en S09E00035 (keileem tussen -8 en -14m NAP)"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.25,1,1,1,1,1,null,null,null,0.75,0.5,1]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.25,1,1,1,2,1,null,null,null,8,3.75,11.75]
[null,null,null,null,null,null,null,"H_Mp_zf",0.25,1,2,1,1,1,null,null,null,0.75,0.5,1]
[null,null,null,null,null,null,null,"H_Vbv_v",0.25,1,2,1,2,1,null,null,null,1.25,1,1.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.25,1,2,1,3,1,null,null,null,8,3.75,11.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.25,1,3,1,1,1,null,null,null,1.25,1,1.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.25,1,3,1,2,1,null,null,null,8,3.75,11.75]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.25,1,4,null,null,null,null,null,null,8,3.75,11.75]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.6,2,1,null,null,null,null,null,null,23,20,25]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.35,2,2,null,null,null,null,null,null,16,14,18]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.05,2,3,1,1,1,null,null,null,15,11.75,18.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Drachten, zeer compact zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.05,2,3,1,2,1,null,null,null,24,22,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[5,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S09E00022 (boven-1.26m is het dijklichaam)"]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,1,0.5,2]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,2,1,1,1,1,null,null,null,4.5,2.75,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms veel organisch stof"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.7,2,1,1,2,1,null,null,null,5.5,3.25,7]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,2,2,null,null,null,null,null,null,6,5,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms veel organisch stof"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,12,11,13.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,15,13,16]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Overwegend matig grof zand, incidenteel met dunne (dunner dan 2m dik) kleilagen rondom -20 en -27m NAP)"]
[]
[5,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S04G00004"]
[null,null,null,null,null,null,null,"H_Mg_zf",0.3,1,1,1,1,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Ml_ko",0.3,1,1,1,3,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Vbv_v",0.3,1,1,1,4,1,null,null,null,9,8.5,9.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.3,1,1,1,5,1,null,null,null,12,11,13.5]
[null,null,null,null,null,null,null,"H_Mg_zf",0.5,1,2,1,1,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,2,1,2,1,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"H_Ml_ko",0.5,1,2,1,3,1,null,null,null,12,11,13]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,1,2,1,4,1,null,null,null,12.5,11.5,13.5]
[null,null,null,null,null,null,null,"H_Mg_zf",0.2,1,3,1,1,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,3,1,2,1,null,null,null,14,12,16]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,2,1,null,null,null,null,null,null,15,13,16]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,18,16,19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Drachten"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,20,18,21]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0,-1.1000000000000001,2]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,1,null,null,null,null,null,null,4,4,5.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,2,null,null,null,null,null,null,6,6,8]
[null,null,null,null,null,null,null,"H_Mp_ko",1,3,1,null,null,null,null,null,null,6.5,5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandvoorkomens uitgesloten"]
[null,null,null,null,null,null,null,"H_Mp_k",1,4,1,null,null,null,null,null,null,13.5,12,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelmatig met dunne Basisveenlaag aan de basis"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,5,1,null,null,null,null,null,null,25,22,35]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,5,2,1,1,1,null,null,null,16,15.5,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,2,1,2,1,null,null,null,25,22,35]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,6,2,null,null,null,null,null,null,40,40,40]
[]
[6,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S03H00019: getijdegeulopvulling op klei"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2,-0.25,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.35,2,1,1,1,1,null,null,null,3,2,3.5]
[null,null,null,null,null,null,null,"H_Mg_zm",0.35,2,1,0.9,2,1,null,null,null,7.5,7,9]
[null,null,null,null,null,null,null,"H_Mg_zm",0.35,2,1,0.1,2,2,1,1,1,4.5,4,6]
[null,null,null,null,null,null,null,"H_Mp_ko",0.35,2,1,0.1,2,2,1,2,1,5.5,4,6]
[null,null,null,null,null,null,null,"H_Mp_ko",0.65,2,2,0.5,1,1,null,null,null,3.25,2.5,4.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.65,2,2,0.5,1,2,null,null,null,3.25,2.5,4.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.65,2,2,1,2,1,null,null,null,3.75,3,4.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen meestal niet dikker dan 0.5 m"]
[null,null,null,null,null,null,null,"H_Mp_k",0.65,2,2,1,3,1,null,null,null,5.5,4,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,3,1,null,null,null,null,null,null,13.25,12.25,15]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,3,2,1,1,1,null,null,null,7.5,6.5,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.15,3,2,1,2,1,null,null,null,11,10,13.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.15,3,2,1,3,1,null,null,null,13.25,12.25,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelmatig met dunne Basisveenlaag aan de basis"]
[null,null,null,null,null,null,null,"P_Rg_zg ",1,6,1,null,null,null,null,null,null,25,22,35]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,7,2,null,null,null,null,null,null,40,40,40]
[]
[6,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,1,null,null,null,null,null,null,2,1.5,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,2,null,null,null,null,null,null,2,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mp_ko",1,2,1,null,null,null,null,null,null,4.5,3.75,4.75]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,1,null,null,null,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Mp_ko",1,4,1,null,null,null,null,null,null,5.5,3,7.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,5,1,1,1,1,null,null,null,8,7.5,11]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,5,1,1,2,1,null,null,null,13,12.25,13]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,5,2,null,null,null,null,null,null,13,12.25,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de basis regelmatig dunne basisveenlaag"]
[null,null,null,null,null,null,null,"P_Rg_zg ",1,6,2,null,null,null,null,null,null,30,30,30]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,7,1,null,null,null,null,null,null,40,40,40]
[]
[6,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,1,1,null,null,null,null,null,null,11.5,8.5,12]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.75,1,1,null,null,null,2.25,1,5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,2,0.25,1,2,null,null,null,2.25,1,5]
[null,null,null,null,null,null,null,"H_Mp_ko",0.95,1,2,1,2,1,null,null,null,4.5,3,5.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.95,1,2,1,3,1,null,null,null,5.25,3.75,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal 0.5-0.8 m dik, zelden dikker dan 1 m"]
[null,null,null,null,null,null,null,"H_Mp_k",1,2,1,null,null,null,null,null,null,11.5,8.5,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de basis regelmatig dunne basisveenlaag"]
[null,null,null,null,null,null,null,"P_Rg_zg ",0.8,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg ",0.1,3,2,1,1,1,null,null,null,13,12,17]
[null,null,null,null,null,null,null,"P_Om_k",0.1,3,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg ",0.1,3,3,1,1,1,null,null,null,13,12,17]
[null,null,null,null,null,null,null,"P_Om_k",0.1,3,3,1,2,1,null,null,null,15,14,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,3,3,1,3,1,null,null,null,40,40,40]
[]
[6,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal bovenkant enkele meters antropogeen verstoord"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2,1.5,3]
[null,null,null,null,null,null,null,"H_Vhv_v",0.1,2,1,null,null,null,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,2,2,0.1,1,1,null,null,null,4,2.5,5]
[null,null,null,null,null,null,null,"H_Mp_ko",0.9,2,2,0.9,1,2,null,null,null,4,2.5,5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,2,2,1,2,1,null,null,null,4.5,3.5,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de basis regelmatig dunne basisveenlaag"]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,3,1,null,null,null,null,null,null,9,6,12]
[null,null,null,null,null,null,null,"H_Mp_ko",0.05,3,2,null,null,null,null,null,null,10.5,9.5,11.5]
[null,null,null,null,null,null,null,"P_Om_k",0.4,4,1,1,1,1,null,null,null,16,11,25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg ",0.6,4,2,1,1,1,null,null,null,11,8,18]
[null,null,null,null,null,null,null,"P_Om_k",0.6,4,2,1,2,1,null,null,null,25,20,35]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,4,2,1,3,1,null,null,null,40,40,40]
[]
[6,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,1,1,null,null,null,null,null,null,4,1,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.15,1,2,1,1,1,null,null,null,2.5,1.5,5]
[null,null,null,null,null,null,null,"H_Mp_ko",0.15,1,2,1,2,1,null,null,null,4,2,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,2,1,1,1,1,null,null,null,7,5,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.15,2,1,1,2,1,null,null,null,10.5,7.5,13]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,2,2,null,null,null,null,null,null,10.5,7.5,13]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.25,2,3,1,1,1,null,null,null,6,5,11]
[null,null,null,null,null,null,null,"H_Mg_zk",0.25,2,3,1,2,1,null,null,null,13,11,17]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.25,2,3,1,3,1,null,null,null,16,11,20]
[null,null,null,null,null,null,null,"P_Om_k",0.95,3,1,1,1,1,null,null,null,30,12,35]
[null,null,null,null,null,null,null,"P_Rg_zg ",0.95,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Om_k",0.05,3,2,1,1,1,null,null,null,16,11,20]
[null,null,null,null,null,null,null,"P_Rg_zg ",0.05,3,2,1,2,1,null,null,null,40,40,40]
[]
[6,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"zeer variabel door woonwijk"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,3,2.5,4.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,2,1,null,null,null,null,null,null,5,4,8]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,2,2,null,null,null,null,null,null,5,3,8]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,1,null,null,null,null,null,null,6,4,7.5]
[null,null,null,null,null,null,null,"H_Mp_k",1,4,1,null,null,null,null,null,null,8,7,12]
[null,null,null,null,null,null,null,"H_Vhv_v",1,5,1,null,null,null,null,null,null,9,7,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S07F00606 voorbeeld van zeer diepe top Pleistoceen met daaronder grof zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.2,6,2,null,null,null,null,null,null,25,20,40]
[]
[6,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.35,1,1,null,null,null,null,null,null,3,2.5,3.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.65,1,2,null,null,null,null,null,null,4.5,4,6]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,5.5,4.5,8.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7.5,5,8]
[null,null,null,null,null,null,null,"P_Om_k",0.5,4,1,1,1,1,null,null,null,20,8,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S08A00096 voorbeeld van dunne Boxtel op Peelo klei op grof zand op -25"]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S08A00130 voorbeeld van grove Peelo"]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld in noordelijk deel hoger dan in zuidelijk deel"]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,1,1,1,1,1,null,null,null,3,1.25,5.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,1,1,1,2,1,null,null,null,4.25,2.25,7.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,1,1,1,3,1,null,null,null,9,7,15]
[null,null,null,null,null,null,null,"H_Mp_k",0.2,1,2,null,null,null,null,null,null,9,7,15]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,9.5,8,11.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,11.5,9,12]
[null,null,null,null,null,null,null,"P_Om_k",0.1,6,1,null,null,null,null,null,null,20,15,30]
[null,null,null,null,null,null,null,"P_Gs_zg",0.9,6,1,null,null,null,null,null,null,40,40,40]
[]
[6,10,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"maaiveld variabel"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,5,3,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inclusief basisveen"]
[null,null,null,null,null,null,null,"H_Ml_ko",1,2,1,null,null,null,null,null,null,6.5,4,13]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,1,null,null,null,null,null,null,7.5,7,8]
[null,null,null,null,null,null,null,"H_Ml_ko",1,4,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,12,9,15]
[null,null,null,null,null,null,null,"P_Om_k",0.1,6,1,null,null,null,null,null,null,20,16,30]
[null,null,null,null,null,null,null,"P_Gs_zg",0.9,6,2,null,null,null,null,null,null,40,40,40]
[]
[6,11,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"maaiveld in noordelijk deel rond nul, zuidelijk rond 1 m NAP"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0,-0.5,4.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,2,1,0.5,1,1,null,null,null,4.5,3.5,6.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,2,1,0.5,1,2,null,null,null,4.5,3.5,6.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,2,1,1,2,1,null,null,null,7.5,6.5,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,2,1,1,3,1,null,null,null,9.5,8.5,10.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,2,2,0.5,1,1,null,null,null,3.5,2,4.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,2,2,0.5,1,2,null,null,null,3.5,2,4.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,2,2,1,2,1,null,null,null,5.5,4.75,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,2,2,1,3,1,null,null,null,8,6.5,9]
[null,null,null,null,null,null,null,"P_Om_k",0.9,3,1,1,1,1,null,null,null,20,16,30]
[null,null,null,null,null,null,null,"P_Om_k",0.9,3,1,1,2,1,null,null,null,35,16,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.9,3,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.1,3,2,null,null,null,null,null,null,40,40,40]
[]
[6,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"maaiveld variabel: in noorden rond 1.75, in het zuiden rond 0.25 m NAP"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Mp_zf",0.2,2,1,null,null,null,null,null,null,3,1,4]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,2,2,null,null,null,null,null,null,5,4.75,5.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,5.5,5.25,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,8,6.5,9]
[null,null,null,null,null,null,null,"P_Om_k",0.5,5,1,null,null,null,null,null,null,20,16,30]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,13,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2,1,2.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.8,2,1,null,null,null,null,null,null,3,2,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.2,2,2,null,null,null,null,null,null,3,2.75,4]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,4.75,4.25,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,7,6,9]
[null,null,null,null,null,null,null,"P_Om_k",0.4,5,1,null,null,null,null,null,null,20,16,30]
[null,null,null,null,null,null,null,"P_Gs_zg",0.6,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,14,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2.75,2.5,5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,5.25,3,6.25]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7.5,6.5,9]
[null,null,null,null,null,null,null,"P_Gs_zg",0.9,4,1,null,null,null,null,null,null,16,15,22]
[null,null,null,null,null,null,null,"P_Om_k",0.1,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,15,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"plaatselijk maaiveld tot -1 m NAP"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1.5,0.25,3]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,2.5,1.5,4.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Om_k",0.1,4,1,null,null,null,null,null,null,20,13,30]
[null,null,null,null,null,null,null,"P_Gs_zg",0.9,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,1,null,null,null,null,null,null,-0.25,-0.5,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk depressieopvulling, dan maximaal 1 meter veen"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,1,2,null,null,null,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Om_k",0.1,4,1,null,null,null,null,null,null,20,13,30]
[null,null,null,null,null,null,null,"P_Gs_zg",0.9,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,17,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,1,null,null,null,null,null,null,4.5,4,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,2,1,1,1,1,null,null,null,10,8,11]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,2,1,1,2,1,null,null,null,11,8,13]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,2,2,null,null,null,null,null,null,11,8,13]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,3,1,1,1,1,null,null,null,13.25,13,13.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.3,3,1,1,2,1,null,null,null,13.75,13.25,15]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,3,2,null,null,null,null,null,null,16,15,18]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,19,18,20]
[null,null,null,null,null,null,null,"P_Om_k",0.2,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.8,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,1,1,null,null,null,null,null,null,-0.5,-1,2]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,2,null,null,null,null,null,null,-0.5,-1,2]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,1,null,null,null,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,2,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Mg_zf",1,3,1,null,null,null,null,null,null,13,12,16]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,4,1,1,1,1,null,null,null,14.75,13.5,15]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,4,1,1,2,1,null,null,null,15,14,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Het basisveen is nooit dikker dan 1 m."]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,4,1,1,3,1,null,null,null,23,22,25]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,4,2,1,1,1,null,null,null,19.5,17,20]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,4,2,1,2,1,null,null,null,20,18,21]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,4,2,1,3,1,null,null,null,23,22,25]
[null,null,null,null,null,null,null,"P_Om_k",0.2,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.8,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,19,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.65,1,1,null,null,null,null,null,null,-0.5,-1,2]
[null,null,null,null,null,null,null,"H_Mp_k",0.35,1,2,null,null,null,null,null,null,-0.5,-1,2]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,4.5,4,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S03G00087 voorbeeld van overgang van kleiig naar schoon getijdegeulenzand"]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,3,1,1,1,1,null,null,null,10.5,8,19]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,3,1,1,2,1,null,null,null,18.5,17,20]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,3,2,null,null,null,null,null,null,18.5,17,20]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,18.75,18,20]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,21,19.5,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Het basisveen is nooit dikker dan 1 m."]
[null,null,null,null,null,null,null,"P_Ova_sd",0.35,6,1,1,1,1,null,null,null,23,20,25]
[null,null,null,null,null,null,null,"P_Gs_zg",0.35,6,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.65,6,2,null,null,null,null,null,null,40,40,40]
[]
[6,20,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,1,1,null,null,null,null,null,null,2.5,-1,3.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,2,null,null,null,null,null,null,2.5,-1.75,3.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,1,null,null,null,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,2,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Mg_zf",1,3,1,null,null,null,null,null,null,18.5,17.5,19.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,4,1,null,null,null,null,null,null,25,19.5,28]
[null,null,null,null,null,null,null,"H_Mp_k",0.2,4,2,null,null,null,null,null,null,20.5,19,22]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,25,21,27]
[null,null,null,null,null,null,null,"P_Ova_sd",0.35,6,1,1,1,1,null,null,null,30,25,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.35,6,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.65,6,2,null,null,null,null,null,null,40,40,40]
[]
[6,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,1,1,null,null,null,null,null,null,2.5,-1,3.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,2,null,null,null,null,null,null,2.5,-1.75,3.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,2,1,1,1,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,2,1,1,2,1,null,null,null,15.5,10,16]
[null,null,null,null,null,null,null,"H_Mg_zk",0.15,2,2,1,1,1,null,null,null,19,19,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S03D00056 voorbeeld van basis geul op 9 m -NAP met daaronder klei en basisveen"]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,2,3,1,1,1,null,null,null,15.5,10,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S03D00088 voorbeeld van diep ingesneden Holocene geul tot in het Pleistoceen"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.05,2,3,1,2,1,null,null,null,16,10.5,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen is nooit dikker dan 1 m."]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,19,11,21]
[null,null,null,null,null,null,null,"P_Ova_sd",0.35,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.65,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,22,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,1,null,null,null,null,null,null,0.5,-1.5,2]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,2,null,null,null,null,null,null,0.5,-1.5,2]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,8,7,13]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,9,7.5,12]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,9.25,7.75,12.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen is nooit dikker dan 0.5 m."]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,10.75,9.25,13.75]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Keileem op potklei"]
[]
[6,23,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,1,null,null,null,null,null,null,2,-1.25,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,2,null,null,null,null,null,null,2,-1.25,2.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,2,1,0.5,1,1,null,null,null,9.5,8,11.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,2,1,0.5,1,2,null,null,null,13.5,12.5,14.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,2,1,1,2,1,null,null,null,15,14.75,15]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,2,2,null,null,null,null,null,null,15,14.75,15]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,15.25,13.5,15.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen is nooit dikker dan 0.5 m en altijd aanwezig"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,16.75,13.75,21]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Westkant Eem Formatie, Oostkant potklei"]
[]
[6,24,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,1,1,null,null,null,null,null,null,3,-1.25,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,1,2,null,null,null,null,null,null,3,-1.25,3.5]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,26,20,30]
[null,null,null,null,null,null,null,"P_Ova_sd",0.15,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Mg_zk",0.85,3,2,null,null,null,null,null,null,40,40,40]
[]
[6,25,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,1,null,null,null,null,null,null,11.5,9,13]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,1,2,null,null,null,null,null,null,11.5,9,13]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,30,25,36]
[null,null,null,null,null,null,null,"P_Om_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[6,26,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.75]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,1,null,null,null,null,null,null,6.5,6,8]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,13,12.5,15]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,13.5,12.5,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen is nooit dikker dan 0.5 m."]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,15.5,14.5,16.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.15,5,1,1,1,1,null,null,null,20,18,22]
[null,null,null,null,null,null,null,"P_Rg_zm",0.15,5,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.85,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,27,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.75]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,1,null,null,null,null,null,null,6.5,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S02G00044 voorbeeld van getijdegeulzandpakketten met veel kleilaagjes in het onderste pakket en weinig kleilaagjes in het bovenste pakket. Ligt op potklei."]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,9.5,8,12]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,12,11,13]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,39.5,20,40]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,28,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mv is fictief: dijklichaam van de Afsluitdijk, met ondergrond van oorspronkelijke afzettingen op ongeveer oorspronkelijk niveau"]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,1.75,1.5,2.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,2,1,1,1,1,null,null,null,5.5,4.5,7]
[null,null,null,null,null,null,null,"H_Vbv_v",0.3,2,1,1,2,1,null,null,null,6,5,7.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,2,2,null,null,null,null,null,null,7.5,6,9]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.7,3,1,1,1,1,null,null,null,10.5,10,11]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.7,3,1,1,2,1,null,null,null,14,13,15.25]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.3,3,2,null,null,null,null,null,null,14,13,15.25]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,20,19.75,20.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,5,1,1,1,1,null,null,null,24,22,25]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,5,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.8,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,29,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.4,1,1,1,1,1,null,null,null,0.5,-0.25,1.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,1,2,1,null,null,null,1.5,0.75,2]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,2,null,null,null,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,10,8,12]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,3,1,null,null,null,null,null,null,16,15,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de basis lokaal dunne (dunner dan 1m dik) veenlaag"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,4,1,null,null,null,null,null,null,23,16,24]
[null,null,null,null,null,null,null,"P_Mg_zm",0.1,4,2,null,null,null,null,null,null,26,24,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal kleilagen tot 2 m dik."]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal kleilagen tot 2 m dik."]
[]
[6,30,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S05D00089"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,null,null,null,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,2,null,null,null,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,2,1,1,1,1,null,null,null,7,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de basis lokaal dunne (dunner dan 1m dik) veenlaag"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.95,2,1,1,2,1,null,null,null,16,15,17]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,2,2,null,null,null,null,null,null,18.5,16,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diepe holocene geul"]
[null,null,null,null,null,null,null,"P_Mg_zm",0.3,3,1,null,null,null,null,null,null,22,21,24]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,3,2,null,null,null,null,null,null,24,22,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,3,3,1,1,1,null,null,null,19,18,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-klei"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.4,3,3,1,2,1,null,null,null,23,22,24.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-klei"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,31,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,1,1,1,null,null,null,7.5,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S05D00321; hierbovenop nog tot 4m dik Antropogeen"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,1,1,1,2,1,null,null,null,17,15,18]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,2,1,1,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,1,2,1,null,null,null,14.5,12,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat kleilagen dunner dan  1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,2,1,1,1,1,null,null,null,18,16,20]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,2,1,1,2,1,null,null,null,22,20,25]
[null,null,null,null,null,null,null,"P_Mg_zm",0.1,2,2,null,null,null,null,null,null,22,21,24]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Omvat lokaal ook (dunner dan 2m) dunne Urk-klei onder de keileem"]
[]
[6,32,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S05D00319"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,1,1,1,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,1,1,2,1,null,null,null,5,4,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"regelmatig minder dan  1m veen aan basis"]
[null,null,null,null,null,null,null,"P_Rbk_zm",0.8,1,1,1,3,1,null,null,null,10,9,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenste 5 m soms met conusweerstanden meer dan40 Mpa"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.8,1,1,1,4,1,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Mg_zm",0.8,1,1,1,5,1,null,null,null,17,16,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-zand"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,1,1,1,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,1,2,1,2,1,null,null,null,17,16,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat kleilagen dunner dan  1.5 m"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.4,2,1,null,null,null,null,null,null,23,21,26]
[null,null,null,null,null,null,null,"P_Ova_sd",0.6,2,2,1,1,1,null,null,null,19.5,15,21.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-klei"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.6,2,2,1,2,1,null,null,null,23,21,26]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[6,33,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S05G00621"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,4,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Overwegend zandig"]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,2,null,null,null,null,null,null,12,8,14]
[null,null,null,null,null,null,null,"H_Mg_zm",0.9,3,1,1,1,1,0.5,1,1,18.5,17.25,19.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,3,1,1,1,1,0.5,1,2,18.5,17.25,19.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,3,1,1,2,1,null,null,null,21.75,21,22.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-klei"]
[null,null,null,null,null,null,null,"H_Mg_zm",0.1,3,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,26.75,26.5,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,5,2,1,1,1,null,null,null,32,30,33]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,5,2,1,2,1,null,null,null,40,40,40]
[]
[6,34,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S05G00017"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,1.5,1,2.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,2,1,1,1,1,null,null,null,7,4.5,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat kleilagen dunner dan  1.5 m"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.3,2,1,1,2,1,null,null,null,7.5,5,9.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.3,2,1,1,3,1,null,null,null,21,20,22]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,2,1,1,1,null,null,null,12,9,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat kleilagen dunner dan  1.5 m"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.5,2,2,1,2,1,null,null,null,21,20,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal aan de basis Eem-zand tot 2m dik"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,2,3,null,null,null,null,null,null,25,21,27]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,26,25.5,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,35,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S05F00027; oostgrens niet heel zeker, kan ook 2500m westelijker liggen. Zie kaart Peter Vos"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,1,0,1.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,2,1,0.4,1,1,null,null,null,18,15,23.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Complex pakket met veel afwisseling zand,klei,leem in diepte en lateraal"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,2,1,0.6,1,2,1,1,1,13,11,14]
[null,null,null,null,null,null,null,"H_Mg_zm",0.95,2,1,0.6,1,2,1,2,2,19,13,23.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.95,2,1,1,2,1,null,null,null,24,21,28.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,2,2,null,null,null,null,null,null,24,21,28.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,36,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S05F00260"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,0,-1,1]
[null,null,null,null,null,null,null,"H_Mg_zk",0.45,2,1,1,1,1,null,null,null,4,2.75,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.45,2,1,0.1,2,1,null,null,null,8,7.5,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal met dun (dunner dan 50cm) veenlaagje"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.45,2,1,0.9,2,2,1,1,1,6.5,5.5,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal met dun (dunner dan 50cm) veenlaagje"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.45,2,1,0.9,2,2,1,2,1,7,6,7.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.45,2,1,1,4,1,null,null,null,10,9,15]
[null,null,null,null,null,null,null,"H_Mg_zk",0.45,2,2,1,1,1,null,null,null,4,2.75,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.45,2,2,0.1,2,1,null,null,null,8,7.5,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal met dun (dunner dan 50cm) veenlaagje"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.45,2,2,0.9,2,2,1,1,1,8,6,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal met dun (dunner dan 50cm) veenlaagje"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.45,2,2,0.9,2,2,1,2,1,9,8,10]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.45,2,2,1,4,1,null,null,null,10,9,15]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,2,3,null,null,null,null,null,null,12,10,16]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,3,1,null,null,null,null,null,null,13,11,16]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,37,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,1,1,1,null,null,null,0,-0.5,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kwelderklei"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,2,1,null,null,null,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.85,2,2,1,1,1,null,null,null,4,3,4.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,2,2,1,2,1,null,null,null,5,4.5,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Weinig humeus, soms meer zandig, incidenteel dunne (dunner dan .25m dik) veenlaagjes"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.85,2,2,1,3,1,null,null,null,5.5,4,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"basisveen meestal 0.5 - 1 m dik, soms tot 2 m dik"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,3,1,null,null,null,null,null,null,9,8.5,10]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,3,2,1,1,1,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.5,3,2,1,2,1,null,null,null,10,9.5,11]
[null,null,null,null,null,null,null,"P_Ova_sd",0.7,4,1,null,null,null,null,null,null,33,29,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Klei, Formatie van Urk, Laagpakket van Tynje (mariene klei) en potklei"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.3,4,2,null,null,null,null,null,null,33,29,39]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Urk, Laagpakket van Veenhuizen, overwegend fluviatiel zand"]
[]
[6,38,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,1,1,1,null,null,null,0,-0.5,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kwelderklei"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,2,1,1,2,1,1,1,1,2.75,2,3.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,2,1,1,3,1,1,2,1,3.25,2.25,3.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.7,2,1,1,4,1,1,3,1,4,3.25,5.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Weinig humeus, soms meer zandig"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,2,2,1,1,1,null,null,null,1,0,2]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,2,2,1,2,1,null,null,null,5,3.25,6]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,1,4,1,null,null,null,5.5,4.5,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.7,4,1,1,1,1,null,null,null,7.75,5,8]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.7,4,1,1,2,1,null,null,null,9.5,8,10]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.3,4,2,null,null,null,null,null,null,9.5,8,10]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,13,12,14.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Urk, Laagpakket van Veenhuizen, overwegend fluviatiel zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,6,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Urk, Laagpakket van Tynje, mariene klei als het op Potklei ligt, dieper dan 40m"]
[]
[6,39,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,1,1,1,1,null,null,null,0,-0.5,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kwelderklei"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.4,1,2,1,2,1,null,null,null,-0.25,-0.5,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kwelderzand"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,2,1,1,1,null,null,null,2.5,2,4]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,2,1,2,1,null,null,null,3,2.5,4.5]
[null,null,null,null,null,null,null,"H_Ml_ko",1,4,2,1,3,1,null,null,null,5,4.5,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Weinig humeus, soms meer zandig"]
[null,null,null,null,null,null,null,"H_Vbv_v",1,5,2,1,4,1,null,null,null,5.5,5,11.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.4,6,1,1,1,1,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.4,6,1,1,2,1,null,null,null,9.5,8.5,11]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.6,6,2,null,null,null,null,null,null,9.5,8.5,11]
[null,null,null,null,null,null,null,"P_Ova_sd",0.7,7,1,1,1,1,null,null,null,14,12,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Urk, Laagpakket van Tynje, mariene klei"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,7,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Urk, Laagpakket van Tynje op Formatie van Urk, Laagpakket van Veenhuizen, beide grof fluviatiel zand"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.3,7,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Peelo, matig fijn zand"]
[]
[6,40,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,null,null,null,null,null,null,3.5,3,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top kwelderzand, lokaal kwelderklei"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,2,1,1,1,null,null,null,2.5,2,3.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top kwelderzand, lokaal kwelderklei"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,1,2,1,2,1,null,null,null,3,2.5,4.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,5,4,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Getijdenplaatengeul, sporadisch onderin dun (dunner dan 50cm dik) basisveen"]
[null,null,null,null,null,null,null,"H_Mg_zk",1,3,1,null,null,null,null,null,null,9.5,8,10.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.2,4,1,1,1,1,null,null,null,10.5,10,11.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.2,4,1,1,2,1,null,null,null,12.5,12,13]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.55000000000000004,4,2,null,null,null,null,null,null,12.5,12,13.5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.25,4,3,null,null,null,null,null,null,17,14,19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holocene laguneklei-opvulling in beekdal"]
[null,null,null,null,null,null,null,"P_Om_zf",0.85,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Om_k",0.15,5,2,1,1,1,null,null,null,20,15,30]
[null,null,null,null,null,null,null,"P_Om_zf",0.15,5,2,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Peelo, matig fijn zand"]
[]
[6,41,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,null,null,null,null,null,null,3.5,3,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top kwelderzand, lokaal kwelderklei"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,1,2,1,1,1,null,null,null,2.25,1.75,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top kwelderzand, lokaal kwelderklei"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,1,2,1,2,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,2,1,1,1,1,null,null,null,5,2.5,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Getijdenplaatengeul"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,2,1,1,2,1,null,null,null,25,20,27]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,2,2,1,1,1,null,null,null,5,2.5,7]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,2,2,1,2,1,null,null,null,8.5,7.75,9.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.05,2,2,1,3,1,null,null,null,8.75,8,9.5]
[null,null,null,null,null,null,null,"P_Om_zf",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Peelo en Fm. Van Urk Lp van Tynje, matig fijn zand"]
[]
[6,42,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,1,1,1,1,null,null,null,25,20,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lauwerszee geul"]
[null,null,null,null,null,null,null,"P_Om_zf",0.3,1,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Peelo, matig fijn zand"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.35,1,2,1,1,1,null,null,null,10,8,12]
[null,null,null,null,null,null,null,"P_Om_zf",0.35,1,2,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Peelo en Fm. Van Urk Lp van Tynje, matig fijn zand"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,3,1,1,1,null,null,null,9.25,8.75,10.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.05,1,3,1,2,1,null,null,null,9.5,9,11]
[null,null,null,null,null,null,null,"P_Om_zf",0.05,1,3,1,3,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Peelo en Fm. Van Urk Lp van Tynje, matig fijn zand"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,4,1,1,1,null,null,null,15,13,20]
[null,null,null,null,null,null,null,"P_Om_k",0.3,1,4,1,2,1,null,null,null,25,20,30]
[null,null,null,null,null,null,null,"P_Om_zf",0.3,1,4,1,3,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Peelo, matig fijn zand"]
[]
[6,43,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S10B00117"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,3.5,2.5,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer zware klei, hoogwad"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,5,4.5,5.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Matig zware klei met wat zandlaagjes"]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,5.5,5,6.25]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,10.5,10,11]
[null,null,null,null,null,null,null,"P_Rbk_zm",1,5,1,null,null,null,null,null,null,14,13,15.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Schoner zand met hogere weerstand"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,6,1,null,null,null,null,null,null,20,19.75,20.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,7,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat mogelijk lokale dunne kleilagen"]
[]
[6,44,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S10B00121"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,3.5,2.5,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer zware klei, hoogwad"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,2,1,1,1,1,null,null,null,5,4.5,5.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.2,2,1,1,2,1,null,null,null,5.5,5,6.25]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,2,1,1,3,1,null,null,null,10.5,10,11]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,2,2,null,null,null,null,null,null,12,11,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Onderdiepte onduidelijk"]
[null,null,null,null,null,null,null,"P_Rbk_zm",1,3,1,null,null,null,null,null,null,14,13,15.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Schoner zand met hogere weerstand"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,20,19.75,20.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat mogelijk lokale dunne kleilagen"]
[]
[6,45,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,3.5,2.5,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer zware klei, hoogwad"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,5,4.5,5.75]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,5.5,5,6.25]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,8.5,7,10]
[null,null,null,null,null,null,null,"P_Rbk_zm",1,5,1,null,null,null,null,null,null,16,14,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Schoner zand met hogere weerstand, aan basis soms 1 m compact veen"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.2,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.8,6,2,1,1,1,null,null,null,20,19.75,20.5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.8,6,2,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat plaatselijk dunne (dunner dan  1 m) kleilagen en plaatselijk kleiige lagen (dunner dan  4 m)"]
[]
[6,46,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mp_zf",0.9,1,1,0.15,1,1,1,1,1,1.5,1,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,1,0.15,1,1,1,2,1,3.75,2.25,4.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,1,0.85,1,2,null,null,null,3.75,2.25,4.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,1,1,1,2,1,null,null,null,5.25,2,5.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal 1-1.5 m dik"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.1,1,2,0.15,1,1,1,1,1,1.5,1,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,2,0.15,1,1,1,2,1,5,4,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,2,0.85,1,2,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,2,1,2,1,null,null,null,7,5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal 1-1.5 m dik"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,3,1,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Rbk_zm",1,4,1,null,null,null,null,null,null,17,16,18]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,23.5,22,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-klei"]
[null,null,null,null,null,null,null,"P_Mg_zm",1,6,1,null,null,null,null,null,null,30,28,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,7,1,1,1,1,null,null,null,36,35,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk-klei"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,7,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk-zand"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,7,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk-zand"]
[]
[6,47,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S10D00092"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.95,1,1,0.4,1,1,1,1,1,1,0.5,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,1,0.4,1,1,1,2,1,3,1,3.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,1,0.6,1,2,null,null,null,3,1,3.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,2,1,null,null,null,3.75,2.5,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.95,1,1,0.8,3,1,1,1,1,4.5,4.25,4.75]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.95,1,1,0.8,3,1,1,2,1,9,6,10.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat ook organische lagen"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.95,1,1,0.2,3,2,null,null,null,9,6,10.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat ook organische lagen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,2,1,1,1,null,null,null,4.5,4,6]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.05,1,2,1,2,1,null,null,null,9,6,10.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat ook organische lagen"]
[null,null,null,null,null,null,null,"P_Gs_zg",0.3,2,1,null,null,null,null,null,null,16,14,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"zeer variabel in korrelgrootte"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.7,2,2,null,null,null,null,null,null,16,14,18]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat plaatselijk dunne (dunner dan  1 m) kleilagen en plaatselijk kleiige lagen (dunner dan  4 m), plaatselijk bijna geheel klei"]
[]
[6,48,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S10D00106"]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,1,null,null,null,null,null,null,2.5,1.25,3.25]
[null,null,null,null,null,null,null,"H_Mp_zf",0.1,1,2,1,1,1,null,null,null,1,0.5,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,2,1,2,1,null,null,null,2.5,1.25,3.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3.5,2.5,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,5.25,4.5,6]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.75,4,1,1,1,1,null,null,null,9.5,9,10.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.75,4,1,1,2,1,null,null,null,12.5,11.5,14]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.25,4,2,null,null,null,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,25.5,24,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.3,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.7,6,2,1,1,1,null,null,null,34.5,33,36]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,6,2,1,2,1,null,null,null,40,40,40]
[]
[6,49,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S10D00113; in polder maaiveld rond 0.50m-NAP"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.4,1,1,1,1,1,null,null,null,0.5,0,1.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.4,1,1,1,2,1,null,null,null,1.5,1.25,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,2,null,null,null,null,null,null,1.5,1.25,2.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3,2.75,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"veen meestal 1 - 2 m dik"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,5,4.75,5.25]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.75,4,1,1,1,1,null,null,null,10,9,12]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.75,4,1,1,2,1,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.25,4,2,null,null,null,null,null,null,15.5,14,16]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,26,24,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Fm. Van Drachten en Lp. Van Tynje in Fm. Van Urk. Kan lokaal dunne kleilagen bevatten."]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,6,2,1,1,1,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,6,2,1,2,1,null,null,null,40,40,40]
[]
[6,50,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S10D00019, Maaiveld direct achter de dijk sterk verlaagd door afgraving."]
[null,null,null,null,null,null,null,"H_Mp_zf",0.4,1,1,1,1,1,null,null,null,2.5,2,2.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.4,1,1,1,2,1,null,null,null,3.25,3,3.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,1,1,1,3,1,null,null,null,3.75,3.5,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"veen meestal 0.5 - 1.5 m dik"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.4,1,1,1,4,1,null,null,null,4.25,4,4.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.2,1,2,null,null,null,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.4,1,3,1,1,1,null,null,null,2.25,2,2.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,1,3,1,2,1,null,null,null,3.5,3.25,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.4,1,3,1,3,1,null,null,null,4.25,4,4.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,2,1,1,1,1,null,null,null,10.5,10,12]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.2,2,1,1,2,1,null,null,null,13,11.5,14.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.8,2,2,null,null,null,null,null,null,13.5,12,15]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,22.5,20,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,4,2,1,1,1,null,null,null,25,20,28]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,1,2,1,null,null,null,40,40,40]
[]
[6,51,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00024, Maaiveld direct achter de dijk sterk verlaagd door afgraving."]
[null,null,null,null,null,null,null,"H_Mp_zf",0.1,1,1,1,1,1,null,null,null,1,0.75,1.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,1,1,2,1,null,null,null,2.25,1.25,2.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,0.9,1,1,null,null,null,2.25,1.25,2.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,0.1,1,2,null,null,null,2.75,2.5,3]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3,2.5,3.25]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,5,4.25,5.5]
[null,null,null,null,null,null,null,"P_Rbk_zm",1,4,1,null,null,null,null,null,null,11,9,15.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat plaatselijk klei en kleiige lagen 0.5 - 2 m dikte"]
[null,null,null,null,null,null,null,"P_Gs_zg",0.2,5,1,null,null,null,null,null,null,17,12.5,19]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.8,5,2,null,null,null,null,null,null,17,12.5,19]
[null,null,null,null,null,null,null,"P_Rg_zf",1,6,1,null,null,null,null,null,null,26,24,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[6,52,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00036; Maaiveld direct achter de dijk sterk verlaagd door afgraving."]
[null,null,null,null,null,null,null,"H_Mp_zf",0.1,1,1,1,1,1,null,null,null,0.75,0.5,1]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,1,1,2,1,null,null,null,1.5,0.75,2.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,null,null,null,null,null,null,1.5,0.75,2.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3.25,2.75,3.75]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,4,3.75,5.5]
[null,null,null,null,null,null,null,"P_Rbk_zm",0.8,4,1,1,1,1,null,null,null,17,12.5,19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat plaatselijk klei en kleiige lagen 0.5 - 2 m dikte"]
[null,null,null,null,null,null,null,"P_Rbk_zm",0.2,4,2,1,1,1,null,null,null,12,11,15]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,4,2,1,2,1,null,null,null,17,15,25]
[null,null,null,null,null,null,null,"P_Gs_zg",1,5,1,null,null,null,null,null,null,25,23,29]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[6,53,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2,1.5,2.75]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3.5,3.25,3.75]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,3,1,null,null,null,null,null,null,7,5.25,10.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenin plaatselijk dunne dekzand-bedekking"]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,4,1,null,null,null,null,null,null,9,8,15]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.5,4,2,null,null,null,null,null,null,12,8.5,15]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,1,null,null,null,null,null,null,15,12,18]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,2,null,null,null,null,null,null,15,12,18]
[null,null,null,null,null,null,null,"P_Rg_zf",1,6,1,null,null,null,null,null,null,23,21,25]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[6,54,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00078"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,0.8,1,1,1,1,1,2.5,1.5,3]
[null,null,null,null,null,null,null,"H_Vbv_v",1,1,1,0.8,1,1,1,2,1,3.5,1.5,4.5]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,0.2,1,2,1,1,1,4,3.5,5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.9,2,1,1,1,1,null,null,null,8,6,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenin plaatselijk dunne dekzand-bedekking"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,2,1,1,2,1,null,null,null,12,10,15]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.1,2,2,1,1,1,null,null,null,9.5,6,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"met veel dikke (meer dan 2m) kleilagen "]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,55,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00100"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.9,2,1,1,1,1,null,null,null,8,6,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenin plaatselijk dunne dekzand-bedekking"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,2,1,1,2,1,null,null,null,12,10,15]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.1,2,2,1,1,1,null,null,null,9.5,6,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"met veel dikke (meer dan 2m) kleilagen "]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,56,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00103; Roode Klif, dus maaiveld loopt op tot 10m+NAP"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,1,1,null,null,null,null,null,null,-5,-5.5,-4]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,57,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00118"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,1.75,1.25,2.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.9,3,1,1,1,1,null,null,null,8,6,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenin plaatselijk dunne dekzand-bedekking"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,3,1,1,2,1,null,null,null,12,10,15]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.1,3,2,1,1,1,null,null,null,9.5,6,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"met veel dikke (meer dan 2m) kleilagen "]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,58,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00114; Kleine keileembult in dijktrace"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.7,1,1,null,null,null,null,null,null,3,2,4]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.3,1,2,null,null,null,null,null,null,9.5,8,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie sondering S15B00113"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,2,1,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[6,59,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00122"]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,1,1,null,null,null,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Ova_zm",0.15,1,2,1,1,1,null,null,null,1.5,1.25,1.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.15,1,2,1,2,1,null,null,null,2.5,2,2.75]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,4,1.5,5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,3,1,null,null,null,null,null,null,20,18,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Fm. van Boxtel en Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,3,2,1,1,1,null,null,null,6.5,6,8]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.5,3,2,1,2,1,null,null,null,8.5,6.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,60,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00126"]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,1,null,null,null,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Ova_zm",0.4,1,2,null,null,null,null,null,null,2.25,1.5,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Strandzandje, plaatselijk zeer grof met grindjes"]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3.5,2.5,4]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,5.5,3.75,7]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,9.5,8,11]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,17,15,19]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[6,61,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00139"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1,0.75,1.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,2,1,null,null,null,null,null,null,1.75,1.25,3]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,3,1,null,null,null,null,null,null,7.5,3.5,13]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,14,12,16]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,62,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00137"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.85,1,1,1,1,1,null,null,null,-3.5,-3.75,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.85,1,1,1,2,1,null,null,null,7.5,5.5,12]
[null,null,null,null,null,null,null,"P_Rg_zf",0.85,1,1,1,3,1,null,null,null,14,12,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.15,1,2,null,null,null,null,null,null,14,12,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Fm. van Boxtel en Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,40,40,40]
[]
[6,63,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00019"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1,0.75,1.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,2,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,16,14,18]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,64,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00126"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0.75,0.5,1]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,2,0.75,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"veen 0.5 - 1.5 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,3,1,1,1,1,null,null,null,3.5,1.25,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.6,3,1,1,2,1,null,null,null,9,6.5,13]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,3,1,1,3,1,null,null,null,16,14,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.4,3,2,null,null,null,null,null,null,16,14,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Fm. van Boxtel en Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,65,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00023; in oostelijk deel maaiveld rond +1m NAP"]
[null,null,null,null,null,null,null,"H_Vhv_v",1,1,1,null,null,null,null,null,null,1,0,1.5]
[null,null,null,null,null,null,null,"P_Gs_zg",0.1,2,1,null,null,null,null,null,null,8,6,12]
[null,null,null,null,null,null,null,"P_Rg_zf",0.9,2,2,null,null,null,null,null,null,1.5,0.25,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,3,1,null,null,null,null,null,null,8,2,13.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,16,14,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[6,66,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15B00028"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,1,1,null,null,null,null,null,null,16,14,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,40,40,40]
[]
[6,67,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Ova_zm",0.5,1,1,null,null,null,null,null,null,1,0.25,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Strandzandje, plaatselijk zeer grof met grindjes"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,1,2,null,null,null,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,2,1,null,null,null,null,null,null,7,4,8]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,16,14,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,68,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-4.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15E00034"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,1,1,null,null,null,null,null,null,-4,-4.75,-3.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,2,1,null,null,null,null,null,null,6,4.75,9]
[null,null,null,null,null,null,null,"P_Gs_zg",0.1,2,1,null,null,null,null,null,null,7,6,9]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,15,13,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,69,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15E00041"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1.25,0.5,2]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,2,1,2.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,3.5,1.5,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,8,6,12]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,5,1,1,1,1,null,null,null,12,9,17]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,5,1,1,2,1,null,null,null,14.5,12.5,16.5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,5,2,null,null,null,null,null,null,14.5,12.5,16.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[6,70,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15E00071; maaiveld varieerd tussen +1m en -0.5m NAP"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0,-0.75,1]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Rg_zm",0.85,3,1,1,1,1,null,null,null,1,-0.25,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.85,3,1,1,2,1,null,null,null,7,4.75,9.75]
[null,null,null,null,null,null,null,"P_Rg_zf",0.85,3,1,1,3,1,null,null,null,11.5,10,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.15,3,2,null,null,null,null,null,null,11.5,10,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Fm. van Boxtel en Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,71,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15F00056"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1.25,0.75,2.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,2.25,1.25,2.75]
[null,null,null,null,null,null,null,"P_Rg_zf",0.85,3,1,1,1,1,null,null,null,2.75,1.5,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.85,3,1,1,2,1,null,null,null,4,3.5,5.5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.85,3,1,1,3,1,null,null,null,11.5,10,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.15,3,2,null,null,null,null,null,null,11.5,10,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Fm. van Boxtel en Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[6,72,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.75]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1.75,1,2.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,12,10,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Boxtel"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.1,4,1,1,1,1,null,null,null,13,12,15]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,4,1,1,2,1,null,null,null,16,14,20]
[null,null,null,null,null,null,null,"P_Rg_zg",0.1,4,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.9,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,73,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15F00108"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2.5,1,3.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,4.5,3,5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,16.5,14.5,17]
[null,null,null,null,null,null,null,"P_Ova_sd",0.6,5,1,1,1,1,null,null,null,21,19,30]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,5,1,1,2,1,null,null,null,32,30,35]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,5,2,null,null,null,null,null,null,32,30,35]
[null,null,null,null,null,null,null,"P_Rg_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[6,74,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S15F00118; boven 0m NAP opgebrachtmateriaal"]
[null,null,null,null,null,null,null,"H_Ova_zf",0.3,1,1,1,1,1,null,null,null,0.5,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dunne Strandzand laag"]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,1,1,2,1,null,null,null,1.5,0.5,2.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,2,null,null,null,null,null,null,1.5,0.75,2.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3,2,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"veen ongeveer 0.5 - soms 1.5 m dik, vaak met dunne, dunner dan 0.3 m, kleiinsluitingen bovenaan"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.8,4,1,1,1,1,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,75,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan westzijde segment hierbovenop antropogeen (oprit); S15F00120"]
[null,null,null,null,null,null,null,"H_Ova_zf",0.45,1,1,1,1,1,null,null,null,2,1.5,2.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Strandzandje"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.45,1,1,1,2,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.45,1,2,1,1,1,null,null,null,1.5,1.25,2]
[null,null,null,null,null,null,null,"H_Vbv_v",0.45,1,2,1,2,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"H_Ova_zf",0.1,1,3,1,1,1,null,null,null,1.5,1.25,1.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,3,1,2,1,null,null,null,2,1.75,3]
[null,null,null,null,null,null,null,"H_Mg_zf",0.1,1,3,1,3,1,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"P_Rg_zf",1,2,1,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.8,3,1,1,1,1,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,2,null,null,null,null,null,null,40,40,40]
[]
[6,76,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S15F00051"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,1,1,2,1,null,null,null,2.75,2,3.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.85,1,2,1,1,1,null,null,null,1.5,0.75,2]
[null,null,null,null,null,null,null,"H_Vbv_v",0.85,1,2,1,2,1,null,null,null,2.75,2,3.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,4,null,null,null,null,null,null,2,1.75,3]
[null,null,null,null,null,null,null,"P_Rg_zf",1,2,1,null,null,null,null,null,null,5,4,7]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,3,1,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,3,2,null,null,null,null,null,null,9,8,14]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Fm. Van Drachten en Urk-Tynje"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,4,2,1,1,1,null,null,null,17,15,18]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,4,2,1,2,1,null,null,null,20,19,21]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,4,2,1,3,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Urk"]
[]
[6,77,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S16A00006"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,1,1,2,1,null,null,null,2.75,2,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,2,1,1,1,null,null,null,1.25,0.75,1.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.6,1,2,1,2,1,null,null,null,2.75,2,3.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,4,null,null,null,null,null,null,2,1.75,3]
[null,null,null,null,null,null,null,"P_Rg_zf",0.9,2,1,1,1,1,null,null,null,17,15,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lokaal dunne dunner dan 1m leem en of veenlaagjes"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,2,1,1,2,1,null,null,null,20,19,21]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,2,1,1,3,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Urk"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,2,2,1,1,1,null,null,null,40,40,40]
[]
[6,78,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,1,1,1,1,null,null,null,1.25,1,2.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,2,1,null,null,null,4,1.75,5.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basis soms sterk lemig"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,2,null,null,null,null,null,null,4.5,3,6]
[null,null,null,null,null,null,null,"P_Rg_zf",1,2,1,null,null,null,null,null,null,10,7,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 1m"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 2m"]
[]
[6,79,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0.75,0.5,1.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,3.5,1.25,4.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basis heel erg soms sterk lemig"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,8.5,7,10.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 1m"]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,4,1,null,null,null,null,null,null,13,12,14]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,17.5,16,19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drachten"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.8,6,1,1,1,1,null,null,null,18.5,16.5,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,6,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 2m"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 2m"]
[]
[6,80,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0.75,0.5,1.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,2.75,1.25,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basis heel erg soms sterk lemig"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,5,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 1m"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.66,4,1,null,null,null,null,null,null,15,12.5,18]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.34,4,2,1,1,1,null,null,null,13.75,13,14.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.34,4,2,1,2,1,null,null,null,15,12.5,18]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,18,16,19]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.8,6,1,1,1,1,null,null,null,18.5,16.5,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,6,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 2m"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 2m"]
[]
[6,81,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,1,1,1,1,1,null,null,null,1,0.75,1.5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.4,1,1,1,2,1,null,null,null,3.5,2,4]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,1,2,null,null,null,null,null,null,3.5,2,4]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,2,1,null,null,null,null,null,null,4.5,1,7]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.1,2,2,null,null,null,null,null,null,11,7,12]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,16,15,17]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,4,1,null,null,null,null,null,null,20,19,22.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne klei,leemlagen zeer lokaal dunner dan 2m"]
[]
[6,82,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk"]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,1.75,1.5,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,2,1,0.2,1,1,1,1,1,5,4.75,5.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,2,1,0.8,1,2,1,1,1,4.5,4,4.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.8,2,1,0.8,1,2,1,2,1,4.75,4.25,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,2,1,1,2,1,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.8,2,1,1,3,1,null,null,null,9.25,8.5,11]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,2,2,1,1,1,null,null,null,6,5,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,2,2,1,2,1,null,null,null,10,9,12]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,13.5,12,14.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,20,19.75,20.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,5,1,1,1,1,null,null,null,26,23,29]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,5,1,1,2,1,null,null,null,29,27,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 3.5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,5,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,83,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S10B00033 voor diepe dunne keileem onder dikke Boxtel, S10B00045 voor dikke keileem"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,null,null,null,null,null,null,2,1.5,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms aan de top een meerbodem"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.4,1,2,null,null,null,null,null,null,2,1.5,3]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,5,4,7]
[null,null,null,null,null,null,null,"P_Rg_zf",0.3,3,1,1,1,1,null,null,null,13.5,12,14.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.3,3,1,1,2,1,null,null,null,20,19.75,20.5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,3,2,1,1,1,null,null,null,18.5,16,19.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.5,3,2,1,2,1,null,null,null,20,19.75,20.5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.2,3,3,null,null,null,null,null,null,22,21,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal dunne (dunner dan .50m) kleilagen; onderin matig grof"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,1,1,1,null,null,null,26,23,29]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,4,1,1,2,1,null,null,null,29,27,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 3.5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,null,null,null,null,null,null,40,40,40]
[]
[6,84,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S10B00043"]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,3.5,3,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"soms kleiige top"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,1,1,1,1,1,1,1,5,4,7]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,2,1,0.5,2,1,1,1,1,9,8,10]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.5,2,1,0.5,2,2,1,1,1,10,9,12]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,2,1,1,1,null,null,null,13,10,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Onderin soms klei met veel zandlagen"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.9,3,1,1,1,1,null,null,null,13.5,12,14.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.9,3,1,1,2,1,null,null,null,15.75,14.5,16]
[null,null,null,null,null,null,null,"P_Rg_zf",0.1,3,2,1,1,1,null,null,null,17,16,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,24,23,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer compact Drachten-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,1,1,1,1,null,null,null,29,27,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 3.5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,2,null,null,null,null,null,null,40,40,40]
[]
[6,85,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; Zeer heterogeen segment; S10A00026 en S10A00028"]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,3.5,3,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"soms kleiige top"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,2,1,1,1,1,null,null,null,11.25,11,11.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.3,2,1,1,2,1,null,null,null,11.75,11.5,12]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.3,2,1,1,3,1,null,null,null,14,9,14.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,2,2,null,null,null,null,null,null,14.5,10,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Onderin soms klei met veel zandlagen"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.1,3,1,1,1,1,null,null,null,15,13,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.1,3,1,1,2,1,null,null,null,16.75,15.5,17]
[null,null,null,null,null,null,null,"P_Rg_zf",0.9,3,2,1,1,1,null,null,null,17.5,17,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,18,17,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Compact Drachten-zand op Urk Tynje-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,5,1,1,1,1,null,null,null,21,19,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, dunner dan  5 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,5,1,1,2,1,null,null,null,39,37,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,5,2,null,null,null,null,null,null,39,37,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat lokale kleilagen dunner dan  2 m dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei"]
[]
[6,86,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; Zeer heterogeen segment; S10A00041 en S10C00003"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.5,1,1,null,null,null,null,null,null,6,5,6.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,2,null,null,null,null,null,null,6,5,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meerbodem, soms met detrituslaagjes"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,1,null,null,null,null,null,null,7,7,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandige kleilaag"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,2,null,null,null,null,null,null,9,7,10]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,14,11,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,17,14,21]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,27,25,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,6,1,1,1,1,null,null,null,31,28,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,6,1,1,2,1,null,null,null,38,37,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,6,2,1,1,1,null,null,null,38,37,40]
[null,null,null,null,null,null,null,"P_Ova_sd",1,7,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei"]
[]
[6,87,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S10C00010 en S10C00017"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.95,1,1,null,null,null,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,2,null,null,null,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,2,1,null,null,null,null,null,null,7.5,7,8]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,2,2,1,1,1,null,null,null,7,6,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Geultje"]
[null,null,null,null,null,null,null,"H_Ml_ko",0.3,2,2,1,2,1,null,null,null,7.5,7,8.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,2,3,null,null,null,null,null,null,8,7.5,10]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,10,8,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,17,10,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top bestaat soms uit zandige Boxtel-klei"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,25,24,26,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje en Drachten-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,29,28,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,35,34,36]
[null,null,null,null,null,null,null,"P_Ova_sd",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei"]
[]
[6,88,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S10C00036"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,1,null,null,null,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,1,2,null,null,null,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,6.75,6.25,7.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat lokaal dunne (dunner dan .50m) kleilagen"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,3,1,null,null,null,null,null,null,8.5,7,9]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,19,12,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basis loop sterk op naar ZW"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,25,24,26,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje en Drachten-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,29,28,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,35,34,36]
[null,null,null,null,null,null,null,"P_Ova_sd",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei"]
[]
[6,89,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S10C00027"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,1,null,null,null,null,null,null,5,4.5,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holoceen onder dijk weggehaald???"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,1,2,null,null,null,null,null,null,5,4.5,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holoceen onder dijk weggehaald???"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,6,5.5,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,3,1,null,null,null,null,null,null,9.5,8,11]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,16,15,17]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,22,20,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje en Drachten-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,26,24,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,39,37,40]
[null,null,null,null,null,null,null,"P_Ova_sd",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei"]
[]
[6,90,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S09H00046"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,null,null,null,null,null,null,7.5,6,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,null,null,null,null,null,null,7.5,6,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,9.5,8,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,3,1,null,null,null,null,null,null,12,11,14]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,20,18,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drachten-zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,25,24,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[6,91,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S09H00039"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,null,null,null,null,null,null,6,5.5,7]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,1,2,null,null,null,null,null,null,7.5,6,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,9.5,8,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, onderaan soms veenlagen tot 1m dik"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,17,14,22]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,32,30,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje zand"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,35,34,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-klei, nooit dikker dan 5 meter"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[6,92,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; "]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,1,1,1,null,null,null,7,5.5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,1,1,1,2,1,null,null,null,7.5,7,8.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,1,2,null,null,null,null,null,null,8.5,7,9]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,14,13,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat regelmatig veenlagen tot 0.5m, incidenteel tot 2m dik"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.6,5,1,1,1,1,null,null,null,16.5,15,18]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,5,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje zand, bevat soms kleilagen van enkele meters dik"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.4,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje zand, bevat soms kleilagen van enkele meters dik"]
[]
[6,93,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S09H00028"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,null,null,null,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,null,null,null,null,null,null,7,6.5,9]
[null,null,null,null,null,null,null,"H_Ml_ko",0.6,2,1,null,null,null,null,null,null,8.5,7,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms vrij zandig ontwikkeld"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,2,2,null,null,null,null,null,null,8,7.5,8.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,11,10,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel-zand, bevat regelmatig veenlagen tot 0.5m, incidenteel tot 2m dik"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,5,1,null,null,null,null,null,null,16,11,18]
[null,null,null,null,null,null,null,"P_Rg_zf",1,6,1,null,null,null,null,null,null,22,20,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drachten-zand"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,7,1,null,null,null,null,null,null,32,30,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje klei"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje zand"]
[]
[6,94,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S09H00031"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,1,1,0.2,1,1,null,null,null,8,7,8.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,1,1,0.8,1,2,null,null,null,8,7,8.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,2,0.2,1,1,null,null,null,7.5,7,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,2,0.8,1,2,null,null,null,7.5,7,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms vrij zandig ontwikkeld"]
[null,null,null,null,null,null,null,"H_Ml_ko",0.3,1,2,1,2,1,null,null,null,8,7,8.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,5,1,null,null,null,null,null,null,13,11,15]
[null,null,null,null,null,null,null,"P_Rg_zf",1,6,1,null,null,null,null,null,null,22,20,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drachten-zand"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,7,1,null,null,null,null,null,null,32,30,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje klei"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje zand"]
[]
[6,95,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S09H00035"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.85,1,1,0.2,1,1,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Mg_zk",0.85,1,1,0.8,1,2,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,1,2,0.2,1,1,null,null,null,3.75,3.25,4.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.15,1,2,0.8,1,2,null,null,null,3.75,3.25,4.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.15,1,2,1,2,1,null,null,null,4,3.5,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vooral in zuidelijke helft"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,5,1,null,null,null,null,null,null,14,13,18]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,6,1,null,null,null,null,null,null,20,18,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drachten-zand, bevat leemlagen tot 4m dik"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,7,1,null,null,null,null,null,null,30,28,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-zand"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-zand"]
[]
[6,96,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Damtrace Cat. B onder Afsluitdijk; S14F00031"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.9,1,1,0.8,1,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,1,0.2,1,2,null,null,null,3,2.5,5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,1,1,1,2,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,2,null,null,null,null,null,null,5,4,7.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,7.5,6,9]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,3,1,null,null,null,null,null,null,12,11,15]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,20,18,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drachten-zand, bevat leemlagen tot 4m dik"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,30,28,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-zand"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urk Tynje-zand"]
[]
[7,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,1,null,null,null,null,null,null,3,2.75,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S15F0050 mooi voorbeeld van kleine getijdegeul waarbij Basisveen ontbreekt"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,2,1,null,null,null,null,null,null,3.75,3.5,4]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,2,2,null,null,null,null,null,null,6,5,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7,6,9]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.8,4,1,null,null,null,null,null,null,7,6,9]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.2,4,2,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,10,9,16]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,6,1,1,1,1,null,null,null,14,11.5,17]
[null,null,null,null,null,null,null,"P_Rg_zg",0.3,6,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,6,2,null,null,null,null,null,null,40,40,40]
[]
[7,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.25]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,1,null,null,null,null,null,null,4.25,4,5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,10.5,8.5,12.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.15,4,1,null,null,null,null,null,null,11,9,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maximaal 0.5 m dik"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.85,4,2,null,null,null,null,null,null,10.5,10.5,10.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,5,1,null,null,null,null,null,null,16,13,17.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.3,5,2,null,null,null,null,null,null,20,19,25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,3,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[7,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,1,null,null,null,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,2,1,null,null,null,null,null,null,4.5,4.5,4.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,2,2,null,null,null,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,5.5,5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,7.5,6.5,8.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,20,17,21]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,25,22,30]
[null,null,null,null,null,null,null,"P_Gs_zg",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[7,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,1,1,1,1,null,null,null,5,4.5,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S15G00016 mooi voorbeeld van dekzand op fijner."]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,1,1,2,1,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,1,2,1,null,null,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,7,5.75,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen nooit dikker dan 0.75 m"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10,9,12]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,15,14,18]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,23.5,23,25]
[null,null,null,null,null,null,null,"P_Ova_sd",0.75,6,1,1,1,1,null,null,null,25,24,27]
[null,null,null,null,null,null,null,"P_Gs_zg",0.75,6,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Gs_zg",0.25,6,2,1,null,null,null,null,null,40,40,40]
[]
[7,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,1,1,1,null,null,null,6.5,5.25,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zuiderzeeafzetting aan de top: zand en klei afwisseling"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,1,1,1,2,1,null,null,null,8,6.5,8.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,2,1,1,1,null,null,null,6.5,5.25,6.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,1,2,1,2,1,null,null,null,8,6.5,8.25]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.6,1,2,1,3,1,null,null,null,12,10,13]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,3,1,1,1,null,null,null,9,8.5,10]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,12,11,13]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,19,17,21]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,4,1,1,1,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,null,null,null,null,null,null,40,40,40]
[]
[7,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,4.5,4,6.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,7.5,5.5,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,20,18,22]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,26,24,28]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[7,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In Urk zelf veel hoger"]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,1,1,null,null,null,null,null,null,9,7,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drachten (Boxtel voor Saale), overgeconsolideerd en daardoor veel weerstand"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,20,19,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S20E00077 goed voorbeeld van keileem op overgeconsolideerde Drachten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[7,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,4,3.5,4.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,7.5,6,8.25]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,22,20,24]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[7,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S20E00055 mooi voorbeeld van H_Mkw_zenk op HV op channel fill op Basisveen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,4.5,4.25,8]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6.5,5.5,8]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.4,3,1,1,1,1,null,null,null,11,10.25,12]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,3,1,1,2,1,null,null,null,11.5,10.75,12.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen nooit dikker dan 0.5 m"]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.6,3,2,null,null,null,null,null,null,12.5,9.5,13]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,13.5,12.5,14.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[7,10,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S20E00078 voorbeeld van Almere afzetting op Veen "]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,6,4.5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[7,11,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,5.5,5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,2,1,1,1,1,null,null,null,6,5.5,7]
[null,null,null,null,null,null,null,"H_Ml_ko",0.4,2,1,1,2,1,null,null,null,8,8,9]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,2,1,1,3,1,null,null,null,9,8.5,9.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,2,2,null,null,null,null,null,null,9,8.5,9.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,4,1,1,1,1,null,null,null,14,13,15]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,1,2,1,null,null,null,16,14,18]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,null,null,null,null,null,null,16,14,18]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,5,1,1,1,1,null,null,null,20,16,26]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,5,1,1,2,1,null,null,null,40,4,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,5,2,null,null,null,null,null,null,40,4,40]
[]
[7,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,"H_Ml_ko",0.7,1,1,null,null,null,null,null,null,6.5,5,10]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,2,1,1,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Ml_ko",0.3,1,2,1,2,1,null,null,null,6.5,5,10]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,8.5,7.5,11.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[7,13,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld wisselt tussen 0.5 en 2 m -NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,1,1,1,null,null,null,4,3,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S21A00115 goed voorbeeld van bay-head delta zand op veen"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,2,1,null,null,null,5.5,5,8.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,null,null,null,null,null,null,6.5,6,7]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,7.5,6.5,8.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,17,16,18]
[null,null,null,null,null,null,null,"P_Ova_sd",0.15,5,1,1,1,1,null,null,null,18,17,19]
[null,null,null,null,null,null,null,"P_Rg_zg",0.15,5,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.85,5,2,null,null,null,null,null,null,40,40,40]
[]
[7,14,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,1,1,1,null,null,null,4,3,7.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,2,1,null,null,null,5.5,5,8.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,null,null,null,null,null,null,6.5,6,7]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,7.5,6.5,8.5]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,3,1,1,1,1,null,null,null,11,10,14]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,3,2,null,null,null,null,null,null,40,40,40]
[]
[7,15,15,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,1.25,1,2]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,2,1,1,1,1,null,null,null,3,2.5,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urkzand"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.2,2,1,1,2,1,null,null,null,10,3.5,25]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.8,2,2,null,null,null,null,null,null,10,3.5,25]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,18,16,40]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[7,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,1.5,1,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Urkzand"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.4,2,1,1,1,1,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.4,2,1,1,2,1,null,null,null,5,2,7.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.6,2,2,null,null,null,null,null,null,5,2,7.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,12.5,11,15]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,17,16,20]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,25,23,31]
[null,null,null,null,null,null,null,"P_Rg_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[7,17,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mv varieert tussen 0.5 en -1.5 m -NAP"]
[null,null,null,null,null,null,null,"H_Ova_zf",0.35,1,1,1,1,1,null,null,null,1.5,1,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sondering S21B000038 mooi voorbeeld van Veen op zand op P_Ova_sd"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.35,1,1,1,2,1,null,null,null,3,2,4]
[null,null,null,null,null,null,null,"H_Ova_zf",0.25,1,2,1,1,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.25,1,2,1,2,1,null,null,null,3,2.5,4]
[null,null,null,null,null,null,null,"H_Vhv_v",0.25,1,2,1,3,1,null,null,null,3.5,2.5,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.35,1,3,1,1,1,null,null,null,2,1,3.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.35,1,3,1,2,1,null,null,null,3.5,2,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,4,null,null,null,null,null,null,5,4.5,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,6.5,5.5,7.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,3,1,1,1,1,null,null,null,14,10,16]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,3,1,1,2,1,null,null,null,18,17,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,3,1,1,3,1,null,null,null,28,26,30]
[null,null,null,null,null,null,null,"P_Rg_zg",0.9,3,1,1,4,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,3,2,1,1,1,null,null,null,28,26,30]
[null,null,null,null,null,null,null,"P_Rg_zg",0.1,3,2,1,2,1,null,null,null,40,40,40]
[]
[7,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,1,1,1,null,null,null,2.75,1,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oud kwelderstrand, verspoeld veen, zandlaagjes en klei"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,1,1,1,2,1,null,null,null,6.5,4,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.4,1,1,1,3,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,2,1,1,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,1,2,1,2,1,null,null,null,3,2,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.6,1,2,1,3,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,15,14,22]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,17,15,21]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,25,22,28]
[null,null,null,null,null,null,null,"P_Gs_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[7,19,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,1,1,1,1,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Vhv_v",0.15,1,1,1,2,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.15,1,1,1,3,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,2,1,1,1,null,null,null,2.5,1.5,3]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,1,2,1,2,1,null,null,null,4,3.5,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,1,2,1,3,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,3,1,1,1,null,null,null,8,6,10]
[null,null,null,null,null,null,null,"P_Rg_zm",0.05,1,3,1,2,1,null,null,null,9,8.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,15,14,18]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,3,1,1,1,1,null,null,null,20,17,25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,1,1,2,1,null,null,null,26,20,28]
[null,null,null,null,null,null,null,"P_Gs_zg",0.8,3,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,2,1,1,1,null,null,null,26,20,28]
[null,null,null,null,null,null,null,"P_Gs_zg",0.2,3,2,1,2,1,null,null,null,40,40,40]
[]
[7,20,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,1,1,1,1,1,null,null,null,1.5,1,2.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.15,1,1,1,2,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.15,1,1,1,3,1,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.75,1,2,1,1,1,null,null,null,1.5,1,2.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.75,1,2,1,2,1,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.75,1,2,1,3,1,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,3,1,1,1,null,null,null,6,4,8]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,1,3,1,2,1,null,null,null,9,8.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,40,40,40]
[]
[7,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grotendeels water aan maaiveld"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,1,1,1,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,1,1,2,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,3,1,null,null,null,6.5,6,7.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,null,null,null,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,8.5,7.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,3,1,1,1,1,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"P_Gs_zg",0.2,3,1,1,2,1,null,null,null,14,12,15]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,3,2,null,null,null,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,22,20,25]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms klei,veenlagen van enkele meters dik"]
[]
[7,22,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,1,1,1,null,null,null,4.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,1,1,2,1,null,null,null,5.5,3.5,6]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,3,1,null,null,null,6.5,4,8.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,null,null,null,null,null,null,7,6,9]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,8.5,7.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.9,3,1,1,1,1,null,null,null,12,11,13]
[null,null,null,null,null,null,null,"P_Gs_zg",0.9,3,1,1,2,1,null,null,null,17.5,16,19]
[null,null,null,null,null,null,null,"P_Rg_zg",0.1,3,2,null,null,null,null,null,null,19,16.5,20]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,22,20,25]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms klei,veenlagen van enkele meters dik"]
[]
[7,23,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,1,1,1,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.35,1,1,1,2,1,null,null,null,5.25,4.5,5.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.35,1,1,1,3,1,null,null,null,5.75,5,6.25]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,2,1,1,1,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.6,1,2,1,2,1,null,null,null,4.75,3.75,5.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.6,1,2,1,3,1,null,null,null,5.75,5,6.25]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,6.25,5.5,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,7.75,7,8.25]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,3,1,1,1,1,null,null,null,13.75,12,14]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,3,1,1,2,1,null,null,null,16.5,15,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Urk veenlaag"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,3,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,3,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms klei,veenlagen van enkele meters dik"]
[]
[7,24,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,1,1,1,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.2,1,1,1,2,1,null,null,null,4.5,4,5.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.75,1,2,1,1,1,null,null,null,0.5,0,1.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.75,1,2,1,2,1,null,null,null,3.75,3.5,4.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.75,1,2,1,3,1,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.05,1,3,null,null,null,null,null,null,4.5,3.75,8]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,5.5,5.25,6.25]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,6.5,6,7]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,1,1,null,null,null,18.5,18,19]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,2,1,null,null,null,19.5,19,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen klei met soms dun veen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms klei,veenlagen van enkele meters dik"]
[]
[7,25,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,1,1,1,null,null,null,0.5,0,1.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.9,1,1,1,2,1,null,null,null,3.75,3.5,4.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,1,3,1,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,1,1,1,4,1,null,null,null,5.5,5.25,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms enkele decimeters dikke leemlaag onder basisveen (Wijchen,beek)"]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.05,1,2,1,1,1,null,null,null,4.5,3.75,8]
[null,null,null,null,null,null,null,"H_Vbv_v",0.05,1,2,1,2,1,null,null,null,5.5,5.25,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms enkele decimeters dikke leemlaag onder basisveen (Wijchen,beek)"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,1,3,null,null,null,null,null,null,6.5,6,8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,6.5,6,7]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,1,1,null,null,null,18.5,18,19]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,2,1,null,null,null,19.5,19,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen klei met soms dun veen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms klei,veenlagen van enkele meters dik"]
[]
[7,26,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,1,1,1,0.7,1,1,0.5,0,1.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,1,1,1,0.3,1,2,2.5,1.5,4]
[null,null,null,null,null,null,null,"H_Rg_zm",0.9,1,1,1,2,1,null,null,null,3.75,3.5,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Is soms ook zeer grof zand met grindjes"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,1,1,1,3,1,null,null,null,5.5,5.25,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms enkele decimeters dikke leemlaag onder basisveen (Wijchen,beek)"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.9,1,1,1,4,1,null,null,null,6.5,5.75,9]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.05,1,2,1,1,1,null,null,null,3.75,3.5,8]
[null,null,null,null,null,null,null,"H_Vbv_v",0.05,1,2,1,2,1,null,null,null,5.5,5.25,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms enkele decimeters dikke leemlaag onder basisveen (Wijchen,beek)"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.05,1,2,1,3,1,null,null,null,6.5,5.75,9]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,1,3,null,null,null,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,17.5,16.75,18.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,3,1,1,1,1,null,null,null,25,19,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Urk  kleilaag met tussenliggende dunne (dunner dan 1m dik) zandlagen "]
[null,null,null,null,null,null,null,"P_Rg_zg",0.3,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,3,2,1,1,1,null,null,null,35,30,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,3,2,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms klei,veenlagen van enkele meters dik"]
[]
[8,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S21C00023 voorbeeld van H_Mkw_zenk op Basisveen op dekzand op Kr op Eem"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.95,1,1,1,1,1,null,null,null,2.5,1.5,3]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,2,1,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.05,1,2,null,null,null,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Mp_k",0.05,4,1,1,1,1,null,null,null,18,15.5,19]
[null,null,null,null,null,null,null,"P_Rg_zm",0.05,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,4,2,null,null,null,null,null,null,40,40,40]
[]
[8,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.95,1,1,1,1,1,null,null,null,1.5,1,3]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,2,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.05,1,2,null,null,null,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,5.5,5,7]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Mp_k",0.95,4,1,1,1,1,null,null,null,18,15.5,19]
[null,null,null,null,null,null,null,"P_Rg_zm",0.95,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.05,4,2,null,null,null,null,null,null,40,40,40]
[]
[8,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.47,1,1,1,1,1,null,null,null,2,1.5,3]
[null,null,null,null,null,null,null,"H_Vbv_v",0.47,1,1,1,2,1,null,null,null,3.5,2.5,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.47,1,1,1,3,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mp_zf",0.03,1,2,1,1,1,null,null,null,3.5,2.5,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.03,1,2,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mp_zf",0.47,1,1,1,1,1,null,null,null,4.5,4,5.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.47,1,1,1,2,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.47,1,1,1,3,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mp_zf",0.03,1,2,1,1,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.03,1,2,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,14,12,16]
[null,null,null,null,null,null,null,"P_Mp_k",0.95,4,1,1,1,1,null,null,null,17,15,18]
[null,null,null,null,null,null,null,"P_Rg_zm",0.95,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.05,4,2,null,null,null,null,null,null,40,40,40]
[]
[8,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.95,1,1,1,1,1,null,null,null,1.5,1,3]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,1,2,1,null,null,null,2.5,2,4]
[null,null,null,null,null,null,null,"H_Mp_zf",0.05,1,2,null,null,null,null,null,null,2.5,2,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,14,13,16]
[null,null,null,null,null,null,null,"P_Mp_k",0.95,4,1,1,1,1,null,null,null,16,15.5,17]
[null,null,null,null,null,null,null,"P_Rg_zm",0.95,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.05,4,2,null,null,null,null,null,null,40,40,40]
[]
[8,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Mp_zf",0.47,1,1,1,1,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Vbv_v",0.47,1,1,1,2,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.47,1,1,1,3,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mp_zf",0.03,1,2,1,1,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.03,1,2,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mp_zf",0.47,1,1,1,1,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Vbv_v",0.47,1,1,1,2,1,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.47,1,1,1,3,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Mp_zf",0.03,1,2,1,1,1,null,null,null,5.5,4.5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.03,1,2,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,15,14,17]
[null,null,null,null,null,null,null,"P_Mp_k",0.95,4,1,1,1,1,null,null,null,16,15,17]
[null,null,null,null,null,null,null,"P_Rg_zm",0.95,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.05,4,2,null,null,null,null,null,null,40,40,40]
[]
[8,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S27A00020 mooi voorbeeld van H_Mkw_zenk op veen op dekzand of P_Rg_zm"]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,3,2.5,4]
[null,null,null,null,null,null,null,"H_Ml_ko",1,2,1,null,null,null,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,13,11,15]
[null,null,null,null,null,null,null,"P_Mp_k",0.8,5,1,1,1,1,null,null,null,16,15,17]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,5,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,5,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Gs_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[8,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,3.25,2.75,4]
[null,null,null,null,null,null,null,"H_Ml_ko",1,2,1,null,null,null,null,null,null,3.75,3.25,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top vaak wat verspoeld"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,15,14,15.5]
[null,null,null,null,null,null,null,"P_Mp_k",0.05,5,1,1,1,1,null,null,null,16,15.5,16.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,5,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,5,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Gs_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[8,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",1,2,1,null,null,null,null,null,null,5.25,4.5,6]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,12,10,17]
[null,null,null,null,null,null,null,"P_Ova_sd",0.95,5,1,1,1,1,null,null,null,18,17,20]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,5,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,5,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Gs_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[8,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",1,2,1,null,null,null,null,null,null,5,4.5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,4,1,1,1,1,null,null,null,11,9,12]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,4,1,1,2,1,null,null,null,12,11,13.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,4,1,1,3,1,null,null,null,16,14.5,21]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,4,2,null,null,null,null,null,null,16,14.5,21]
[null,null,null,null,null,null,null,"P_Ova_sd",0.97,5,1,1,1,1,null,null,null,24.5,24,27]
[null,null,null,null,null,null,null,"P_Rg_zg",0.97,5,1,1,2,1,null,null,null,32,30,34]
[null,null,null,null,null,null,null,"P_Rg_zg",0.03,5,2,null,null,null,null,null,null,32,30,34]
[null,null,null,null,null,null,null,"P_Gs_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[8,10,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sondering  S26G00034 (alleen figuur)"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.2,1,1,null,null,null,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"H_Mp_zf",0.8,1,2,1,1,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Ml_ko",0.8,1,2,1,2,1,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,4,3.5,4.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,1,1,1,1,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,1,1,2,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,2,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,1,1,null,null,null,8.5,7.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,4,1,1,2,1,null,null,null,15,14.5,16.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,4,2,null,null,null,null,null,null,15,14.5,16.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,1,1,1,null,null,null,40,40,40]
[]
[8,11,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,2,1,null,null,null,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.2,2,2,1,1,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,2,2,1,2,1,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,1,null,null,null,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,2,1,1,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,3,2,1,2,1,null,null,null,8.5,7.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,2,1,3,1,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,2,1,1,1,null,null,null,16,14,17]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,2,1,2,1,null,null,null,40,40,40]
[]
[8,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,1,1,1,null,null,null,2.2000000000000002,2,2.5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.3,1,1,1,2,1,null,null,null,2.5,2.2000000000000002,2.8]
[null,null,null,null,null,null,null,"H_Mp_zf",0.7,1,2,1,1,1,null,null,null,2.5,2.2000000000000002,2.8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,1,1,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,3,2,1,1,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,4,1,1,1,1,null,null,null,8.5,7.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,1,2,1,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,1,1,1,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,2,1,1,1,null,null,null,16,14,17]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,2,1,2,1,null,null,null,40,40,40]
[]
[8,13,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Mp_zf",0.9,1,1,1,1,1,null,null,null,2,1,3]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,2,1,1,1,null,null,null,1.5,1,2.8]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,1,1,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,3,2,1,1,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,4,1,1,1,1,null,null,null,8.5,7.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,1,2,1,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,1,1,1,null,null,null,11,9,13]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,2,1,1,1,null,null,null,16,14,17]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,2,1,2,1,null,null,null,40,40,40]
[]
[8,14,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,1,1,1,1,null,null,null,2.5,1.5,3]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,1,1,1,2,1,null,null,null,3,1.5,4]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,1,2,null,null,null,null,null,null,2.5,2,3.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,4,3.5,6]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,1,null,null,null,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,3,2,null,null,null,null,null,null,16,14,17]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,3,3,null,null,null,null,null,null,32,30,34]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,15,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,0.25,1,1,null,null,null,3.25,3,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,0.75,1,2,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Ml_ko",0.75,1,2,null,null,null,null,null,null,2.25,2,2.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,3,null,null,null,null,null,null,3.25,2.5,4]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,3.25,2.5,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,19,18,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ook met humeuze lagen"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,22,21,23]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Mg_zk",0.5,6,2,null,null,null,null,null,null,40,40,40]
[]
[8,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,0.25,1,1,null,null,null,3,3,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,0.75,1,2,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,2,0.8,1,1,null,null,null,2,2,2.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,2,0.2,1,2,null,null,null,2.75,2.5,3]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,1,null,null,null,null,null,3,2.25,4]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,5,1,null,null,null,null,null,null,12.5,12,13.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.1,5,2,null,null,null,null,null,null,19,15,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Afwisseling zand en kleilagen"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,6,1,null,null,null,null,null,null,19,15,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Afwisseling zand en kleilagen"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Mg_zk",0.5,7,2,null,null,null,null,null,null,40,40,40]
[]
[8,17,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,null,null,null,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,2,0.75,1,1,null,null,null,2.75,2.5,3.5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,2,0.25,1,2,null,null,null,4,3.75,4.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,5,4,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veenlaag wordt nooit doorsneden"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top dekzand golvend met relief van 1-2 m."]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.5,4,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.5,4,1,null,null,null,null,null,null,17,16,19]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.75]
[null,null,null,null,null,null,null,"H_Ml_ko",1,1,1,null,null,null,null,null,null,4.75,4.5,5.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7,6.5,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Venige opvulling van beekdal, met diepste punt gecentreerd"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.5,3,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.5,3,1,null,null,null,null,null,null,17,16,19]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,19,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.45,1,1,null,null,null,null,null,null,4.5,4,5.5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.45,1,2,null,null,null,null,null,null,5.75,5.5,6.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,3,null,null,null,null,null,null,5,3,5.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6.25,4.75,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen nooit weg"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10,8,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Golvend dekzandlandschap bepaalt onderkant en dikte veen"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,26,20,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ook met zandtrajecten in de ondoorlatende laag"]
[null,null,null,null,null,null,null,"P_Gs_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,20,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,1,null,null,null,null,null,null,5.25,4.5,6.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,2,null,null,null,null,null,null,5.25,4.5,6.25]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6.5,5.5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen altijd aanwezig"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,null,null,null,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,4,2,null,null,null,null,null,null,16,15,19]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,3,null,null,null,null,null,null,17,16,18]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,18,17,19]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,6,1,null,null,null,null,null,null,19,18,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ongeveer 1 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,6,2,null,null,null,null,null,null,20,19,21]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,22,21,24]
[null,null,null,null,null,null,null,"P_Gs_zg",1,8,1,null,null,null,null,null,null,40,40,40]
[]
[8,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,1,1,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.3,1,1,1,2,1,null,null,null,5.5,4.75,7.25]
[null,null,null,null,null,null,null,"H_Ml_ko",0.7,1,2,null,null,null,null,null,null,5.5,4.75,7.25]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7.75,7.25,8.75]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10.5,9.5,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S26C00115 mooi voorbeeld van P_Wdz_zf op P_Rbk_zens op Drente"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,18,17,19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms wat kleiige trajecten"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veelal fluvioglacial met ook grof zand trajecten"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,5,2,1,1,1,null,null,null,19,18.5,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal 1-2 m dik, soms aangeduid als keileem"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,5,2,1,2,1,null,null,null,40,40,40]
[]
[8,22,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,1,1,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.4,1,1,1,2,1,null,null,null,5.5,4.75,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms wat zandiger net boven veenlaag"]
[null,null,null,null,null,null,null,"H_Ml_ko",0.6,1,2,null,null,null,null,null,null,5.5,4.75,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms wat zandiger net boven veenlaag"]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6,5.5,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen nooit weg"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,8,7.5,9]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.1,4,1,1,1,1,null,null,null,10,9,10.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,4,1,1,2,1,null,null,null,13,12,14]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.9,4,2,null,null,null,null,null,null,13,9,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Richting het westen komt het gestuwde materiaal omhoog."]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,23,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In vrijwel gehele zuidkant Flevoland is ter plaatse van de dijk het Holocene klei- en veenpakket weggebaggerd"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,1,null,null,null,null,null,null,3,2.5,3.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,2,null,null,null,null,null,null,3,2.5,3.25]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,2,1,null,null,null,null,null,null,3.75,3,5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.05,2,2,null,null,null,null,null,null,3.5,3.25,3.75]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wellicht dunne Boxtel aan de top"]
[]
[8,24,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,"H_Mp_zf",0.8,1,1,null,null,null,null,null,null,2.75,2.5,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,1,1,1,null,null,null,2.5,2.25,2.75]
[null,null,null,null,null,null,null,"H_Mp_zf",0.2,1,2,1,2,1,null,null,null,3.25,3,3.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.05,2,1,null,null,null,null,null,null,5.5,3.75,6.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,2,2,1,1,1,null,null,null,5,3.25,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Segment ligt op een naar het noorden toe aflopende helling"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.95,2,2,1,2,1,null,null,null,5.5,3.75,6.75]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,5.75,4,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maximaal een halve meter dik"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,7.75,6,8.5]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,25,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,null,null,null,null,null,null,5.5,3,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,1,2,null,null,null,null,null,null,4,2.5,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.1,2,1,1,1,1,null,null,null,6.25,6,6.75]
[null,null,null,null,null,null,null,"H_Mp_zf",0.1,2,1,1,2,1,null,null,null,7,6.75,7.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,2,1,1,3,1,null,null,null,7.5,7.25,7.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nooit dikker dan 1"]
[null,null,null,null,null,null,null,"H_Ml_ko",0.55000000000000004,2,2,1,1,1,null,null,null,7.5,7.25,7.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.55000000000000004,2,2,1,2,1,null,null,null,8,7.75,8.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nooit dikker dan 1"]
[null,null,null,null,null,null,null,"H_Ml_ko",0.35,2,3,1,1,1,null,null,null,7.5,7.25,7.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.35,2,3,1,2,1,null,null,null,8,7.75,8.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nooit dikker dan 1"]
[null,null,null,null,null,null,null,"H_Ml_ko",0.35,2,3,1,3,1,null,null,null,9,8.75,9.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.35,2,3,1,4,1,null,null,null,9.5,9.25,9.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nooit dikker dan 1"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,11,10.5,12]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,26,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3]
[null,null,null,null,null,null,null,"H_Mp_zf",0.25,1,1,null,null,null,null,null,null,3.5,3,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandlaag voornamelijk in het westelijke gedeelte"]
[null,null,null,null,null,null,null,"H_Mp_k",0.75,1,2,null,null,null,null,null,null,3.5,3,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S25F00112 voorbeeld van dubbele veenlaag"]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,2,1,1,1,1,null,null,null,5,4.5,6.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,2,1,1,2,1,null,null,null,6,5.5,7.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,2,2,null,null,null,null,null,null,6,5.5,7.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,1,null,null,null,null,null,null,6.75,6.5,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veenlaag varieert in dikte van 0.25 m tot 1.5 m."]
[null,null,null,null,null,null,null,"H_Mg_zk",0.02,4,1,null,null,null,null,null,null,10.5,10.25,17]
[null,null,null,null,null,null,null,"H_Mp_k",0.88,4,2,null,null,null,null,null,null,10.5,8.5,11.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms humeuze lagen ingeschakeld"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,4,3,1,1,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,4,3,1,2,1,null,null,null,10.5,8.5,11.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,5,1,null,null,null,null,null,null,11,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen soms afwezig door ingesneden geul, veen maximaal 1.5 m dik"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,6,1,null,null,null,null,null,null,13,12,14]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,7,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In het westen soms afgedekt met Drente (soms keileem), in het oosten door Kreftenheye Formatie. Ondoorlatende lagen in P_Ggs_zg komen met name voor tussen 12-14 m -NAP en 20-22 m -NAP"]
[]
[8,27,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S26A00606 GEF voorbeeld van diepe geul"]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,1,null,null,null,null,null,null,6,5,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S26A00352 GEF"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,2,null,null,null,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7,6,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen maximaal 2 dik."]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,8,8,8]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,4,1,1,1,1,null,null,null,10.75,9.75,12.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,4,1,1,2,1,null,null,null,11,9.75,13]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,4,1,1,3,1,null,null,null,14,13,15]
[null,null,null,null,null,null,null,"H_Mg_zk",0.39,4,2,1,2,1,null,null,null,10.75,9.75,12.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.39,4,2,1,3,1,null,null,null,11,10,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Altijd dunner dan 0.5 m"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.39,4,2,1,4,1,null,null,null,14,13,15]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,4,3,1,2,1,null,null,null,17,12,18]
[null,null,null,null,null,null,null,"H_Mr_kz",0.01,4,4,null,null,null,null,null,null,19,16,20]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,23,20,26]
[null,null,null,null,null,null,null,"P_Ggs_zg",0.3,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms keileem aan de top"]
[null,null,null,null,null,null,null,"P_Mg_zm",0.7,6,2,null,null,null,null,null,null,40,40,40]
[]
[8,28,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S26A00085 tif"]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,1,null,null,null,null,null,null,6.5,6,7.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,2,1,1,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,2,1,2,1,null,null,null,6.5,6,7.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,3,1,1,1,1,null,null,null,10,9,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan in extreme gevallen het veen geerodeerd hebben."]
[null,null,null,null,null,null,null,"H_Mp_k",0.15,3,1,1,2,1,null,null,null,10.75,9,11.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,3,2,null,null,null,null,null,null,10.75,9,11.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,11.5,10.5,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen nooit weg door kleilaag erboven, maximaal 1.5 m dik."]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,13.5,12.5,14.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,6,1,1,1,1,null,null,null,14,13,15]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Mg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[8,29,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gebaseerd op een verhoging in het Pleistoceen"]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,1,null,null,null,null,null,null,6.5,6,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S26B00024 tif"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,2,1,1,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,2,1,2,1,null,null,null,6.5,6,7.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.75,2,1,null,null,null,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"H_Vhv_v",0.25,2,2,null,null,null,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,3,1,1,1,1,null,null,null,8,7.5,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,3,1,1,2,1,null,null,null,8.5,7.5,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,3,2,null,null,null,null,null,null,8.5,7.5,9]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,9,8.5,9.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,13,12.5,14]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,6,1,1,1,1,null,null,null,14,13,15]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Mg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[8,30,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pingo-opvulling?: S20D00054 tif,B20D0959 (t.o. 't Bovenwater) rand pingo in S20D00053?"]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,1,null,null,null,null,null,null,6.5,6,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"deel NO van haveningang Lelystad: S20D00031 GEF"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,2,1,1,1,null,null,null,5.5,5,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"deel ZW (w van Oostvaardersdiep) S20D00051"]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,2,1,2,1,null,null,null,6.5,6,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pingo's ook in S20D00037, B20D0183?"]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7,6.5,8]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,3,1,1,1,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,3,1,1,2,1,null,null,null,9,8,10.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,3,2,null,null,null,null,null,null,9,9,21]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,10,9,12]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,12.5,12,15]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,6,1,1,1,1,null,null,null,13.5,13,14]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Mg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[8,31,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"zuidelijk deel: S20D00160 GEF"]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,1,1,1,1,null,null,null,7.5,6.5,9]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,2,1,1,1,null,null,null,6.5,5,7.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,2,1,2,1,null,null,null,7.5,6.5,9]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,1,1,1,null,null,null,8,7.5,9.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,3,1,1,1,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,3,1,1,2,1,null,null,null,9,8,10.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,3,2,1,1,1,null,null,null,9,9,21]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,1,1,1,null,null,null,11,10.5,12]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,1,1,1,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,6,1,1,1,1,null,null,null,16,13,18]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,6,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,6,2,1,1,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,7,1,1,1,1,null,null,null,26,24,28]
[null,null,null,null,null,null,null,"P_Mg_zm",0.3,7,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Mg_zm",0.7,7,2,1,1,1,null,null,null,40,40,40]
[]
[8,32,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S20G00026 tif, S20G00031 tif"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.8,1,1,null,null,null,null,null,null,6.5,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H_Mp_zf in dit geval antropogeen dijkzand, polder opgevuld?"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.2,1,2,1,1,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,1,2,1,null,null,null,6.5,6,8]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,8.5,7,9]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,10.5,10,11]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,11,10.5,12]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,1,1,1,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,6,1,1,1,1,null,null,null,16,13,18]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,6,1,1,2,1,null,null,null,20,19,25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,6,2,1,1,1,null,null,null,20,19,25]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,7,1,1,1,1,null,null,null,21,20,26]
[null,null,null,null,null,null,null,"P_Mg_zm",0.3,7,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Mg_zm",0.7,7,2,1,1,1,null,null,null,40,40,40]
[]
[8,33,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S20E00037 tif"]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,1,1,1,1,null,null,null,4.5,4.2,5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,1,2,1,null,null,null,6.5,5.5,7]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,2,null,null,null,null,null,null,6.5,5.5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,2,1,null,null,null,null,null,null,8.5,6.5,9]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,2,2,1,1,1,null,null,null,7.5,6.5,8]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,2,2,1,2,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Vbv_v",0.7,3,1,1,1,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,3,2,1,2,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,13,12,14]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,24,20,26]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,6,1,1,1,1,null,null,null,25,21,27]
[null,null,null,null,null,null,null,"P_Mg_zm",0.2,6,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Mg_zm",0.8,6,2,null,null,null,null,null,null,40,40,40]
[]
[8,34,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S20F00012 tif"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,1,1,1,1,1,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,1,1,2,1,null,null,null,6.5,5.5,7]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,1,1,1,null,null,null,6.5,5.5,7]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,3,1,1,1,null,null,null,6.5,5.5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7.5,7,8]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,3,1,1,1,1,null,null,null,8.3000000000000007,8,9]
[null,null,null,null,null,null,null,"H_Vbv_v",0.3,3,1,1,2,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,3,2,null,null,null,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,12.5,12,14]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,17.5,15,20]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,23,19,25]
[null,null,null,null,null,null,null,"P_Mg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[]
[8,35,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,1,1,1,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,1,1,2,1,null,null,null,7.5,6.5,8]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,2,1,1,1,null,null,null,7.5,6.5,8]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,3,1,1,1,null,null,null,7.5,5.5,8]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,2,1,1,1,1,null,null,null,8.5,6,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,2,1,1,2,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,2,1,1,3,1,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,2,2,1,1,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,2,2,1,2,1,null,null,null,10,9,10]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,2,2,1,3,1,null,null,null,11,9,11]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,12.5,12,14]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,1,null,null,null,null,null,null,23,19,25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,2,1,1,1,null,null,null,19,17,20]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,2,1,2,1,null,null,null,23,19,25]
[null,null,null,null,null,null,null,"P_Mg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[8,36,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S20H00052 GEF"]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,1,null,null,null,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,2,null,null,null,null,null,null,6.5,6,7]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7.5,7,9]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10.5,9,13]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,1,1,1,1,null,null,null,26,24,30]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,2,null,null,null,null,null,null,40,40,40]
[]
[8,37,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S21C00057 tif"]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,1,null,null,null,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,2,null,null,null,null,null,null,5.5,5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6.5,6,7.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,10,8,11]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,1,1,1,1,null,null,null,16,15,18]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,1,2,1,null,null,null,18,16,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,2,null,null,null,null,null,null,18,16,20]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,2,null,null,null,null,null,null,40,40,40]
[]
[8,38,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,1,null,null,null,null,null,null,4.5,4,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stratigrafie onder Boxtel Fm. "]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,2,null,null,null,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,1,1,1,1,null,null,null,16,15,18]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,1,2,1,null,null,null,18,16,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,2,null,null,null,null,null,null,18,16,20]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,2,null,null,null,null,null,null,40,40,40]
[]
[8,39,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,3,2,4]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,2,1,null,null,null,null,null,null,5.5,4.5,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,2,2,1,1,1,null,null,null,5.5,4.5,6]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,2,2,1,2,1,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,1,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,5,1,null,null,null,null,null,null,26,24,28]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,5,2,null,null,null,null,null,null,26,24,28]
[null,null,null,null,null,null,null,"P_Gs_zg",0.5,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,2,null,null,null,null,null,null,40,40,40]
[8,40,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S21C00006 GEF"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,3,1,1,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,6,5,9]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,0.1,1,2,null,null,null,6,5.5,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandig geultje"]
[null,null,null,null,null,null,null,"H_Ml_ko",0.8,1,2,0.2,3,2,null,null,null,9.75,9.5,10]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,25,24,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KR-zand, meestal matig grof maar soms uiterst grof, vooral lager in dit pakket"]
[8,42,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Houtribdijk. S20A00172"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.7,3,1,1,1,1,8,7.5,8.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.2,2,1,null,null,null,null,null,null,12.5,12,13]
[null,null,null,null,null,null,null,"P_Mp_k",1,5,1,null,null,null,null,null,null,31.5,30,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-klei"]
[null,null,null,null,null,null,null,"P_Mg_zm",1,6,1,null,null,null,null,null,null,35,34,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-zand is matig tot uiterst grof met bijmenging grind"]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6.5,6,7.75]
[null,null,null,null,null,null,null,"H_Vbv_v",0.8,5,2,1,2,1,null,null,null,12.5,12,13]
[]
[null,null,null,null,null,null,null,"H_Ml_ko",0.4,2,1,1,1,1,null,null,null,10.5,10.25,10.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat incidenteel dunne (~.25m) veenlaag bovenin"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,3,2,1,2,1,null,null,null,12.5,12,13]
[null,null,null,null,null,null,null,"P_Gs_zg",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drente Schaarsbergen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,9,8.5,9.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandige klei met zandlaagjes, soms sterk humeus"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,5,1,null,null,null,null,null,null,15.5,14.5,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dekzand, fijn tot matig grof"]
[null,null,null,null,null,null,null,"H_Aa_ht",0.1,1,1,null,null,null,null,null,null,10,9,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stortzand"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,2,0.3,2,2,1,2,1,10,9.75,10.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms met organische kleiwig erin tot 25cm dik"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.6,2,2,1,2,1,null,null,null,12.5,12,13]
[8,47,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,4.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Houtribdijk"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,1,1,null,null,null,null,null,null,6,5.75,6.25]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,2,2,1,2,1,null,null,null,8.5,8,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms met organische kleiwig erin tot 25cm dik"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,15,14.5,15.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dekzand, soms lemig traject"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,null,null,null,null,null,null,5,4.75,5.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meerbodem, soms detrituslaag aan basis"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,2,3,1,2,1,null,null,null,7.75,7.5,8.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,24.5,23.5,25.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KR-zand, matig fijn tot uiterst grof"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,1,1,0.6,1,1,null,null,null,6.5,6.25,7.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,3,1,null,null,null,null,null,null,11.5,11.25,11.75]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,6,2,1,2,1,null,null,null,25,24,26]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,2,1,1,1,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,15,14,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dekzand"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,1,3,null,null,null,null,null,null,2.25,1.5,2.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,5,3,7]
[null,null,null,null,null,null,null,"P_Mg_zk",0.5,5,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,12,10.5,14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen-klei, bevat sporadisch dunne (dunner dan 50cm) veenlagen"]
[]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.85,2,1,1,3,1,null,null,null,27,25,29]
[]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.3,1,2,1,1,1,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Rg_zg",0.25,2,2,null,null,null,null,null,null,31,30,34]
[9,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.3,1,2,1,2,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.3,1,2,1,2,1,null,null,null,3,2,3.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,22,20,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sporadisch dunne (dunner dan 50cm) kleilagen"]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,2,1,1,1,null,null,null,0.25,0,0.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.35,1,1,1,1,1,null,null,null,0.5,0.25,0.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.1,1,3,1,1,1,null,null,null,3,2.5,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Alleen dik veen"]
[9,10,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"P_Rg_zm",0.3,1,2,1,3,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Mp_k",0.4,1,1,1,1,1,null,null,null,2,1.75,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikke klei"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,1,2,1,3,1,null,null,null,8.25,7.5,9]
[9,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,1,1,null,null,null,null,null,null,7.5,7,8]
[null,null,null,null,null,null,null,"H_Vhv_v",1,1,1,null,null,null,null,null,null,3,2,3.5]
[9,15,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-4]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,26,25,27]
[null,null,null,null,null,null,null,"P_Rg_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7.5,7,8.5]
[9,17,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,1,1,1,null,null,null,3,2,9]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,3,2,null,null,null,null,null,null,17,15,20]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.65,1,2,1,1,1,null,null,null,0,-0.5,1.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,7,6,9]
[10,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.15,1,2,1,2,1,null,null,null,3.5,2.5,4.5]
[10,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rivierduin, maaiveld wisselt tussen +4 en +6m NAP"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,2,2,null,null,null,null,null,null,4.5,4,6]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.05,1,2,null,null,null,null,null,null,0.5,-0.5,1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,3,1,1,1,1,1,1,0.75,0.5,1.5]
[]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Kreftenheye, Urk en Appelscha. Bevat soms kleilagen, met name rond 10 m -NAP van 1-2 m dik"]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,null,null,null,null,null,null,5.5,4.75,6.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,1,0.6,1,1,null,null,null,0.75,0.25,1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,2,1,1,1,null,null,null,0.5,0.25,1]
[10,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"achter de dijk maaiveld ~ 2m-NAP, deels veen weggegraven"]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,1,2,0.5,1,2,null,null,null,3.25,3,3.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,7,5,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms ook fijn tot uiterst grof"]
[null,null,null,null,null,null,null,"H_Rk_k",0.9,1,2,null,null,null,null,null,null,1,0.75,1.5]
[]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,3,1,1,1,null,null,null,1.75,1.5,2]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,3,1,1,1,1,null,null,null,16,15,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Kreftenheye. Soms onderbroken kleilagen van 1-2 m "]
[10,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S21G00276 voorbeeld van dik veen. S21G00269 voorbeeld van H_Ro_kenz als geulopvulling"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,1,0.8,1,1,null,null,null,0.75,0.5,1.75]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,3,1,1,1,null,null,null,0.75,0.5,1.75]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Appelscha. Soms onderbroken kleilagen van 1-2 m "]
[null,null,null,null,null,null,null,"H_Vbv_v",0.6,1,1,1,2,1,null,null,null,1.25,1,1.75]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,9,7,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms ook fijn tot uiterst grof (Fm. van Boxtel, meestal Kreftenheye)"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7.5,5,9]
[11,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,14,13,16]
[11,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,14.5,11,16]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,1,1,1,null,null,null,1.5,0.5,2]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.02,1,3,null,null,null,null,null,null,3,2,4]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,2,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,1,2,null,null,null,null,null,null,3.5,2,4]
[11,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,2,1,3,1,null,null,null,4.5,4,5.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,1,null,null,null,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,7,5.5,7.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,2,1,2,1,null,null,null,3.5,2.5,5.5]
[null,null,null,null,null,null,null,"H_Rr_o&z",1,1,1,null,null,null,null,null,null,7,5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling, mogelijk estuariene invloed a.g.v. segment 11-12"]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,9,6,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kronkelwaard, mogelijk estuariene invloed a.g.v. segment 11-12"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.25,1,2,1,1,1,null,null,null,0.25,-0.25,0.75]
[]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,1,2,1,2,1,null,null,null,1,0,1.75]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.4,1,2,1,3,1,null,null,null,2.5,2,3.5]
[11,14,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.2,2,1,1,2,1,null,null,null,12,11,14]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,1,1,1,1,null,null,null,0.75,0.5,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Buitendijks is de klei deels afgegraven en volgestort met (grof)zand"]
[12,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld van -1 tot +7m tov NAP"]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,1,null,null,null,null,null,null,2,1,2.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.7,1,1,1,1,1,null,null,null,0,-1,1]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,2,1,2,1,null,null,null,3.75,3,4.5]
[]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,3,1,1,1,1,null,null,null,9,8.5,10]
[12,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,3.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,1,2,1,2,1,null,null,null,6.5,5.5,8]
[null,null,null,null,null,null,null,"P_Gkl_kz",1,2,1,null,null,null,null,null,null,8,6.5,12.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,1,2,1,null,null,null,7,5,8]
[12,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.2,1,3,1,2,1,null,null,null,8.75,8.5,9.25]
[null,null,null,null,null,null,null,"P_Mg_zk",0.2,2,2,1,3,1,null,null,null,25,24,26,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eem-zand"]
[]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.2,3,2,1,1,1,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"P_Mg_zk",0.1,3,3,1,3,1,null,null,null,26,25,27]
[null,null,null,null,null,null,null,"H_Ova_zm",1,2,1,null,null,null,null,null,null,3,2,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hol. Strandafzettingen"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,13,12.5,13.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Boxtel Tilligte "]
[null,null,null,null,null,null,null,"P_Mg_zk",0.4,6,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.45,1,1,1,3,1,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,3,1,null,null,null,null,null,6,4.5,8]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,2,1,null,null,null,null,null,null,12,11.5,14.5]
[13,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,2,1,2,1,null,null,null,4,3,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen niet dikker dan 0.75m"]
[null,null,null,null,null,null,null,"P_Mg_zk",0.2,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mr_kz",0.2,1,2,1,1,1,null,null,null,20,19,23]
[]
[null,null,null,null,null,null,null,"H_Ml_ko",1,4,1,null,null,null,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,1,1,1,1,null,null,null,1.5,1.25,1.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.1,2,2,null,null,null,null,null,null,5.75,5.5,6.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sporadisch een dun veenlaagje (dunner dan 20cm)"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,1,1,4,1,null,null,null,4,2.5,5]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,2,1,2,1,null,null,null,3,2.25,4]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,1,2,1,3,1,null,null,null,4,2.5,5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,3,1,2,1,null,null,null,7.5,7.25,7.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.35,1,5,1,2,1,null,null,null,14,12.5,16]
[null,null,null,null,null,null,null,"H_Mp_k",1,2,1,null,null,null,null,null,null,2.5,2,4.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.4,4,2,1,2,1,null,null,null,11.5,8,16.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.2,1,1,1,1,1,null,null,null,9,5,13.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.4,1,2,1,3,1,null,null,null,15,13,17]
[]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,31.5,31,32]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,1,2,1,null,null,null,5,3.5,6.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,2,1,null,null,null,null,null,null,23,22,23.5]
[null,null,null,null,null,null,null,"H_Mp_zf",1,1,1,null,null,null,null,null,null,4,3.25,5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.4,2,2,1,2,1,null,null,null,7.5,7,8]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,3,1,null,null,null,null,null,null,19,18.5,19.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.3,1,1,1,1,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.3,3,1,1,2,1,null,null,null,15,13,17]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.25,3,1,1,1,1,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Mg_zk",0.75,3,2,1,2,1,null,null,null,20,19,21]
[null,null,null,null,null,null,null,"H_Mp_zf",0.5,1,1,1,1,1,null,null,null,1.75,1.5,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,2,2,null,null,null,null,null,null,5.5,4.5,7]
[null,null,null,null,null,null,null,"P_Mg_zm",0.2,7,1,1,2,1,null,null,null,39,38,39.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.5,1,1,1,1,1,null,null,null,2,1.75,2.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,2,2,null,null,null,null,null,null,11.5,11.25,12]
[13,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,2,1,1,2,1,null,null,null,6.5,4.5,7.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,2,2,null,null,null,null,null,null,6.5,4.5,7.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,3,2,1,3,1,null,null,null,13.5,12.5,14]
[null,null,null,null,null,null,null,"P_Gs_zg",1,8,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.6,2,1,1,1,1,null,null,null,12,11,14]
[null,null,null,null,null,null,null,"P_Mp_k",0.4,4,1,1,1,1,null,null,null,33,32,37.5]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,10.5,9.5,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleipakket omvat ook dunne incidenteel voorkomende Hollandveen-lagen"]
[null,null,null,null,null,null,null,"P_Gs_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,29,28,31]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,2,1,1,1,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Gs_zg",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,2,1,1,1,null,null,null,12,10,15]
[null,null,null,null,null,null,null,"P_Mg_zm",0.1,6,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,1,2,null,null,null,null,null,null,16.5,8,19]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,16.5,16,19]
[]
[null,null,null,null,null,null,null,"H_Mr_kz",0.4,2,2,null,null,null,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"P_Mg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,5.75,5.25,6.25]
[null,null,null,null,null,null,null,"P_Mg_zm",1,8,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.35,1,2,1,1,1,null,null,null,3.5,3.25,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikke klei op dun veen"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,3,1,null,null,null,null,null,null,20,18,21]
[null,null,null,null,null,null,null,"H_Mp_k",0.35,1,1,1,1,1,null,null,null,2,1.75,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dun klei op dik veen"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.05,1,3,1,2,1,null,null,null,4.25,3.5,5]
[]
[null,null,null,null,null,null,null,"H_Mp_ko",1,5,1,null,null,null,null,null,null,17,16.5,17.5]
[13,30,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0.5,0.25,0.75]
[null,null,null,null,null,null,null,"P_Mg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,1,2,1,2,1,null,null,null,4.25,3.75,4.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.7,3,3,1,2,1,null,null,null,12.5,12,13]
[null,null,null,null,null,null,null,"P_Mg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,4.5,3.75,5.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,5,1,null,null,null,null,null,null,13,12,14.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Basisveen soms niet aanwezig, dan is het lagunaire klei"]
[13,33,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Voorbeeldsonderingen S25E03815 en S25E03799 (dikke Eem-klei)"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,4,2,1,2,1,null,null,null,12.75,12,13]
[null,null,null,null,null,null,null,"P_Mp_k",1,9,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,4.75,4,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,6,1,null,null,null,null,null,null,15.75,15.25,16]
[13,35,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"H_Mr_kz",0.8,1,1,null,null,null,null,null,null,6.5,5.75,7.75]
[null,null,null,null,null,null,null,"H_Ml_ko",0.8,2,1,1,2,1,null,null,null,10,9.5,10.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"inclusief lokaal dun (dunner dan 0.5m) basisveen"]
[null,null,null,null,null,null,null,"P_Mp_k",1,6,1,null,null,null,null,null,null,30.5,30,31]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,5.5,2.5,6.25]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,4,1,null,null,null,null,null,null,12.5,12,13]
[null,null,null,null,null,null,null,"P_Gs_zg",1,9,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,3,2,null,null,null,null,null,null,10.5,10,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vooral zand, minder zandige klei,leem"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,27.75,27,28.5]
[null,null,null,null,null,null,null,"H_Mr_kz",1,1,1,null,null,null,null,null,null,2.25,1.75,2.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,3,2,1,1,1,null,null,null,10,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat zandlagen van "]
[null,null,null,null,null,null,null,"P_Mg_zm",1,7,1,null,null,null,null,null,null,34,32.5,39]
[null,null,null,null,null,null,null,"H_Ml_ko",1,3,1,null,null,null,null,null,null,13.5,13,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"inclusief dun (dunner dan 0.5m) basisveen"]
[null,null,null,null,null,null,null,"P_Gs_zg",1,8,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ml_ko",1,3,1,null,null,null,null,null,null,16.5,14.5,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"inclusief dun (dunner dan 0.5m) basisveen"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,24,21.25,26]
[]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,4,1,null,null,null,null,null,null,17,16,17.25]
[null,null,null,null,null,null,null,"P_Mp_k",0.2,7,2,1,1,1,null,null,null,28.5,28,29]
[null,null,null,null,null,null,null,"P_Ggs_zg",0.2,7,3,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,25.5,24,27]
[13,43,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S19H00032"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,12,10.5,13]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,25.5,24,27]
[null,null,null,null,null,null,null,"P_Mg_zm",0.4,6,2,1,1,1,null,null,null,35,32,38]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,5,1,null,null,null,null,null,null,15,13.5,16]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",1,4,1,null,null,null,null,null,null,10,9,11.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,5,1,null,null,null,null,null,null,13,12.5,13.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,8,1,null,null,null,null,null,null,32,30,33]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,6.5,6,7.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,28,27,30]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1.5,1.25,2.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,7,1,null,null,null,null,null,null,16,14.5,17]
[13,48,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.25]
[null,null,null,null,null,null,null,"H_Vbv_v",1,6,1,null,null,null,null,null,null,13.5,12,15.5]
[13,49,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,2,1,1,1,1,null,null,null,9,8,11]
[null,null,null,null,null,null,null,"P_Mg_zm",0.7,5,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,2,null,null,null,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,4,1,null,null,null,null,null,null,18.5,17,20]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,23,22,24]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6.25,6,6.5]
[null,null,null,null,null,null,null,"H_Mp_ko",0.5,5,2,null,null,null,null,null,null,12.25,11.5,12.75]
[13,52,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"rand duingebied, variabel maaiveld; S14C000143"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KR geul en Eem geul"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KR geul en Eem geul"]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.4,3,1,null,null,null,null,null,null,16.5,16,17.5]
[]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.4,3,1,null,null,null,null,null,null,16.5,16,17.5]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,3,2,1,2,1,null,null,null,13.5,11.5,14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Variabele samenstelling met zandige kleilagen tot 2.5m dik"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KR geul en Eem geul"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,1,1,1,3,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,1,1,1,4,1,null,null,null,9.75,9.25,10.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top soms organische klei"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,2,0.7,4,1,1,2,1,9.25,9,9.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top soms organisch"]
[null,null,null,null,null,null,null,"P_Gs_zg",1,4,1,null,null,null,null,null,null,37,35,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drente Schaarsbergen grof zand met bovenop dun grof Eem-zand"]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,9,8.75,9.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokale dunne veenlaagjes en zandlaagjes en is soms wat organisch"]
[null,null,null,null,null,null,null,"P_Gs_zg",1,9,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Drente Schaarsbergen grof zand met bovenop dun grof Eem-zand"]
[null,null,null,null,null,null,null,"H_Mg_zm",0.5,1,2,null,null,null,null,null,null,20,16,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holocene geul; kleiig gelaagd"]
[13.1,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sterk opgehoogd tot ongeveer +2mNAP IJburg"]
[null,null,null,null,null,null,null,"H_Mg_zm",0.5,1,2,null,null,null,null,null,null,20,16,22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holocene geul; kleiig gelaagd"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,null,null,null,null,null,null,9,8.75,9.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms dunne dunner dan 25cm veenlagen en organische kleien"]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,3,1,null,null,null,null,null,null,16,15,17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vuile Boxtel met leem en veenlagen"]
[13.1,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sterk opgehoogd tot ongeveer +2mNAP IJburg; S25G00715"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.9,1,1,1,1,1,3.5,3,4]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,1,2,1,3,1,null,null,null,10.5,10,10.75]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,13.5,12,15]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2.25,1.5,3.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,5,1,null,null,null,null,null,null,15,14.5,15.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hierin opgenomen ook een dunne (dunner dan 1m) kleilaag bovenop het basisveen"]
[14,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Segment ligt op het sluizencomplex Ijmuiden (Noordzeekanaal) dus veel afgegraven"]
[null,null,null,null,null,null,null,"H_Mp_ko",1,3,1,null,null,null,null,null,null,19,18.5,19.5]
[14,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-5]
[null,null,null,null,null,null,null,"H_Ova_zm",0.3,2,2,1,2,1,null,null,null,18,17.5,18.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeezand"]
[null,null,null,null,null,null,null,"P_Mg_zm",0.9,6,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,2,2,null,null,null,null,null,null,17,16,18.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis klei sporadisch dun basisveen (dunner dan 25cm)"]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,1,1,1,1,1,null,null,null,1.25,1,1.5]
[null,null,null,null,null,null,null,"H_Mp_ko",0.2,1,2,1,3,1,null,null,null,4.5,4,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Klei met veenlagen"]
[14,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Segment bevat diverse kleine strandwalletjes haaks op de dijk, tot een breedte van maximaal 100 meter. Daartussen liggen klei,veen pakketten, afgezet in de beschutting van de strandwalletjes."]
[null,null,null,null,null,null,null,"H_Mg_zm",1,2,1,null,null,null,null,null,null,22.5,21,23]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,32,30,35]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,4.5,3.75,5.5]
[null,null,null,null,null,null,null,"H_Mg_zf",0.2,4,2,null,null,null,null,null,null,22,18,28]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,4.75,4.25,5.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,7,1,null,null,null,null,null,null,14.5,14,15]
[14,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,3,1,1,3,1,null,null,null,12.25,11.75,12.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.2,6,2,1,1,1,null,null,null,20,19,21]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,5,4.5,5.25]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,7,1,null,null,null,null,null,null,15,14.5,15.5]
[null,null,null,null,null,null,null,"H_Mp_ko",1,1,1,null,null,null,null,null,null,2,1.75,2.25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,1,1,2,1,null,null,null,20.5,19.5,21]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gestuwd"]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,3,1,1,2,1,null,null,null,12,11.5,12.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,6,1,null,null,null,null,null,null,18.5,17.5,20]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,5,3,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anthropogeen, verschillende lithologieen, ook puin, beton, hout etc."]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,27.5,26,30]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,4,3,10]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,12.5,12,13]
[null,null,null,null,null,null,null,"P_Mp_k",0.8,8,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,2,2,1,1,1,null,null,null,5.5,4.75,6]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,6,1,null,null,null,null,null,null,19.5,16,21]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,1,1,1,1,1,null,null,null,4.5,2,5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,2,1,null,null,null,null,null,null,16,14,18]
[]
[14,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,2,1,2,1,null,null,null,6,5.5,9]
[null,null,null,null,null,null,null,"H_Mp_ko",0.8,2,2,null,null,null,null,null,null,11,10,13]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,1,1,1,null,null,null,3.5,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S25G12943 voorbeeld van H_Mkw_zenk op H_Mp_ko op Boxtel op dikke Eem"]
[null,null,null,null,null,null,null,"H_Mp_ko",0.8,2,2,null,null,null,null,null,null,9,7,11]
[14,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[]
[null,null,null,null,null,null,null,"H_Rk_ko",1,3,1,null,null,null,null,null,null,6.5,4.5,11]
[]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,6.5,5.5,8]
[14,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.5,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,1,1,1,2,1,null,null,null,6.5,5.5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S31E00304 voorbeeld van ingesneden Holocene geul tot in dekzand"]
[null,null,null,null,null,null,null,"H_Rk_k",0.2,1,2,1,1,1,null,null,null,2.5,2,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S31E00555 voorbeeld van zandige oeverwal op basisveen op dekzand"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,1,1,1,null,null,null,9,8,9.5]
[14,23,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,1,1,null,null,null,null,null,null,2,1.5,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S31H000954 voorbeeld van H_Rk_ko op H_Vhv_v"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,4,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.25,1,2,1,1,1,null,null,null,2,1.5,3.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,2,2,1,2,1,null,null,null,36,33,40]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,2.5,1.75,5]
[]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,1,1,1,1,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"H_Eg_z&k",1,2,1,null,null,null,null,null,null,14,12,15]
[null,null,null,null,null,null,null,"H_Rk_k",0.95,1,1,0.7,1,1,1,1,1,3,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk smalle ondiepe zandige geultjes"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.95,1,1,0.7,1,1,1,2,1,4.5,3.5,6]
[null,null,null,null,null,null,null,"H_Rg_zm",0.95,1,1,0.1,2,2,1,2,1,11,9,16]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,2,1,null,null,null,null,null,null,15,14,16]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,5,4,7.75]
[null,null,null,null,null,null,null,"H_Rk_ko",0.25,3,2,1,3,1,null,null,null,12.5,12,13]
[]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,3,2,1,1,1,null,null,null,10,9.5,11]
[null,null,null,null,null,null,null,"P_Rg_zg",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,3,1,1,1,1,null,null,null,11,10.75,11.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",0.8,1,1,1,3,1,null,null,null,10,7,11]
[]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,11,9.25,12]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,29.5,28,31]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,2.5,1.75,3.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,32,31,33]
[null,null,null,null,null,null,null,"H_Rk_ko",0.7,3,1,null,null,null,null,null,null,10,9.5,10.25]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",1,3,1,null,null,null,null,null,null,9,7,9.25]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,4,2.5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",0.75,2,1,null,null,null,null,null,null,5.5,4,7]
[14,41,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Rg_zm",0.25,1,2,1,2,1,null,null,null,13,8.5,15]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,2,2,null,null,null,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,8,6,10]
[null,null,null,null,null,null,null,"H_Rg_zg",0.15,2,2,null,null,null,null,null,null,8,6,10]
[null,null,null,null,null,null,null,"H_Rk_ko",0.5,2,1,null,null,null,null,null,null,2,1.25,3.75]
[14,48,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mogelijk dunne (dunner dan 2m) klei-,leemlagen rond -25m NAP."]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,1,null,null,null,null,null,null,16,15,18]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.3,2,4,1,3,1,null,null,null,16,15,16.5]
[]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.95,2,1,1,1,1,1,2,1,8,7,9]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,2,1,2,1,null,null,null,12,11,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nieuwe Maasbedding"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,27,23,31]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k&v",1,2,1,1,1,1,1,2,1,8,7,9]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,17,16.5,17.5]
[14,53,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-3]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.9,2,1,0.8,2,1,1,2,1,15,14,16]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,2,2,1,1,1,null,null,null,10,5,13]
[14,54,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-3]
[null,null,null,null,null,null,null,"H_Rk_k&v",1,2,1,0.2,2,2,null,null,null,14,13.5,15.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,2,1,1,4,1,null,null,null,16.5,16,17]
[14,55,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-3]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.3,2,2,1,1,1,null,null,null,8,7.5,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat vaak 1 tot 2 veenlagen van 1-3 m dik"]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,17,16.5,17.5]
[14,56,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld lokaal 0 m NAP"]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,3,2,7]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.7,2,1,0.15,2,2,null,null,null,16.5,16,17]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,17,16.5,17.5]
[14,57,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld lokaal 0 m NAP"]
[null,null,null,null,null,null,null,"H_Mp_ko",1,4,1,null,null,null,null,null,null,9,8.5,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat lokaal veenlagen van 0.5-1 m"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.15,5,2,1,2,1,null,null,null,21,20,23]
[null,null,null,null,null,null,null,"H_Mp_ko",0.7,1,1,null,null,null,null,null,null,4,2.5,5.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.85,4,1,0.3,1,2,null,null,null,18,17,19]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,2,2,1,1,1,null,null,null,2.5,2,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Met veel zandlaagjes"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.85,3,1,1,2,1,null,null,null,20,19,22]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Beneden 32 m -NAP plaatselijk kleiig (Formatie van Waalre)"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,3,1,null,null,null,null,null,null,4.5,3.5,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Met veel zandlaagjes"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,3,2,1,1,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Mg_zm",0.7,5,1,null,null,null,null,null,null,18.5,18,19.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat kleiige zandlagen van meer dan 1 m dik"]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,0,-0.5,0.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.1,2,2,1,3,1,null,null,null,4,3.5,4.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,5,1,null,null,null,null,null,null,19.5,19,23]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,0.6,1,2,null,null,null,7,6,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,2,1,1,2,1,null,null,null,7,6,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.75,1,2,1,2,1,null,null,null,3,2,4.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.85,4,1,1,2,1,null,null,null,20.5,19,24]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,17,15,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maeslantkering"]
[]
[14,66,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-5.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,3,2,1,2,1,null,null,null,7.5,5.5,8]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,2,2,null,null,null,null,null,null,7,4,8]
[null,null,null,null,null,null,null,"H_Mg_zm",0.1,5,2,null,null,null,null,null,null,22,20,24]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,2,1,1,2,1,null,null,null,19,18.5,19.5]
[14,69,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uitwaterende sluis Katwijk"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,3,2,1,1,1,null,null,null,9,7,11]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,3,2,1,3,1,null,null,null,12.5,12,13]
[15,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.3,3,1,1,3,1,null,null,null,13.75,13.5,14]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,34.5,33.5,35.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",0.9,3,1,null,null,null,null,null,null,12,11.25,13]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,5,1,null,null,null,null,null,null,14.5,13.5,15.5]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,3,2.25,4.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk smalle ondiepe zandige geultjes"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,3,2,1,2,1,null,null,null,12,10,14]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7.5,5,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",1,3,1,null,null,null,null,null,null,10.5,10.25,12.25]
[15,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,2]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,1,1,1,2,1,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,20,10,25]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,1,1,1,1,null,null,null,0.75,0.5,2]
[null,null,null,null,null,null,null,"H_Rg_zm",0.15,1,1,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.85,1,2,1,3,1,null,null,null,2.75,2.5,3]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.03,1,1,1,3,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,12,9,15]
[null,null,null,null,null,null,null,"H_Rg_zm",0.7,1,1,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.27,1,3,0.5,2,2,null,null,null,2.75,1.25,3.25]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,3,1,null,null,null,null,null,null,27,25,32]
[15,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Rg_zm",0.25,3,1,1,2,1,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,1,1,1,1,null,null,null,18,13,32]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.02,2,3,null,null,null,null,null,null,3.5,2.5,4.5]
[null,null,null,null,null,null,null,"H_Rk_k&v",1,3,1,null,null,null,null,null,null,5.75,5.25,6.75]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,7,1,1,2,1,null,null,null,21,20,22]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,2,2,1,2,1,null,null,null,3,2,6]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,23,20,25]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,0.5,0,1.5]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.25,3,3,null,null,null,null,null,null,9,7,10]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,6,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",1,3,1,null,null,null,null,null,null,10,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelmatig fijnzandige trajecten"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,6,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,1,1,1,3,1,null,null,null,3.5,3,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat ingeschakelde kleilagen"]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,5.25,4.75,5.75]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,7,2,1,1,1,null,null,null,22,18,24]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,7,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.75,1,1,1,3,1,null,null,null,3,2,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat ingeschakelde kleilagen"]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.5,2,2,null,null,null,null,null,null,5.5,4.5,7.25]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,7,2,1,1,1,null,null,null,22,18,24]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,2,1,1,1,1,null,null,null,5,0,6]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.8,3,2,null,null,null,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,7,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,2,1,1,1,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Rg_zf",0.15,2,3,1,3,1,null,null,null,6.5,6,8.25]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.65,1,1,1,3,1,null,null,null,4.25,3.75,5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,3,1,2,1,null,null,null,1,0.75,1.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,4,1,null,null,null,null,null,null,10,9,10.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Naar beneden toe kleiiger en soms overgaand in gyttja"]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,5,1,null,null,null,null,null,null,10.75,10,12.25]
[15,22,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.75,1,1,0.35,2,2,1,2,1,6.25,5.5,6.75]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.75,1,1,0.4,3,2,1,2,1,11,10.5,11.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,1,1,1,null,null,null,1.75,1.25,7]
[null,null,null,null,null,null,null,"H_Rk_k",0.8,1,1,0.6,1,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Rk_k",0.15,1,2,0.6,1,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,1,3,1,2,1,null,null,null,11.25,10.75,13]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,2,1,1,1,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,2,3,1,2,1,null,null,null,7,6.5,7.5]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.5,3,2,1,1,1,null,null,null,12.5,12,13]
[15,25,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,2,2,1,3,1,null,null,null,9.5,8.5,10.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,2,3,1,1,1,null,null,null,9.5,8.5,10.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,15,14,16]
[15,26,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,2,2,1,2,1,null,null,null,6.5,6,8]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.5,3,1,1,3,1,null,null,null,12.5,12,13]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,6,2,null,null,null,null,null,null,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,2,1,1,3,1,null,null,null,9,8,11]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.5,3,1,1,3,1,null,null,null,12.5,12,13]
[]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.1,3,1,null,null,null,null,null,null,13,12,14]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,2,null,null,null,null,null,null,40]
[null,null,null,null,null,null,null,"H_Rk_k&v",1,4,1,null,null,null,null,null,null,8.5,7.5,10]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,2,1,1,1,1,null,null,null,4,3,4.5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.2,2,1,1,2,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Rk_k",0.6,1,1,1,1,1,null,null,null,2,0.5,2.75]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,2,2,1,1,1,null,null,null,5,4.5,5.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,3.5,2.25,4.5]
[16,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,3,2,1,1,1,null,null,null,3.5,3.25,4.75]
[]
[]
[null,null,null,null,null,null,null,"H_Rk_ko",0.5,2,2,1,1,1,null,null,null,6,5.5,6.5]
[16,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,1.75,1.5,2.5]
[]
[]
[16,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",1,2,1,null,null,null,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,1,0.5,1.5]
[]
[16,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zie S38F001126"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,1,2,1,3,1,null,null,null,4.75,4.5,5.5]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,-0.5,-1,0]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,2,2,1,1,1,null,null,null,1,0,2.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,10,8,12]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,2,1,1,2,1,null,null,null,3,2.5,4.5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,2,3,1,1,1,null,null,null,3,2.5,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat ook veenlagen tot 1m dik"]
[]
[16,19,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld wordt lager naar westen toe; S38F02353 met organische klei en Basisveen"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.15,2,1,1,4,1,null,null,null,5,4,5.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,8,7,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top vaak een dunne kleilaag tot 1m dik"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,2,1,1,1,1,null,null,null,1,0,2.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,2,1,2,1,null,null,null,7.5,6.5,8]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.35,2,1,1,3,1,null,null,null,4.5,4,5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,2,3,1,2,1,null,null,null,4.5,4,5.5]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,-0.75,-1,-0.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,2,1,2,1,null,null,null,6,5.5,8]
[]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.4,2,1,1,3,1,null,null,null,6.5,4,7.5]
[16,24,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld wordt lager naar westen toe; S38F02118 voor kleiige opvulling; S38F02120 voor Holoceen zand op Basisveen"]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,-0.75,-1,-0.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.15,2,1,1,5,1,null,null,null,6.25,6,7]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,10,8,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top vaak een dunne kleilaag tot 1m dik"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,1,1,1,4,1,null,null,null,6.25,5,7]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,1,3,1,2,1,null,null,null,6.25,5,7]
[null,null,null,null,null,null,null,"P_Rg_zg",0.1,3,1,1,3,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Urk en Sterksel"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.25,1,1,1,2,1,null,null,null,3,2,5]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.25,1,2,1,3,1,null,null,null,8,7,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rivierduin"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.25,1,4,1,1,1,null,null,null,2,1,3]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,11,10,15.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top vaak een dunne kleilaag tot 1m dik"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.8,1,1,1,2,1,null,null,null,3.5,1,4]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,2,1,1,1,null,null,null,1,0,1.5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.15,1,2,1,2,1,null,null,null,2,1,4.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,0.5,1,1,1,1,1,0,-1,2]
[16,28,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S38E00454"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.2,1,1,1,5,1,null,null,null,7.5,6.5,8.75]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,1,3,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,11,10,15.5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.6,1,1,1,2,1,null,null,null,2,1.5,3.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,2,1,1,1,null,null,null,0.5,0,2]
[null,null,null,null,null,null,null,"H_Rk_ko",0.15,1,3,1,2,1,null,null,null,2,1.5,3.5]
[null,null,null,null,null,null,null,"H_Vbv_v",0.15,1,3,1,7,1,null,null,null,8.5,8,9.75]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Kreftenheye, Urk en Sterksel"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,1,0.7,1,1,1,1,1,1,0,3]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,2,1,1,1,null,null,null,7.5,7.5,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zand soms ook zeer grof"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,2,1,2,1,null,null,null,8.5,8,9.75]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Kreftenheye, Urk en Sterksel"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,1,1,3,1,null,null,null,9,8.5,9.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,3,1,1,1,null,null,null,1,0,1.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,3,1,6,1,null,null,null,9.5,9,10.75]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,13.5,11.75,15.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.8,2,1,1,1,1,null,null,null,10,8,10]
[]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.35,1,1,1,5,1,null,null,null,13,12.5,14]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.3,1,3,1,1,1,null,null,null,4.5,3,5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.05,1,4,1,4,1,null,null,null,13,12.5,14]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.33,1,1,1,2,1,null,null,null,12,11.5,12.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Kreftenheye, Urk en Sterksel"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,1,2,1,2,1,null,null,null,8,6,8.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,3,0.3,1,2,1,1,1,4.5,2,5.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,4,0.3,1,2,1,1,1,4.5,2,5.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,1,4,1,6,1,null,null,null,13,12,15]
[null,null,null,null,null,null,null,"H_Vhv_v",0.15,1,1,1,2,1,null,null,null,4.5,4,6]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,2,0.7,1,2,1,1,1,4.5,2,5.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,3,null,null,null,null,null,null,11.5,10,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandige klei met organische kleilagen ertussen"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,35,34,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Kreftenheye en Urk"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.15,1,1,1,2,1,null,null,null,6,5.5,8]
[null,null,null,null,null,null,null,"P_Rg_zm",0.15,1,1,1,5,1,null,null,null,14,13,15]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.3,1,2,1,5,1,null,null,null,11,10,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Donk"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,1,3,1,null,null,null,10.5,8.5,11.5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.05,1,3,1,4,1,null,null,null,13,12,13.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,6,0.5,1,1,1,1,1,6,5,7]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.3,1,6,1,5,1,null,null,null,11.5,10,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wychen"]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.7,1,1,0.3,1,1,1,1,1,11.75,10.5,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sterk organische klei met dunne veenbanden"]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.7,1,1,0.2,3,1,1,1,1,13,12,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rivierduin"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.25,1,2,1,4,1,null,null,null,13.5,13,14]
[]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.6,1,1,0.3,1,2,1,3,1,11.5,10.5,12]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,1,1,0.2,1,4,1,3,1,9,8,10]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.6,1,1,0.8,3,2,1,1,1,14,13,16]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,1,1,1,null,null,null,3.5,2,4]
[16,40,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.25]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.7,1,1,0.2,1,3,1,1,1,5,3.5,7]
[null,null,null,null,null,null,null,"H_Rg_zm",0.7,1,1,0.2,1,3,1,2,1,6.5,6,7]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.7,1,1,0.2,1,4,1,4,1,10.5,9,11]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,3,null,null,null,null,null,null,12,10,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Crevasse opvulling"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,1,1,2,1,null,null,null,13.5,13.5,15]
[16,42,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veel verstoring door ophoging etc. S38C02637 voor zandige ondergrond (betrouwbaar), andere sonderingen twijfelachtig betreft locatie (S38C02619,2620,2621)"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,1,3,0.5,3,1,1,1,1,12.75,12,13.5]
[16,43,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S38C02575 zandige geulopvulling, S38C02581 zandige geul met organische klei halverwege."]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.2,1,1,1,5,1,null,null,null,13,12,14]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,25,24,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Kreftenheye"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.35,1,1,1,1,1,null,null,null,4.25,3.5,4.75]
[null,null,null,null,null,null,null,"H_Rk_ko",0.35,1,2,1,1,1,null,null,null,3.25,2.25,4]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,3,1,2,1,null,null,null,6,3.5,7.75]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,25,24,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Kreftenheye"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Waalre"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.25,1,1,1,3,1,null,null,null,8,7,10]
[null,null,null,null,null,null,null,"H_Rk_vk",0.3,1,2,1,2,1,null,null,null,10,9,12]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,2,null,null,null,null,null,null,30,25,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Kreftenheye en Sterksel; bevat sporadisch dunne kleilagen tot 2m dik"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,1,1,1,2,1,null,null,null,6.5,5,8]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,2,1,1,1,null,null,null,11,10,14]
[null,null,null,null,null,null,null,"H_Vbv_v",0.55000000000000004,1,3,1,4,1,null,null,null,10,9.75,10.25]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. van Waalre; deels zandig onwikkeld"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,2,0.5,1,1,1,1,1,2,1.5,3.5]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.3,1,3,0.6,1,1,1,1,1,3.5,3,5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,4,1,1,1,null,null,null,2,1,4]
[null,null,null,null,null,null,null,"H_Rk_k",0.5,1,1,1,1,1,null,null,null,2,1.75,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk organische klei"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,1,1,0.3,3,3,1,2,1,9,8.5,9.25]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.5,1,1,0.3,3,3,1,3,1,9.5,9,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wychen"]
[null,null,null,null,null,null,null,"H_Rk_k",0.25,1,4,1,1,1,null,null,null,4,3,6]
[]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,25,24,27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenste 4-5 m kan kleiig zijn"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.1,2,1,1,1,1,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"H_Eg_zm",0.3,3,1,null,null,null,null,null,null,16,15.5,18]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,6.5,6,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal circa twee meter dik"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,5,2,1,2,1,null,null,null,17,16.5,17.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.45,1,1,1,1,1,null,null,null,5,4,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk weinig zandlaagjes"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.45,1,2,1,3,1,null,null,null,11,10,12]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.85,3,2,1,2,1,null,null,null,17,16.5,17.5]
[17,5,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,"H_Mp_ko",1,1,1,null,null,null,null,null,null,7,5,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk weinig zandlaagjes"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.7,4,2,1,2,1,null,null,null,17,16.5,17.5]
[17,6,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.75,4,2,1,1,1,null,null,null,15.5,13,16.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tussen H_Rk_kenv en P_Rk_kens plaatselijk 1-1.5 m zand"]
[]
[null,null,null,null,null,null,null,"H_Rk_ko",0.45,3,1,1,2,1,null,null,null,10,9.5,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms sterk siltig,zandig"]
[null,null,null,null,null,null,null,"H_Rk_k",0.5,5,1,null,null,null,null,null,null,16,15.5,18]
[17,8,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,2,1,0.4,1,2,0.5,2,2,9.5,8,11]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,3,1,1,2,1,null,null,null,23,21,28]
[]
[null,null,null,null,null,null,null,"H_Rk_ko",0.3,2,1,0.7,3,1,null,null,null,13.5,12.5,14.5]
[null,null,null,null,null,null,null,"H_Rg_zf",0.6,2,2,1,2,1,null,null,null,13.5,12.5,14.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,24,22,27]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",0.95,1,1,0.7,2,1,null,null,null,11,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat veenlagen dunner dan  1m dik"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,1,2,0.5,2,2,1,2,1,11,9,12]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,0.5,0,3]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,2,1,0.5,1,2,null,null,null,11,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat organische kleilagen dunner dan  1m dik"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,3,1,null,null,null,null,null,null,23,22,25]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,1,0.5,1,1,1,1,1,2,1,3.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat organische kleilagen dunner dan  1m dik"]
[null,null,null,null,null,null,null,"H_Rg_zf",0.05,1,2,1,2,1,null,null,null,13,11,14.5]
[17,13,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"plaatselijk opgehoogd en vergraven (bebouwing)"]
[null,null,null,null,null,null,null,"H_Mp_k",0.15,1,2,1,1,1,null,null,null,1,0.5,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat organische kleilagen dunner dan  1m dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dikker dan 2 m en aaneengesloten"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.85,1,1,0.9,1,1,0.3,2,2,7,6,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bevat organische kleilagen dunner dan  1m dik"]
[null,null,null,null,null,null,null,"H_Rg_zf",0.15,1,2,1,2,1,null,null,null,13,10,14.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,2,1,null,null,null,null,null,null,22,21,30]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.65,1,1,0.8,1,1,1,1,1,3,2,5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,1,3,1,1,1,null,null,null,13,12,14]
[null,null,null,null,null,null,null,"H_Rg_zf",0.05,1,5,1,2,1,null,null,null,13,12,14]
[]
[null,null,null,null,null,null,null,"H_Rk_k",0.5,1,1,1,2,1,1,1,1,16,14,19]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,1,4,1,2,1,null,null,null,16,14,19]
[null,null,null,null,null,null,null,"P_Rg_zf",0.3,2,2,null,null,null,null,null,null,22,21,30]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,1,0.2,1,2,1,1,1,5,4,6]
[null,null,null,null,null,null,null,"H_Rk_k",0.1,1,3,1,2,1,null,null,null,18,17,19]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,2,1,null,null,null,null,null,null,22,21,30]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,1,0.8,1,1,1,1,1,4,3,5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,2,1,2,1,null,null,null,6,5,9]
[null,null,null,null,null,null,null,"H_Mp_ko",0.2,1,2,1,3,1,null,null,null,13,12,16]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.1,1,4,1,2,1,null,null,null,15,14,16]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,1,2,1,2,1,null,null,null,7.5,7,8]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.75,2,2,1,2,1,null,null,null,18,17.75,19]
[null,null,null,null,null,null,null,"H_Vhv_v",0.15,1,1,1,2,1,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"H_Vhv_v",0.15,1,3,1,2,1,null,null,null,11.5,10,14]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,2,2,1,2,1,null,null,null,13.5,12.5,15]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,5,1,1,1,1,null,null,null,11.5,10.5,12]
[null,null,null,null,null,null,null,"P_Ova_sd",1,8,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,2,1,1,1,1,null,null,null,6,5.5,6.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,2,1,1,2,1,null,null,null,7,6.5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk organische klei-insluitingen"]
[null,null,null,null,null,null,null,"H_Vhv_v",1,4,1,null,null,null,null,null,null,12,10.5,14]
[19,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-3]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.7,3,1,null,null,null,null,null,null,17,16,18]
[]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.4,2,3,1,1,1,null,null,null,5,4,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenste 2 meter lokaal slappe klei"]
[null,null,null,null,null,null,null,"P_Rk_k&s",1,4,1,null,null,null,null,null,null,19,18.5,19.5]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.6,1,2,1,1,1,null,null,null,5,4,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenste 2 meter lokaal slappe klei"]
[null,null,null,null,null,null,null,"H_Mg_zm",0.7,2,2,1,2,1,null,null,null,17,16,18]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.7,1,1,1,1,1,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.2,2,2,1,1,1,null,null,null,12,11,13]
[]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.2,2,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.8,2,2,1,1,1,null,null,null,7.5,6,8]
[null,null,null,null,null,null,null,"H_Mg_zm",0.4,3,2,1,2,1,null,null,null,19,18.5,19.5]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,0.5,0,1.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.95,3,1,0.5,1,2,1,2,1,19.5,19,22]
[null,null,null,null,null,null,null,"H_Mg_zm",0.05,3,2,0.5,1,2,1,2,1,20,19.5,21]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,2,2,null,null,null,null,null,null,9,7.5,10]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.5,4,2,null,null,null,null,null,null,20,19,21]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,0.5,0,1.5]
[null,null,null,null,null,null,null,"H_Mg_zm",0.25,6,1,1,1,1,null,null,null,11,10,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat kleiige lagen van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,9,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.05,1,2,null,null,null,null,null,null,5.5,5,6]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"H_Mp_ko",0.5,1,1,1,4,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Mg_zm",1,3,1,null,null,null,null,null,null,16.5,13.5,17]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,1,1,2,1,null,null,null,5.75,4,6.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veendikte constant 1.5-2 m. Variatie vooral in diepteligging."]
[null,null,null,null,null,null,null,"H_Mg_zk",1,3,1,null,null,null,null,null,null,18,17.5,22]
[]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,1,0.5,3,1,1,1,1,5.25,5,5.75]
[null,null,null,null,null,null,null,"H_Mg_zm",1,2,1,null,null,null,null,null,null,14.5,13.5,15.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre Formatie mogelijk niet continu"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,2,null,null,null,null,null,null,5.25,4.75,7]
[null,null,null,null,null,null,null,"H_Mg_zk",0.6,4,2,1,1,1,null,null,null,8.5,8,11]
[20,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.85,1,1,1,1,1,null,null,null,1,0.5,3.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.15,1,2,1,2,1,null,null,null,5.25,4.75,7]
[null,null,null,null,null,null,null,"H_Mg_zm",0.5,3,2,1,2,1,null,null,null,14,12.5,15]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,2.25,2,3.75]
[null,null,null,null,null,null,null,"H_Mg_zm",1,7,1,null,null,null,null,null,null,16,15,17]
[20,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,5,1,1,1,1,null,null,null,7,6,7.5]
[null,null,null,null,null,null,null,"H_Ova_zm",1,8,1,null,null,null,null,null,null,20.75,20.25,21.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vermoedelijk aangeklopt strandzand"]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,2.75,2.25,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen altijd aanwezig"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.35,3,1,1,5,1,null,null,null,21,19.5,22]
[null,null,null,null,null,null,null,"H_Mg_zm",0.5,3,3,null,null,null,null,null,null,21,19.5,23]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,2,2,null,null,null,null,null,null,2.5,2,3.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,4,1,null,null,null,null,null,null,21,20,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan zeer dun basisveen bevatten"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_zf",0.5,1,1,0.8,1,2,1,2,1,1,0.75,2.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.5,1,2,0.8,1,2,1,2,1,1,0.75,2.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.65,4,2,1,2,1,null,null,null,18.5,16.5,20.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,1,null,null,null,null,null,null,4.5,3.5,5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,25,23,27]
[20,14,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mg_zm",0.5,2,2,null,null,null,null,null,null,20,19,21]
[20,15,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(achter de dijk ligt een kanaal)"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.5,3,1,1,2,1,null,null,null,19,18,20]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,5,1,null,null,null,null,null,null,40]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.7,3,1,null,null,null,null,null,null,10,9,11]
[null,null,null,null,null,null,null,"P_Rg_zm",0.75,5,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"P_Rg_zm",0.25,5,2,null,null,null,null,null,null,25,23,27]
[20,17,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mv plaatselijk lager en waterbodem"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.75,3,1,1,2,1,null,null,null,25,23,27]
[20,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mv plaatselijk lager en waterbodem"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.75,3,1,1,1,1,null,null,null,21.5,20.5,23]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zm",1,3,1,null,null,null,null,null,null,8,7,10]
[null,null,null,null,null,null,null,"P_Rg_zm",0.25,5,2,null,null,null,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"H_Mr_kz",1,1,1,null,null,null,null,null,null,1.5,1,2.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.75,4,1,1,2,1,null,null,null,25,23,27]
[]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,2,2,null,null,null,null,null,null,15,12,16]
[null,null,null,null,null,null,null,"H_Mg_zm",1,3,1,null,null,null,null,null,null,23,20,29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"regelmatig fijn zand,kleiig zand lagen"]
[null,null,null,null,null,null,null,"H_Mg_zm",1,2,1,null,null,null,null,null,null,23,20,29]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,null,null,null,null,null,null,10,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"vnl. Zand"]
[21,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.1,2,1,1,4,1,null,null,null,15,14,19]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.15,2,2,0.6,1,2,1,2,1,18.5,17.5,23]
[null,null,null,null,null,null,null,"H_Mr_kz",0.4,2,4,0.4,1,1,1,1,1,10,8,14]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,26,23,30]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,2,1,1,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",1,5,1,null,null,null,null,null,null,10,9,12.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,9,1,null,null,null,null,null,null,30,28,35]
[null,null,null,null,null,null,null,"H_Mp_ko",0.2,1,1,1,3,1,null,null,null,4.5,3.5,5]
[null,null,null,null,null,null,null,"H_Mp_ko",0.8,1,2,1,3,1,null,null,null,8.5,8,9]
[null,null,null,null,null,null,null,"H_Eg_z&k",1,2,1,null,null,null,null,null,null,14,13.5,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat zandlagen van meer dan 2 m dikte. Vooral tussen 10 en 12 m -NAP"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,33,30,35]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,1,1,2,1,null,null,null,3.5,3,4]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.3,2,1,null,null,null,null,null,null,10,7,11]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,33,30,35]
[null,null,null,null,null,null,null,"H_Mg_zm",0.6,1,1,0.25,1,1,1,2,1,4,3,4.5]
[null,null,null,null,null,null,null,"H_Mg_zm",0.6,1,1,1,4,1,null,null,null,15,12.5,16.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms fijnzandig tussen 11-13 m -NAP"]
[null,null,null,null,null,null,null,"H_Eg_z&k",1,2,1,null,null,null,null,null,null,18,17,21]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,0.75,1,2,null,null,null,2,1.5,3]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,1,2,1,3,1,null,null,null,9,8,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,28,26,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer zelden dunne Wijchen laag"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.35,1,1,1,3,1,null,null,null,4,3.5,4.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.65,1,2,1,3,1,null,null,null,6.5,5.5,7]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,2,2,1,1,1,null,null,null,23,21,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bovenste 4-5 m bevat fijne zandlagen"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,2,2,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Waalre"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,1,1,1,3,1,null,null,null,8,6,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms weinig organisch"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.15,1,2,1,3,1,null,null,null,22,20,25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,4,0.15,1,2,1,2,1,6,5,6.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,2,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,1,1,0.7,2,1,1,1,1,4.25,4,4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal 0.5 m dik"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,1,2,0.9,1,2,1,2,1,6.5,6,7]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,20,19,33]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,1,0.7,1,2,null,null,null,3,1,4]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,1,1,1,6,1,null,null,null,40,40,40]
[21,11,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,1,1,1,4,1,null,null,null,13.5,12.5,15]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,1,2,1,5,1,null,null,null,13.5,12.5,15]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.3,1,3,null,null,null,null,null,null,18,16,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelmatig zeer kleiige trajecten van meerder meters dik"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,2,null,null,null,null,null,null,3,2.5,4]
[null,null,null,null,null,null,null,"P_Ova_sd",1,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,1,1,1,3,1,null,null,null,4.25,3.75,5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,3,1,2,1,null,null,null,5.75,5,6.25]
[]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,1,2,1,1,1,null,null,null,5,3.5,6]
[null,null,null,null,null,null,null,"H_Mp_ko",0.5,2,2,null,null,null,null,null,null,7.5,7,8]
[21,15,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,2,1,1,1,null,null,null,4.5,3.5,5.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,null,null,null,null,null,null,9.25,8.75,10.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nooit dikker dan 0.25 m en vrijwel altijd aanwezig. Soms afwezig ivm aanwezigheid, met klei opgevulde restgeul"]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,1,null,null,null,null,null,null,2,0.5,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Met humeuze trajecten"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.75,5,1,0.5,1,1,null,null,null,8.25,7.5,9.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.75,5,1,0.5,1,2,null,null,null,8.25,7.5,9.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,25,18,29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal fijnere bovenste 1-2 m. Lijkt niet direct op dekzand."]
[null,null,null,null,null,null,null,"H_Mp_ko",0.45,1,1,1,3,1,null,null,null,11.5,9.5,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms met dunne basisveenlaag op Pleistoceen zand. In extreme gevallen begint H_Mp_ko op -16 m NAP"]
[null,null,null,null,null,null,null,"H_Mp_ko",0.4,1,3,1,3,1,null,null,null,5.25,4.75,5.75]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.35,1,1,0.8,3,2,1,2,1,9,8,10]
[null,null,null,null,null,null,null,"H_Mg_zk",0.6,1,2,1,2,1,null,null,null,4.5,3,5.25]
[null,null,null,null,null,null,null,"H_Mg_zm",0.6,1,2,0.8,4,2,1,3,1,10.25,9.75,14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan tot Pleistoceen gaan"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,1,0.2,1,2,null,null,null,4.5,3,5.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,1,0.3,4,2,null,null,null,15.5,13.5,17.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_ko",0.6,1,1,1,3,1,null,null,null,5.25,3.75,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen maximaal 2 m dik"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,0.85,4,1,null,null,null,10,9,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelmatig dunne kleilaag (max 0.5 m dik) rond 8.5 m -NAP"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.3,1,2,1,2,1,null,null,null,4.25,3.5,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms met dunne basisveenlaag op Pleistoceen zand."]
[null,null,null,null,null,null,null,"H_Eg_z&k",0.1,1,3,1,1,1,null,null,null,17,16.5,18.5]
[21,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,2,1,2,1,null,null,null,7.5,6,9]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,26,24,35]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,1,0.1,1,2,1,1,1,2.25,1.5,4.25]
[null,null,null,null,null,null,null,"H_Vbv_v",0.3,1,1,1,4,1,null,null,null,9.5,9,10.5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.7,1,2,0.5,3,1,null,null,null,12,10.5,13.5]
[22,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.8,1,2,0.6,1,1,1,1,1,0,-0.25,0.75]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,15,12.75,16.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,1,1,2,1,null,null,null,7.5,7,9.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,1,1,1,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleipakket aan de top is maximaal 6 m. dik. "]
[null,null,null,null,null,null,null,"H_Vhv_v",0.75,1,1,1,3,1,null,null,null,5,4,5.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleipakket aan de top is tussen 7 en 12 m. dik. "]
[22,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," in noordelijk deel van dit segment tot opgehoogd tot maximaal 4 m. In overig deel 1 a 2 m. opgehoogd."]
[null,null,null,null,null,null,null,"H_Vbv_v",0.6,1,1,1,4,1,null,null,null,12.75,11.5,15]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,1,2,0.8,3,1,null,null,null,13.25,12.25,15]
[22,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Groot deel van dit segment opgehoogd tot maximaal 3.5 m."]
[null,null,null,null,null,null,null,"H_Rk_ko",0.8,1,1,0.8,3,1,null,null,null,11.5,10.75,12.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,2,1,2,1,null,null,null,7.25,5.25,9.5]
[22,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,1,0.5,3,2,null,null,null,11,10.25,12]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,1,2,1,2,1,null,null,null,6.5,4,9]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,1,2,0.3,3,1,null,null,null,12.5,11.75,14]
[23,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Vbv_v",0.6,1,1,1,4,1,null,null,null,9,8.25,9.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,31,30,34]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,1,1,1,2,1,null,null,null,3.75,1.75,4.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleiige traject bevatten"]
[null,null,null,null,null,null,null,"H_Rk_k",0.6,1,2,1,1,1,null,null,null,0,-0.5,1.25]
[null,null,null,null,null,null,null,"H_Rg_zg",0.6,1,2,0.7,4,2,null,null,null,10.5,8.5,11.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,1,1,1,1,null,null,null,0,-0.75,0.75]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.7,1,1,1,6,1,null,null,null,10.75,9.25,11]
[null,null,null,null,null,null,null,"H_Rg_zg",0.3,1,2,0.7,4,2,null,null,null,12,11.5,12.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.7,1,1,1,2,1,null,null,null,4,2.25,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleiige traject bevatten"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.7,1,1,1,6,1,null,null,null,10.75,9.25,11]
[null,null,null,null,null,null,null,"H_Rg_zg",0.3,1,2,0.7,4,2,null,null,null,12,11.5,12.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,28,25,30]
[null,null,null,null,null,null,null,"H_Rk_k",0.6,1,1,0.7,1,2,null,null,null,-0.75,-2,0.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,1,2,1,2,1,null,null,null,1.75,1,2.25]
[]
[null,null,null,null,null,null,null,"H_Rk_k",0.95,1,1,0.6,2,1,1,2,1,5,3.25,6]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,1,1,1,null,null,null,0.5,0,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld bij deze optie 0.5 -1 m +NAP"]
[24,3,3,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk bovenlaag sterk verstoord en opbracht ivm vestingwerken"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.1,1,1,1,5,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Rg_zm",0.35,1,3,1,2,1,null,null,null,9,8,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Met kleilagen van 0.1-0.5 m"]
[null,null,null,null,null,null,null,"H_Rk_k",0.95,1,1,0.4,1,1,null,null,null,1.5,0.75,2.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,0.15,3,2,1,1,1,5,4,6]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,1,1,1,null,null,null,1,0.5,4]
[24,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.75,1,1,0.7,1,1,1,1,1,1,0,1.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.75,1,1,0.6,3,1,1,2,1,5.5,4.5,6.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,8.75,8.25,9.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nooit dikker dan 2 m"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,1,0.1,1,2,null,null,null,2,1,3]
[null,null,null,null,null,null,null,"H_Rk_ko",0.8,1,1,0.7,2,2,1,2,1,9,8.5,10.75]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,1,null,null,null,null,null,null,7,6,8]
[24,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veel boringen op of dichtbij de dijk."]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,3,1,0.4,3,1,1,1,1,8,7.5,8.5]
[null,null,null,null,null,null,null,"H_Vbv_v",1,4,1,1,3,1,null,null,null,9.25,8.75,10]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,1,0.8,1,1,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,26,21.5,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan grofzandige trajecten bevatten."]
[null,null,null,null,null,null,null,"H_Rk_k",0.9,1,1,0.9,1,1,null,null,null,0,-0.5,0.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,0.1,1,2,null,null,null,0,-0.5,0.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,1,2,1,2,1,null,null,null,6.5,5.5,8]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,1,0.8,1,1,null,null,null,0,-0.75,0.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,2,1,2,1,null,null,null,4.25,3.75,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan grofzandige en grindige trajecten bevatten."]
[24,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,1,1,4,1,null,null,null,4,2.5,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan grofzandige en grindige trajecten bevatten."]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,3,1,2,1,null,null,null,5.5,4.5,7.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,1,1,1,1,null,null,null,-0.25,-0.75,0]
[null,null,null,null,null,null,null,"H_Rk_k",0.25,1,2,0.6,1,2,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,39,35,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,0.7,2,1,null,null,null,0.5,0,0.75]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,3,0.8,2,1,null,null,null,0.5,0,1.5]
[]
[24,15,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan leemlagen tot 2 m. bevatten."]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,1,0.8,2,2,null,null,null,2,0.25,3]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,2,0.8,2,2,null,null,null,4.25,3.5,4.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan een dun veenlaagje (max. 50 cm) bevatten."]
[24,17,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2]
[null,null,null,null,null,null,null,"H_Rg_zm",0.8,1,1,1,3,1,null,null,null,7.25,6.5,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleine kans op  grofzand."]
[24,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,4,2,null,null,null,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,2,null,null,null,null,null,null,-1,-2,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan een dun veenlaagje (max. 20 cm) bevatten."]
[]
[null,null,null,null,null,null,null,"H_Rk_k",0.9,1,1,0.4,4,1,null,null,null,7.5,7,8]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,21,20,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ten oosten van B42F0934 kan aan de basis lokaal dun basisveen voorkomen."]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,null,null,null,null,null,null,36.5,35.5,37.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,1,1,1,1,null,null,null,0,-0.5,5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.5,1,2,1,2,1,null,null,null,2.25,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Niet dikker dan 1.5 m"]
[]
[null,null,null,null,null,null,null,"H_Mp_zf",0.9,1,2,0.4,1,2,null,null,null,1.75,0.75,3.25]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,2,2,null,null,null,null,null,null,33,31,35]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,2,null,null,null,null,null,null,3.5,2.5,4]
[null,null,null,null,null,null,null,"P_Rg_zg",1,6,1,null,null,null,null,null,null,30.5,28.5,32.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,1,1,1,3,1,null,null,null,13,10,16.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Geleidelijk oplopend relief"]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.7,3,2,null,null,null,7.5,6,9]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,3,1,null,null,null,null,null,null,5,4.25,6]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,7,1,1,1,1,null,null,null,14.25,13,16.5]
[25,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,1,1,1,null,null,null,0.5,0,5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,3,0.3,1,1,null,null,null,3.25,2.5,4.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,1,3,0.5,4,1,1,2,1,12,10,13.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,3,2,1,1,1,null,null,null,25,22,28]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,1,2,1,2,1,null,null,null,20.25,19.25,21.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,1,3,1,4,1,null,null,null,20.25,19.25,21.25]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",1,3,1,null,null,null,null,null,null,28.5,26,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan top een kleine kans op klei en veen."]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan top kleipakket van 6 tot 9 m dikte."]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,14,13,16]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,1,null,null,null,null,null,null,25,18,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleilagen bevatten"]
[]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,2,1,1,1,null,null,null,0.5,0,2]
[null,null,null,null,null,null,null,"H_Mp_zf",0.8,1,2,1,2,1,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,1,7,1,null,null,null,10,7,13]
[null,null,null,null,null,null,null,"H_Mg_zk",0.4,1,1,1,2,1,null,null,null,20,17,25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.6,1,1,null,null,null,null,null,null,25,21,30]
[null,null,null,null,null,null,null,"P_Mg_zm",1,2,1,null,null,null,null,null,null,35,33,37]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,1,1,1,2,1,null,null,null,4.75,4.5,7]
[null,null,null,null,null,null,null,"H_Vbv_v",0.95,1,1,0.6,5,1,1,2,1,10.5,10,11]
[25,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Volkerakdam, tot onbekende diepte verstoord,antropogeen"]
[null,null,null,null,null,null,null,"H_Mp_ko",0.15,1,1,0.5,4,2,null,null,null,6.5,6,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.85,1,2,0.9,1,1,null,null,null,17,15,19]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,1,1,1,1,null,null,null,0.75,0.25,2.75]
[null,null,null,null,null,null,null,"H_Mp_ko",0.9,1,1,0.2,4,2,1,1,1,6,5.5,7.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat, met name beneden de 25 m -NAP enkele kleilagen dunner dan 1.5 m"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,1,2,1,2,1,null,null,null,2,1.5,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veen nooit dikker dan 1m"]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.25,2,2,1,1,1,null,null,null,20,13,28]
[26,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,2,2,1,1,1,null,null,null,30,27,33]
[26,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.25]
[]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,1,1,1,5,1,null,null,null,27,25,28]
[null,null,null,null,null,null,null,"H_Vbv_v",0.2,1,2,1,5,1,null,null,null,15.25,15,15.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incl. Hollandveen veentjes tot 50cm"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,4,1,3,1,null,null,null,23,20,26]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,2,1.75,2.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"met mogelijk 0.4 m zand aan top"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"H_Mp_k",1,2,1,null,null,null,null,null,null,4,3,5.5]
[26,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,null,null,null,null,null,null,31.5,30,33]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,1,1,1,2,1,null,null,null,2,1.25,3.25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,1,2,1,null,null,null,29,28,30]
[null,null,null,null,null,null,null,"H_Mg_zk",0.35,1,1,null,null,null,null,null,null,20,18,23]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.35,1,3,1,1,1,null,null,null,3.5,2,4.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,1,1,1,null,null,null,3,0.75,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,2,0.4,1,2,null,null,null,2.25,1,3]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,0.4,5,2,null,null,null,16,14,20]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,2,0.9,1,1,null,null,null,1.75,0.5,2]
[null,null,null,null,null,null,null,"H_Mr_kz",0.2,2,1,1,2,1,null,null,null,25,23,27]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,2,1,1,3,1,null,null,null,34,30,37]
[null,null,null,null,null,null,null,"H_Aa_ht",1,1,1,0.5,1,1,null,null,null,3,2.5,3.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,2,2,1,4,1,null,null,null,9,8,10]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,2,0.3,1,1,null,null,null,1,0.25,2]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,2,1,5,2,null,null,null,27,25,29]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,1,1,1,null,null,null,1.25,1,1.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,2,0.9,1,2,null,null,null,3,2.75,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.8,5,1,null,null,null,16.5,15.75,17.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. 40 cm basisveen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,-0.25,-1,0.25]
[26,17,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,2,0.3,3,2,null,null,null,5.5,5,7]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,2,1,1,2,null,null,null,1.5,1,2]
[null,null,null,null,null,null,null,"H_Mr_kz",0.05,1,2,1,3,2,null,null,null,5,4,7]
[26,19,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.4,1,1,null,null,null,1.5,0.75,2.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,0.6,5,1,null,null,null,15,13.5,16.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. 40 cm basisveen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,1,1,1,1,null,null,null,0.25,0,0.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,1,2,1,2,1,null,null,null,2.5,1.75,3]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,0.2,5,2,null,null,null,15.5,14.5,16.5]
[26,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oosterscheldekering. Tot onbekende diepte verstoord"]
[null,null,null,null,null,null,null,"H_Mg_zm",0.1,1,2,0.5,2,2,null,null,null,13,12,15]
[null,null,null,null,null,null,null,"P_Rg_zm",0.25,2,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,5.5,3.75,6.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.2,4,3,1,2,1,null,null,null,11.5,11,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"aan basis meestal basisveen, meestal 20 cm, max. 50 cm dik"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,1,null,null,null,null,null,null,2,1.5,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,1,2,null,null,null,null,null,null,3.25,2.5,4]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,4,2,1,1,1,null,null,null,6.75,4,8]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,4,4,null,null,null,null,null,null,13,12,15]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,3.75,2,5.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.15,4,3,1,1,1,null,null,null,10,8.25,11.5]
[null,null,null,null,null,null,null,"H_Mg_zk",2.5000000000000001E-2,4,5,1,1,1,null,null,null,10,8.25,11.5]
[]
[null,null,null,null,null," ",null,"H_Vhv_v",0.5,1,2,1,2,1,null,null,null,3.5,2,5]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,3,1,3,1,null,null,null,7.75,6,10]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,1,4,1,3,1,null,null,null,4.5,3.75,5.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.05,1,5,1,2,1,null,null,null,3,2,5]
[27,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1.25]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,2,0.3,3,2,null,null,null,9,7.25,10.5]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,2,1,5,2,null,null,null,23,19,25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,1,1,1,2,1,null,null,null,8.5,7,11]
[null,null,null,null,null,null,null,"H_Vhv_v",0.95,1,2,1,2,1,null,null,null,4.75,2.25,6.25]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,3,1,null,null,null,null,null,null,5,4.5,5.5]
[27,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,2,0.3,1,2,null,null,null,3.25,2.5,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.95,5,1,null,null,null,11.75,10,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. 25 cm basisveen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,1,1,1,1,null,null,null,-0.5,-1.25,0.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.18,1,2,1,2,1,null,null,null,3.25,3,3.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.01,1,3,1,1,1,null,null,null,-0.5,-1.25,0.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_ko",0.6,3,2,1,3,1,null,null,null,5,4.25,5.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,3,2,0.3,4,1,null,null,null,5.25,5,5.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.4,3,3,1,5,1,null,null,null,11.75,10.75,12.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,1,1,3,2,null,null,null,24,22.5,30]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,2,1,2,1,null,null,null,3,2.25,4.5]
[27,20,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.85,1,2,0.7,1,2,null,null,null,2.5,2,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,1,2,0.9,6,1,null,null,null,11,10.25,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. ong. 40 cm basisveen"]
[27,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dijk evenwijdig aan geulrand, dus geul soms net wel en net niet aangesneden. Boringen in geul hebben geen Hollandveen, buiten geul wel."]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,0.8,1,2,null,null,null,3,2.25,4]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,1,2,0.9,5,2,null,null,null,20,18,25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,null,null,null,null,null,null,0.5,-1,0.75]
[27,23,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dijk evenwijdig aan geulrand, dus geul soms net wel en net niet aangesneden. Boringen in geul hebben geen Hollandveen, buiten geul wel."]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,1,2,1,2,2,null,null,null,3.25,2,4]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,1,2,1,3,1,null,null,null,5.25,3.5,7]
[27,24,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.6,1,1,null,null,null,2.5,1.25,3.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,0.6,5,1,null,null,null,12.5,10,14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. ong. 40 cm basisveen"]
[27,25,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,1,2,1,1,1,null,null,null,0.5,0,5]
[27,27,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Philipsdam. Bodemopbouw kan tot grote diepte verstoord zijn."]
[27,28,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oesterdam. Bodemopbouw kan tot grote diepte verstoord zijn"]
[null,null,null,null,null,null,null,"H_Mp_ko",0.85,3,2,1,2,1,null,null,null,7.5,6.5,9]
[27,29,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oesterdam. Bodemopbouw kan tot grote diepte verstoord zijn"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre Formatie, bevat dunne kleilagen"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.95,1,1,0.2,1,1,1,3,1,5.5,5,6]
[null,null,null,null,null,null,null,"H_Aa_ht",0.95,1,1,0.8,1,2,1,1,1,3.5,2.5,5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,15,10,21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelmatig dunne (1-2 dm) leemlaag net onder de top"]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,1,0.2,1,1,1,2,1,3.5,3,4.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,1,0.1,3,2,null,null,null,8,7,13]
[]
[null,null,null,null,null,null,null,"H_Aa_ht",0.95,1,1,0.8,1,2,1,1,1,2.5,2,5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,1,1,0.75,3,3,1,2,1,15,12,17]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,1,1,1,5,1,null,null,null,25,18,28]
[null,null,null,null,null,null,null,"H_Mr_kz",0.15,1,4,1,2,1,null,null,null,17,15,23]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,1,0,3]
[28,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,2,3,0.2,3,1,null,null,null,10.25,3.5,13]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,0.5,-0.5,1.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,2,2,null,null,null,null,null,null,31,29,34]
[28,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,2,3,1,4,1,null,null,null,32,30,33.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,2,2,null,null,null,null,null,null,31,29,32.5]
[28,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,2,3,1,4,1,null,null,null,23,20,26]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,2,2,null,null,null,null,null,null,23,20,26]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,1,null,null,null,null,null,null,-0.5,-1,0.25]
[28,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,1,1,1,null,null,null,2.25,1.5,2.75]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,0.95,5,1,null,null,null,9.25,9,9.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. 25 cm basisveen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,2,null,null,null,null,null,null,3.5,2.5,5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,1,1,1,null,null,null,0.75,-0.5,2.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.4,1,1,1,2,1,null,null,null,9.5,8,12.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,1,2,1,2,1,null,null,null,2.5,1.75,3.75]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleiige lagen of lenzen bevatten"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,2,1,1,2,null,null,null,0.25,-0.25,0.75]
[28,13,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,2,1,4,1,null,null,null,10,9.5,10.5]
[28,14,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,1,2,0.4,3,1,null,null,null,3.25,2.5,4]
[28,15,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandkreekdam, lokaal grond verstoord door aanleg dam. Waterdiepte zal rond 5 m -NAP zijn"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.8,1,1,null,null,null,4,2,8]
[28,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veerse Gatdam"]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,2,3,1,2,1,null,null,null,23,14,28]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,1,1,1,3,1,null,null,null,6.5,3.25,8.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. ong. 25 cm basisveen"]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.2,4,2,null,null,null,5.5,5,7]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,1,1,1,null,null,null,2.75,2.25,3]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,1,2,0.1,5,2,null,null,null,7.5,7,8]
[29,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Mg_zk",1,1,2,1,4,1,null,null,null,4.5,4.25,4.75]
[]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,2,1,null,null,null,null,null,null,2,0.5,3.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.7,3,2,1,3,1,null,null,null,3.5,2,5.25]
[null,null,null,null,null,null,null,"P_Rg_zf",1,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,3,1,1,1,1,null,null,null,2.5,1.5,5]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,3,1,1,2,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"P_Rg_zf",1,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.25,3,1,1,3,1,null,null,null,23,20,27]
[null,null,null,null,null,null,null,"H_Mg_zm",0.4,3,3,1,3,1,null,null,null,23,20,27]
[null,null,null,null,null,null,null,"H_Ova_zf",1,1,1,null,null,null,null,null,null,0.25,-0.25,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Duinzand kan ontbreken en is dikker waar maaiveld hoger ligt"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,1,null,null,null,null,null,null,3.25,3,3.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,5,2,null,null,null,null,null,null,20,18,22]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,1,2,1,2,1,null,null,null,1,-1.5,2.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zm",1,3,1,null,null,null,null,null,null,22,17,26]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,1,1,1,1,null,null,null,1.5,1.25,1.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,2,1,2,1,null,null,null,3.5,2,4.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,0.2,3,1,null,null,null,3.75,3.25,4]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,27,25,29]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,2,2,null,null,null,null,null,null,27,25,31]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,1,1,null,null,null,null,null,null,0.5,-1.5,1.25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,3,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.5,3,1,null,null,null,null,null,null,3.5,3,4]
[30,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[30,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,2,1,2,1,null,null,null,3,2.75,4.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.95,1,2,1,2,1,null,null,null,3,2,4.25]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,1,2,1,2,1,null,null,null,16,14,17]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.85,1,3,0.4,1,1,null,null,null,2,1,2.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.85,1,3,0.8,4,2,null,null,null,12,9,16]
[30,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.75,1,2,1,3,1,null,null,null,5,3.5,8.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.01,1,2,1,2,1,null,null,null,3.25,2.75,3.5]
[]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.2,1,2,null,null,null,2.25,0.75,3.75]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mr_kz",0.3,1,2,1,1,1,null,null,null,1.75,-1,5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,null,null,null,null,null,null,2.75,2,3.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.6,4,2,1,3,1,null,null,null,6.75,6,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"aan basis meestal basisveen, meestal 20 cm, max. 50 cm dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,2,3,1,2,1,null,null,null,22,20,24]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,2,0.8,1,1,null,null,null,2,1,2.5]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,20,18,22]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,2,1,1,1,null,null,null,-0.25,-0.5,0.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,2,0.4,1,1,null,null,null,1.25,1,1.75]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,27,25,29]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,1,1,1,3,2,null,null,null,23,18,27]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleiige lagen of lenzen bevatten"]
[null,null,null,null,null,null,null,"H_Mr_kz",0.2,1,2,1,2,1,null,null,null,3.5,2.75,4.5]
[30,20,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,2,0.3,1,2,null,null,null,2.75,2.5,3]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.9,5,1,null,null,null,10,8.75,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis max. 25 cm basisveen"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,1,2,0.1,5,2,null,null,null,17,15,22]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.1,1,1,1,1,1,null,null,null,0.5,-0.5,1.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,0.7,3,1,null,null,null,3.75,3.5,4.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,2,0.7,1,1,1,1,1,0,-0.5,2]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,2,0.3,3,1,null,null,null,3.5,2.75,4.25]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleiige lagen of lenzen bevatten"]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,32,28,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleiige lagen of lenzen bevatten"]
[null,null,null,null,null,null,null,"H_Vhv_v",0.05,1,1,1,2,1,null,null,null,3,2.25,3.5]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.95,1,2,0.1,2,1,1,2,1,10,8,12]
[31,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.7,1,1,null,null,null,2,1,2]
[null,null,null,null,null,null,null,"H_Mg_zk",0.9,1,2,0.6,5,2,null,null,null,14,12,20]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.4,1,1,null,null,null,1.75,0.75,2.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,2,0.6,1,2,null,null,null,2.5,1.5,3.5]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,27,18,30]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,1,2,1,1,1,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,1,4,1,2,1,null,null,null,3.5,2.75,4.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,4,1,5,1,null,null,null,13.5,8,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis evt. dun (25 cm) basisveen tussen 8 en 10 m-NAP"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,3,null,null,null,null,null,null,3.25,2.5,4.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,4,5,1,4,1,null,null,null,13,11,17]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,2,null,null,null,null,null,null,-1,-2.25,0]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,4,4,1,1,1,null,null,null,6.25,4.5,8.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,1,2,1,2,1,null,null,null,3.25,3,3.75]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,22,20,24]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,1,1,1,3,1,null,null,null,17,15,19]
[null,null,null,null,null,null,null,"H_Mg_zk",0.95,1,2,1,4,1,null,null,null,7.75,7.25,8]
[31,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,2,1,2,1,null,null,null,3.25,2.5,3.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,1,0.9,3,2,null,null,null,15,12,18]
[null,null,null,null,null,null,null,"H_Mp_k",0.9,1,2,1,4,1,null,null,null,4,2.5,5.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,1,1,0.5,3,1,null,null,null,7.25,7,7.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,0.6,3,2,null,null,null,6.75,4.5,7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis soms max. 25 cm basisveen. Waar top Pleistoceen hoog ligt wordt H_Mp_k dun of verdwijnt, waardoor basisveen 1  veenlaag vormt met bovenliggend Hollandveen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.4,1,1,null,null,null,null,null,null,3.5,2.5,6]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,19,14,24]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,36.5,35.5,37.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.6,1,1,null,null,null,null,null,null,3.5,2.5,4.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,5,1,null,null,null,null,null,null,35,33,37]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,2,2,1,2,1,null,null,null,15,10,20]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,2,null,null,null,null,null,null,3.25,1.75,5.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,1,1,1,null,null,null,-0.75,-1,-0.5]
[null,null,null,null,null,null,null,"H_Mp_ko",0.3,1,2,1,3,1,null,null,null,6.75,6,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan dun basisveen bevatten (0.25 cm)"]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.05,1,3,1,6,2,null,null,null,9.5,8.25,10.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan basisveen en gyttja bevatten"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mr_kz",0.1,1,2,1,2,1,null,null,null,3.5,2.75,4.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,-1,-1.5,-0.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.05,2,4,1,2,1,null,null,null,2.5,2,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,1.75,0,2.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,2,1,null,null,null,null,null,null,12,9.5,15]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mg_zk",0.4,2,3,1,2,1,null,null,null,30,21,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kan onderin ook Oosterhout-zand bevatten"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,1,1,2,1,null,null,null,5,4,8.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.25,1,2,1,5,1,null,null,null,6.75,6.25,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"aan basis mogelijk dun basisveen"]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.3,1,4,1,1,1,null,null,null,0,-0.5,1.5]
[null,null,null,null,null,null,null,"H_Mp_k",0.3,1,4,1,6,1,null,null,null,5.75,4.75,6.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"aan basis mogelijk dun basisveen"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.6,2,2,1,1,1,null,null,null,24.5,22.5,26]
[32,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mp_k",0.1,3,2,null,null,null,null,null,null,6.5,6,7.5]
[32,8,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,28,26,30]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,3,null,null,null,null,null,null,2.75,2.25,3.5]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,2,3,1,2,1,null,null,null,21,20,22]
[null,null,null,null,null,null,null,"H_Mp_k",0.4,1,1,null,null,null,null,null,null,1.25,0.5,2.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,5,2,1,1,1,null,null,null,7.5,5.75,11]
[32,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5]
[null,null,null,null,null,null,null,"H_Mp_k",1,3,1,null,null,null,null,null,null,4,2.75,4.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,5,2,null,null,null,null,null,null,6.5,4.5,8.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,1.75,1.25,3]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,0.5,-1.5,1.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,2,1,null,null,null,null,null,null,3.25,1.75,4.75]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,25,20,30]
[null,null,null,null,null,null,null,"H_Mg_zk",1,2,1,null,null,null,null,null,null,33,30,36]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,4,1,1,2,1,null,null,null,22,20,24]
[32,18,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.6,2,2,1,1,1,null,null,null,24,19,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dit scenario komt voor in noordwestelijke helft van segment"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,2,1,2,1,null,null,null,7,4,9]
[32,20,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"H_Mg_zk",1,3,1,null,null,null,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,1,2,1,2,1,null,null,null,9.5,7,11.75]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,4,2,1,1,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dit komt alleen voor in landwaartse bocht van dijk"]
[null,null,null,null,null,null,null,"H_Mr_kz",0.2,1,2,1,3,1,null,null,null,16.5,15.5,17.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan vrij zandig zijn en ook zandige lagen bevatten"]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,3,1,1,2,1,null,null,null,5,4,6]
[null,null,null,null,null,null,null,"H_Mr_kz",0.3,3,1,1,3,1,null,null,null,8,7,9]
[32,24,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5]
[null,null,null,null,null,null,null,"H_Mg_zk",1,5,1,null,null,null,null,null,null,28,26,30]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.7,3,1,1,1,1,null,null,null,0,-0.75,2]
[null,null,null,null,null,null,null,"P_Ova_sd",1,7,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.15,1,5,null,null,null,null,null,null,-0.75,-1.25,-0.5]
[null,null,null,null,null,null,null,"H_Mg_zk",0.25,1,1,1,2,1,null,null,null,4,2.5,6]
[null,null,null,null,null,null,null,"H_Mp_ko",0.3,1,2,1,3,1,null,null,null,9,8.25,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wordt dunner in oostelijke richting, mogelijk afwezig in uiterste oosten van segment"]
[null,null,null,null,null,null,null,"H_Mp_ko",0.15,1,3,1,5,1,null,null,null,12.25,10.5,14]
[null,null,null,null,null,null,null,"H_Mg_zk",0.3,1,5,1,4,1,null,null,null,18,16,20]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.45,1,2,0.2,1,1,null,null,null,4.5,2.75,6]
[null,null,null,null,null,null,null,"H_Mg_zk",0.45,1,2,1,4,1,null,null,null,9.5,8.5,10.25]
[null,null,null,null,null,null,null,"H_Vhv_v",0.2,1,3,1,2,1,null,null,null,6,5,8.25]
[null,null,null,null,null,null,null,"H_Mp_k",0.2,1,3,0.7,3,1,null,null,null,8.75,7.75,9.75]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.25,1,5,0.2,1,1,null,null,null,4.5,2.75,6]
[null,null,null,null,null,null,null,"H_Mg_zk",0.25,1,5,1,5,1,null,null,null,13,12,15]
[null,null,null,null,null,null,null,"H_Mp_zf",0.1,1,2,0.1,1,1,null,null,null,3.25,1.5,5.25]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.6,1,3,0.9,1,2,null,null,null,3.25,1.5,5.25]
[null,null,null,null,null,null,null,"H_Mp_zf",0.2,1,4,0.1,1,1,null,null,null,3.25,1.5,5.25]
[null,null,null,null,null,null,null,"H_Vhv_v",0.05,1,5,1,2,1,null,null,null,5.5,3.5,7]
[33,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2.75]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,2,1,2,1,null,null,null,9.5,8.5,12]
[null,null,null,null,null,null,null,"H_Vhv_v",0.1,1,3,1,2,1,null,null,null,5.25,4.5,5.5]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,5,3,6]
[null,null,null,null,null,null,null,"P_Rg_zf",1,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan lemige lagen of lenzen bevatten"]
[]
[null,null,null,null,null,null,null,"H_Mg_zk",0.7,1,2,1,2,1,null,null,null,7,6,10]
[null,null,null,null,null,null,null,"H_Mp_k",0.05,1,3,1,3,1,null,null,null,5.25,4,6]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.05,1,1,1,1,1,null,null,null,2.75,2,3.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,1,2,1,2,1,null,null,null,5.25,4,7]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.8,1,2,0.1,5,3,1,2,1,12,9,14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan basis van Schelde geulen gyttja."]
[]
[null,null,null,null,null,null,null,"H_Mp_k",0.2,3,1,null,null,null,null,null,null,4.5,3,5]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,5,3,1,2,1,null,null,null,23,16,27]
[null,null,null,null,null,null,null,"H_Mg_zk",0.1,1,1,1,2,1,null,null,null,15,11,20]
[null,null,null,null,null,null,null,"H_Mg_zk",0.8,1,2,0.7,5,2,null,null,null,9.5,8.5,10.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan lemige lagen of lenzen bevatten"]
[null,null,null,null,null,null,null,"H_Mg_zk",0.2,2,2,1,1,1,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Mr_kz",0.2,2,2,1,2,1,null,null,null,8.5,7.5,9.5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.65,1,1,0.2,1,1,null,null,null,2.5,1.75,4.25]
[null,null,null,null,null,null,null,"H_Mg_zk",0.65,1,1,1,4,1,null,null,null,5.5,4.5,6.25]
[null,null,null,null,null,null,null,"H_Mp_zf",0.35,1,2,0.8,1,2,1,2,1,2.5,2,2.75]
[34,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"H_Mg_zk",0.45,1,2,1,4,1,null,null,null,14,13,21]
[null,null,null,null,null,null,null,"H_Mg_zk",0.05,1,3,1,5,1,null,null,null,6.5,6,7]
[34,10,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75]
[null,null,null,null,null,null,null,"H_Mg_zk",0.5,4,1,null,null,null,null,null,null,11,9,12]
[]
[null,null,null,null,null,null,null,"H_Mp_k",0.95,1,2,1,3,1,null,null,null,7,5.5,7.75]
[null,null,null,null,null,null,null,"P_Rg_zf",0.95,1,2,0.4,6,2,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan lemige lagen of lenzen bevatten"]
[34,12,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Buitendijks gebied is opgehoogd."]
[null,null,null,null,null,null,null,"H_Mkw_z&k",1,1,1,null,null,null,null,null,null,2.5,1.5,4]
[34,13,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In westelijk deel van het segment is buitendijks gebied opgehoogd."]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.95,1,1,0.2,1,4,1,1,1,0.25,0,0.75]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,7,6.5,9.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fijn zandig pakket kan afwezig zijn door holocene erosie."]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.9,1,1,1,1,1,null,null,null,0.5,-0.5,1]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,2,1,1,2,1,null,null,null,3.5,2.25,4.75]
[34,16,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In zuidelijk deel van segment loopt maaiveld op tot 3-4 m."]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.2,1,2,1,1,1,null,null,null,-1,-1.25,-0.5]
[34.1,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In midden van dit segment is opgebrachte grond (ong. 2 m)."]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,5,3,5.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,1,0.5,2,1,1,1,1,1,0.5,2]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,5,3.5,6.5]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,1,1,null,null,null,null,null,null,0,-0.5,2]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,3,2,null,null,null,null,null,null,24,23,25]
[35,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,2,1,2,1,null,null,null,11,10,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dunne laag klei,veen, maximaal 1 m dik"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.45,1,2,1,2,1,null,null,null,1.75,1,2]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,2,1,2,1,null,null,null,11,10,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dunne laag klei,veen, maximaal 1 m dik"]
[]
[null,null,null,null,null,null,null,"P_Rg_zf",0.7,2,2,null,null,null,null,null,null,4,3,6]
[]
[null,null,null,null,null,null,null,"H_Mp_zf",0.95,1,1,0.1,1,4,null,null,null,1.5,1.25,1.75]
[null,null,null,null,null,null,null,"H_Vhv_v",0.95,1,1,1,2,1,null,null,null,1.75,1.5,2.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,2,1,null,null,null,null,null,null,2.25,1.5,2.75]
[35,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Merendeels opgehoogd, schatting zonder ophoging"]
[null,null,null,null,null,null,null,"H_Mp_zf",0.8,1,1,0.3,1,2,0.6,1,2,3,2.75,4]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k",0.8,1,1,0.1,1,2,1,1,1,0.25,-0.75,1.25]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,31,28,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan lokaal kleiige geulopvulling bevatten."]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,1,1,0.9,1,1,1,3,1,2.5,1,3.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,1,2,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Aa_ht",0.1,1,1,null,null,null,null,null,null,12,10,15]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,2,1,2,1,null,null,null,6,5,7]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.45,1,3,1,1,1,null,null,null,-1,-1.5,-0.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,1,1,1,1,null,null,null,-0.5,-1,0]
[null,null,null,null,null,null,null,"H_Rg_zm",0.85,1,3,1,2,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,1,1,2,1,null,null,null,-1.25,-1.5,-1]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,1,2,1,2,1,null,null,null,0.75,0.5,1]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,2,1,1,3,1,null,null,null,25,20,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan lokaal kleiige geulopvulling bevatten"]
[null,null,null,null,null,null,null,"H_Rg_zg",0.2,1,1,1,2,1,null,null,null,3.5,2.75,4]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,3,1,1,1,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,2,1,1,3,1,null,null,null,25,20,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan lokaal kleiige geulopvulling bevatten"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,1,1,1,1,null,null,null,-2.25,-2.5,-1]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.1,1,2,1,3,1,null,null,null,1.25,1,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inclusief basisveen"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,2,1,1,3,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre zand"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,1,0.8,1,2,null,null,null,-1,-2.5,0]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre zand"]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,0.3,1,3,null,null,null,-1,-2.5,0]
[null,null,null,null,null,null,null,"P_Rg_zm",0.3,3,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre zand; bevat dunne (dunner dan 3m) kleilagen rond -35m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,0.7,1,1,null,null,null,-4,-5,-3]
[null,null,null,null,null,null,null,"H_Rg_zg",0.3,2,2,1,1,1,null,null,null,-1,-1.5,-0.75]
[36,11,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-7.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grens met segment 36-12 gelegd o.b.v. breuk"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,3,null,null,null,null,null,null,-3,-4,-2.5]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,1,2,1,2,1,null,null,null,-5,-6,-4]
[null,null,null,null,null,null,null,"H_Rg_zg",0.2,2,2,1,3,1,null,null,null,3,2,4]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.35,1,2,1,2,1,null,null,null,-7,-8,-5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,4,1,1,2,1,null,null,null,22,20,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre- en Kiezelooliet-zand; kan kleilagen tot 3m dik bevatten"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,null,null,null,null,null,null,22,20,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre- en Kiezelooliet-zand; kan kleilagen tot 3m dik bevatten"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,1,1,1,2,1,null,null,null,-3,-4,-2.5]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oosterhout- en onderin Breda-zand; kan (deels) opgebouwd zijn uit klei,leem en schelpenlagen. "]
[37,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2.75]
[null,null,null,null,null,null,null,"H_Rg_zm",1,2,1,0.7,2,1,null,null,null,4.5,3.75,6]
[null,null,null,null,null,null,null,"H_Rk_k",0.9,1,2,null,null,null,null,null,null,-2,-2.25,-1.75]
[null,null,null,null,null,null,null,"H_Rg_zm",0.9,2,4,0.7,2,1,null,null,null,4.5,4.25,4.75]
[null,null,null,null,null,null,null,"H_Rk_k",0.9,1,2,null,null,null,null,null,null,-2,-2.5,-1.75]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,4,0.3,2,1,null,null,null,4.25,4,4.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-0.75,-1,-0.25]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.3,3,2,1,2,1,null,null,null,8,7,8.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-1.75,-2.25,-0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top kan kleiig zijn."]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,3,1,0.3,2,2,null,null,null,8,7,9]
[null,null,null,null,null,null,null,"H_Rk_ko",0.4,3,2,1,1,1,null,null,null,5,3.75,6.75]
[]
[null,null,null,null,null,null,null,"H_Rk_vk",0.4,3,1,1,2,1,null,null,null,6,4.5,8]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.4,3,1,1,2,1,null,null,null,1.25,0.5,3.25]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,3,3,1,1,1,null,null,null,1,0,3]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,1,null,null,null,null,null,null,-3.5,-3.75,-3.25]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,3,1,0.1,4,3,1,1,1,2.5,2,3]
[null,null,null,null,null,null,null,"P_Rg_zg",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top van het Pleistoceen kan Wijchen-klei voorkomen."]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,3,1,0.3,1,1,1,1,1,-1.5,-2,0]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,3,3,1,1,1,null,null,null,-0.25,-1.25,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan ook grofzandig, fijn grindig zijn."]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,3,1,0.8,1,1,1,2,1,1.5,1,2.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,3,1,0.2,1,2,null,null,null,1.75,1.5,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan dunne veenlaagjes bevatten (max. 50 cm.)."]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,2,3,1,1,1,null,null,null,1.5,0.5,2.5]
[]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.2,2,1,1,2,1,null,null,null,7,6.5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top kan veen voorkomen."]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.3,2,3,1,4,1,null,null,null,7,6.5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top kan veen voorkomen."]
[38,10,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-4.75]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,2,3,1,2,1,null,null,null,-1,-2.5,0]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,3,1,1,1,null,null,null,-2.75,-3.25,-2.25]
[]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.5,2,2,1,2,1,null,null,null,2.5,1.75,3]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,4,1,2,1,null,null,null,2,1,3]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,5,null,null,null,null,null,null,3,1,6]
[null,null,null,null,null,null,null,"H_Rk_k",0.5,1,2,null,null,null,null,null,null,-4.75,-5,-4.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.1,2,3,1,4,1,null,null,null,2,1.5,3]
[41,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-5.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.05,2,1,0.8,2,2,1,2,1,30,25,35]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.8,2,2,0.5,2,2,1,2,1,0,-1,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,2,2,0.8,4,2,1,2,1,30,25,35]
[null,null,null,null,null,null,null,"P_Rg_zg",0.15,2,3,0.8,3,2,1,1,1,18,15,22]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,2,1,1,1,1,null,null,null,2,1,4]
[null,null,null,null,null,null,null,"H_Rk_k",0.35,2,2,1,1,1,null,null,null,-2.25,-3,-1]
[null,null,null,null,null,null,null,"P_Rg_zg",0.35,2,2,0.2,3,2,null,null,null,1.25,0.5,4]
[null,null,null,null,null,null,null,"H_Rk_k",0.15,2,3,1,1,1,null,null,null,-2,-3,-1]
[null,null,null,null,null,null,null,"H_Rg_zm",0.15,2,3,1,2,1,null,null,null,2,1,4]
[null,null,null,null,null,null,null,"P_Rg_zm",0.15,2,3,0.8,3,2,1,3,1,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k",0.1,2,2,0.8,1,1,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.3,2,1,0.5,1,1,null,null,null,-1.25,-1.75,-0.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.45,2,2,1,3,1,null,null,null,3,0,5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,3,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,2,2,null,null,null,null,null,null,2,-2,4]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.05,2,4,1,1,1,null,null,null,-2,-3,1]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.65,2,2,0.75,2,1,null,null,null,0,-2,4]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.2,2,3,1,3,1,null,null,null,-2.5,-3,0]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,2,0.5,2,1,null,null,null,0,-2,3]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,2,0.5,2,2,1,1,1,-5,-5.5,-4]
[]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,2,2,0.5,2,1,null,null,null,-4,-5.5,-2.5]
[41,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-8.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.2,2,2,0.5,2,2,null,null,null,-4.5,-5.5,-3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,3,2,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,1,1,2,1,null,null,null,0,-2,2]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,3,2,1,1,1,null,null,null,8,6,15]
[null,null,null,null,null,null,null,"H_Rg_zg",0.8,2,1,null,null,null,null,null,null,-1,-3,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.25,3,2,null,null,null,null,null,null,1,0,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan uit keileem bestaan"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.25,3,1,1,1,1,null,null,null,1,0,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan uit keileem bestaan"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,4,2,1,2,1,null,null,null,22,20,28]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,2,1,null,null,null,null,null,null,0,-0.5,1]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,2,4,1,1,1,null,null,null,-1,-2,1]
[]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.4,2,1,1,2,1,null,null,null,-0.5,-1,0]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.4,2,3,1,4,1,null,null,null,0.5,-0.5,3]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-4,-5,-3]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.35,2,2,1,2,1,null,null,null,0,-1,2]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.8,1,1,1,2,1,null,null,null,-3,-4,-1]
[null,null,null,null,null,null,null,"P_Rg_zm",0.75,3,2,null,null,null,null,null,null,14,13,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan verspreid dunne kleilagen bevatten"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.75,1,1,null,null,null,null,null,null,-7.5,-8.5,-6.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.65,2,2,1,2,1,null,null,null,-3,-5,0]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,10,6,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye en Beegden-zand, soms met dunne kleilaag aan de top"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,null,null,null,null,null,null,-6.5,-7,-4]
[null,null,null,null,null,null,null,"H_Rg_zm",0.7,2,2,1,2,1,null,null,null,-0.5,-3,2]
[]
[null,null,null,null,null,null,null,"H_Rk_k",0.15,2,2,0.3,2,2,null,null,null,-4,-5,-2]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,1,1,2,1,null,null,null,25,21,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre- en Kiezelooliet-zand; kan kleilagen bevatten"]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-6,-6.25,-5]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.5,2,3,0.5,1,2,null,null,null,-1,-2,2]
[41,21,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-6]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,2,1,1,2,1,null,null,null,-2,-3,0]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,1,1,1,null,null,null,17,13,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Meestal niet dikker dan enkele meters"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,2,1,0.5,1,1,null,null,null,-3,-4.5,-2]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.4,2,2,1,2,1,null,null,null,-1.25,-2,0.25]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,3,null,null,null,null,null,null,-1.5,-2.75,0]
[]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.9,3,1,1,1,1,null,null,null,-2.25,-2.75,-1.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Regelmatig dunne veenlaag (enkele decimeters) aan de top"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre kan kleilagen bevatten. "]
[null,null,null,null,null,null,null,"H_Rk_k",0.2,1,3,1,1,1,1,1,1,-8,-8.5,-7]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k",0.45,1,1,null,null,null,null,null,null,-8.5,-9.5,-7]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,4,1,null,null,null,null,null,null,28,25,35]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",1,2,1,null,null,null,null,null,null,-2,-5,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,5,1,1,1,1,null,null,null,26,23,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre klei, niet dikker dan 8 m"]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,2,null,null,null,null,null,null,-8,-9.5,-7.5]
[]
[42,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-10.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld loopt op van zuid naar noord tot plaatselijk 12 m NAP"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,3,1,null,null,null,null,null,null,8,-1,15]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.97,1,1,null,null,null,null,null,null,-10,-11,-8.75]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Twello,Waalre"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.9,1,1,null,null,null,null,null,null,1,0.5,2]
[null,null,null,null,null,null,null,"H_Vbv_v",0.9,2,1,1,4,1,null,null,null,9,7.5,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hoogteligging varieert, dikte is ca. 0,5 m "]
[null,null,null,null,null,null,null,"H_Vbv_v",0.05,2,3,1,3,1,null,null,null,9,7.5,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hoogteligging varieert, dikte is ca. 0,5 m "]
[43,2,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Doorbraak gevuld met grof zand in de eerste 200 m van het segment"]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.7,2,1,1,4,1,null,null,null,9,8,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hoogteligging varieert, dikte is ca. 0,5 m "]
[null,null,null,null,null,null,null,"H_Vbv_v",0.15,2,3,1,3,1,null,null,null,9,7.5,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hoogteligging varieert, dikte is ca. 0,5 m "]
[43,3,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-1.25]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.1,1,1,1,6,1,null,null,null,7.5,7,8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hoogteligging varieert, dikte is ca. 0,5 m "]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,3,1,1,1,null,null,null,1,0,2]
[43,4,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld rond de 2.5m bij geul in ondergrond, anders 1,5 meter"]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,1,0.2,1,1,null,null,null,0.5,-1,2]
[null,null,null,null,null,null,null,"H_Rg_zm",0.7,1,1,0.2,2,2,null,null,null,5,4.75,6]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.3,1,2,0.7,2,1,1,3,1,6,5,7.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-1,-1.5,0]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,2,1,0.5,2,2,null,null,null,5,4,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan zandlagen tot 1m bevatten"]
[43,6,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-2.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,2,1,0.4,2,2,null,null,null,5,4,5.5]
[43,7,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-3]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,2,1,1,1,null,null,null,6,4,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan kleilagen dikker dan 2 m bevatten"]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.8,2,2,null,null,null,null,null,null,5,4,7]
[43,10,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-3.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,1,1,1,1,null,null,null,-1,-2,0]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,1,3,1,2,1,null,null,null,5,4,6]
[43,11,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-4]
[null,null,null,null,null,null,null,"H_Rk_k",0.6,2,1,0.5,1,2,1,2,1,2,1.5,2.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,3,1,2,1,null,null,null,5,4.5,6]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.2,1,1,1,2,1,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.8,1,2,0.5,2,1,1,3,1,4,3.5,5]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.5,2,1,null,null,null,null,null,null,1,0.5,2]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.3,2,3,0.3,2,1,1,2,1,1,0.5,2]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,4,2,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,2,1,1,1,null,null,null,0,-1,0.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,2,1,1,1,null,null,null,28,24,31]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.8,2,1,null,null,null,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.15,2,2,1,1,1,null,null,null,-0.5,-1,0]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,4,2,1,1,1,null,null,null,22,18,25]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,2,2,1,1,1,null,null,null,2,1,3]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,3,2,1,1,1,null,null,null,22,18,25]
[]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.6,2,3,1,1,1,null,null,null,2,1,3]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,3,1,1,1,null,null,null,6,5,8]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-4,-4.5,-2.5]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.2,2,2,1,2,1,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.05,3,2,null,null,null,null,null,null,6.5,3,8]
[43,19,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-6]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,3,1,1,1,null,null,null,-1,-1.5,-0.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,2,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,2,null,null,null,null,null,null,1,-1,1.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.1,2,1,1,2,1,null,null,null,-1.5,-2,-1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,1,1,2,1,null,null,null,35,30,37]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,2,1,1,1,1,null,null,null,-3.5,-4.5,-2]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_ko",0.05,2,1,1,2,1,null,null,null,-3,-4,-2]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,4,null,null,null,null,null,null,1,-1,1.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k",0.95,2,1,0.25,1,2,null,null,null,-6.5,-7.5,-5.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,5,4,11]
[43,25,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-8.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-8,-8.25,-7.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,2,3,1,1,1,null,null,null,-3.75,-4.25,-3]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,4,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rk_k&s",0.25,2,1,1,3,1,null,null,null,-4,-4.5,-3.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.25,2,4,1,1,1,null,null,null,-4.75,-5.25,-3.5]
[]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.4,3,2,null,null,null,null,null,null,-5,-5.75,-3.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.75,5,2,null,null,null,null,null,null,8,7,11]
[43,28,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-10]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,2,null,null,null,null,null,null,-2,-3,0]
[43,29,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-10]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,2,null,null,null,null,null,null,0,-2,1]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,4,2,null,null,null,null,null,null,11,9,20]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Waalre, kan verspreid kleilagen bevatten van 1-2 m dik"]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.85,2,1,0.5,2,2,null,null,null,-5.5,-6.25,-4.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms Wijchenachtig aan de basis"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,12,5,17]
[null,null,null,null,null,null,null,"H_Rk_k&v",0.9,2,1,0.2,1,1,null,null,null,-9.5,-10,-8.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,12,10,15]
[null,null,null,null,null,null,null,"H_Rk_k",0.9,1,1,null,null,null,null,null,null,-9,-10,-8]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,2,2,1,1,1,null,null,null,20,18,22]
[null,null,null,null,null,null,null,"H_Rk_k",0.6,2,1,1,1,1,null,null,null,-8,-9,-7]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,2,4,1,1,1,null,null,null,-9,-10,-8]
[null,null,null,null,null,null,null,"P_Rg_zm",0.75,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mogelijks deels gestuwd"]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,1,2,1,1,1,null,null,null,-8.5,-9.5,-6]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,1,2,null,null,null,null,null,null,-9.25,-10,-8.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,2,1,null,null,null,null,null,null,-1,-3,1]
[43,36,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-10.25]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,4,1,1,1,null,null,null,-7.5,-8.5,-7]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,4,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k",0.78,2,2,0.1,1,1,null,null,null,4,3.5,4.5]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,2,1,1,2,1,null,null,null,10,7,11]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,2,2,0.1,2,2,1,2,1,10,7,11]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,2,1,1,1,1,null,null,null,2,1.25,3]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,2,2,0.5,1,2,null,null,null,5.25,4.5,6]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,2,null,null,null,null,null,null,-1.5,-3.5,0]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,4,1,1,1,null,null,null,3,0,5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.25,1,1,1,1,1,null,null,null,-2,-2.75,-0.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.25,1,1,1,2,1,null,null,null,2.5,1,4]
[null,null,null,null,null,null,1,"H_Rg_zm",0.25,1,2,1,2,1,null,null,null,5,4,7]
[null,null,null,null,null,null,null,"H_Rk_ko",0.25,1,4,0.5,2,1,null,null,null,1,-0.25,2]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,2,1,1,1,null,null,null,1,0.5,2]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,1,1,2,1,null,null,null,7,5,8]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,2,2,1,3,1,null,null,null,2,1,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer zelden dikker dan 2 m, in dit scenario zeer zelden afwezig"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.65,2,1,0.5,1,1,null,null,null,1.5,-0.5,2.25]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,2,3,null,null,null,null,null,null,3,2.25,4]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,1,1,1,1,null,null,null,-3.75,-4,-1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,3.25,2.75,4]
[null,null,null,null,null,null,null,"H_Rk_k",0.25,1,4,1,1,1,null,null,null,-0.25,-1,1]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.75,1,1,1,3,1,null,null,null,-0.75,-1.25,1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zelden dikker dan 1 m, in dit scenario zeer zelden geerodeerd"]
[null,null,null,null,null,null,null,"H_Rk_k",0.15,1,4,1,1,1,null,null,null,0,-0.5,0.5]
[]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,2,2,0.5,2,1,null,null,null,2.5,1.75,3.75]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,2,3,1,2,1,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,-4,-4.75,-3.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,10,8,13]
[43,49,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-6]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,2,3,1,1,1,null,null,null,-3,-3.5,-1.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.85,4,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,1,0.65,2,2,1,1,1,-2.5,-4.5,0]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,1,0.65,2,2,1,2,1,1,-0.5,2]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,3,0.2,3,2,null,null,null,1,-0.75,2]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,2,3,1,1,1,null,null,null,0,-1.5,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,1,1,1,null,null,null,13,11,16]
[null,null,null,null,null,null,null,"H_Rk_k",1,1,1,null,null,null,null,null,null,-6,-6.75,-5.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,2,3,1,2,1,null,null,null,0,-2,2]
[null,null,null,null,null,null,null,"P_Rg_zf",0.8,3,2,1,2,1,null,null,null,4.5,4,14]
[null,null,null,null,null,null,null,"H_Rg_zm",0.95,1,1,0.8,2,1,null,null,null,0,-2.5,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat fijn- en grofzand lagen van enige meters dikte"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,2,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,1,1,1,1,null,null,null,-4.5,-5.5,-3]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,3,null,null,null,null,null,null,-3.5,-5,-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat soms zandlagen van1-2 m dikte"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,3,2,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.25,1,1,0.3,2,3,1,1,1,-6.5,-7.5,-4.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Deels gestuwd en daarom deels diagonaal gelegen zand,klei pakketten"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,2,1,1,1,null,null,null,-8.5,-8.75,-7.75]
[null,null,null,null,null,null,null,"H_Rk_k",0.2,1,3,null,null,null,null,null,null,-5,-5.5,-4]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rk_k",0.5,1,2,0.2,1,2,1,1,1,-8.5,-9,-7]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,15,10,25]
[null,null,null,null,null,null,null,"H_Rg_zg",0.95,2,1,0.4,1,1,1,1,1,-7.5,-8,-6.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,7,1,10]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",1,2,1,null,null,null,null,null,null,-3,-4,1.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,1,1,1,1,null,null,null,25,20,32]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-4.5,-5.5,-3.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,2,1,null,null,null,null,null,null,0.5,-1,2.5]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,1,1,1,null,null,null,-3,-4,-2]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,3,1,1,1,1,null,null,null,40,40,40]
[44,3,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,-4.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,2,1,1,1,1,null,null,null,5.5,4,7]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,3,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,1,2,1,2,1,null,null,null,3,2,4]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,1,2,1,2,1,null,null,null,3,2,4]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,2,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,1,1,1,2,1,null,null,null,7.5,6.5,8]
[null,null,null,null,null,null,null,"H_Vhv_v",0.7,1,3,1,2,1,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"H_Rk_ko",0.7,1,3,1,3,1,null,null,null,5.5,4.5,6.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,3,1,1,2,1,null,null,null,29,27,31]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,1,1,1,2,1,null,null,null,4,3,5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.3,3,1,1,1,1,null,null,null,14,12,16]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,1,1,1,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,3,1,1,2,1,null,null,null,20,15,21]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,1,2,1,null,null,null,29,27,31]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,1,2,1,1,1,null,null,null,7.5,7,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kan erg grof zijn"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.3,2,1,1,1,1,null,null,null,14,12,16]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,3,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Rg_zm",0.05,2,2,null,null,null,null,null,null,3.5,2.5,4.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,4,1,1,2,1,null,null,null,26,25,27]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,4,1,1,3,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rbk_zm",0.2,1,1,1,2,1,null,null,null,4.5,2,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer variabel in korrelgrootte"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.1,1,2,null,null,null,null,null,null,1,0,2]
[]
[null,null,null,null,null,null,null,"P_Rbk_zm",0.8,3,1,1,2,1,null,null,null,5,4,6]
[]
[]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,2,1,2,1,null,null,null,5.5,5,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"meest siltig tot fijnzandige klei, soms venig"]
[]
[null,null,null,null,null,null,null,"H_Ml_ko",0.95,1,2,1,2,1,null,null,null,5.5,4,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"meest siltig tot fijnzandige klei, soms venig"]
[]
[null,null,null,null,null,null,null,"H_Vhv_v",0.6,2,2,1,1,1,null,null,null,8.5,7.5,11]
[]
[44,19,null,null,null,null,null,"mv",null,null,null,null,null,null,null,null,null,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"plaatselijk opgehoogd"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,3,1,null,null,null,null,null,null,14,13,15]
[null,null,null,null,null,null,null,"H_Mp_k",1,2,1,null,null,null,null,null,null,2,1.5,2.5]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,4,1,1,1,1,null,null,null,6.5,6,7]
[null,null,null,null,null,null,null,"P_Ova_sd",1,7,1,1,1,1,null,null,null,27,25,29]
[null,null,null,null,null,null,null,"H_Vhv_v",0.8,3,1,1,1,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"H_Mkw_z&k",0.8,4,1,1,2,1,null,null,null,10.5,9.5,11]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,8,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"gestuwd, scheve lagen (tot 45 graden) mert kleilagen, fijn en grof zandlagen"]
[null,null,null,null,null,null,null,"H_Vhv_v",1,3,1,null,null,null,null,null,null,5.5,4,7]
[null,null,null,null,null,null,null,"P_Ova_sd",1,8,1,null,null,null,null,null,null,38,30,40]
[null,null,null,null,null,null,null,"H_Vbv_v",1,3,1,null,null,null,null,null,null,18.5,18,19]
[null,null,null,null,null,null,null,"H_Aa_ht",0.5,1,1,null,null,null,null,null,null,18,16,22]
[null,null,null,null,null,null,null,"H_Mp_k",0.5,1,2,1,4,1,null,null,null,6.25,5.5,8]
[null,null,null,null,null,null,null,"H_Mr_kz",0.5,1,2,1,5,1,null,null,null,11,10,12.75]
[null,null,null,null,null,null,null,"P_Rbk_z&s",1,2,1,null,null,null,null,null,null,19.5,19,20]
[null,null,null,null,null,null,null,"H_Mp_k",0.85,1,2,null,null,null,null,null,null,3.5,2.75,4.5]
[null,null,null,null,null,null,null,"H_Mp_zf",0.25,5,2,1,1,1,null,null,null,12.75,12,13.5]
[null,null,null,null,null,null,null,"P_Mp_k",1,9,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,2,1,1,1,1,1,1,1,12,11,13]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,2,1,1,1,1,1,1,1,2.5,0.5,3.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,20,19,21]
[null,null,null,null,null,null,null,"H_Mp_k",1,1,1,null,null,null,null,null,null,1,0,2.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,5,2,null,null,null,null,null,null,16,14,17]
[45,4,6,6,null,null,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,3,2,null,null,null,null,null,null,10,8,11]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.9,4,1,1,1,1,null,null,null,12,10,14]
[45,5,null,6,null,null,null,"mv",null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,3,2,null,null,null,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,1,1,0.3,3,1,1,1,1,4.5,3.5,5]
[null,null,null,null,null,null,null,"H_Ml_ko",0.2,1,2,1,3,1,null,null,null,10,8,11]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,3,2,null,null,null,null,null,null,14,12,16]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,7.5,5,8]
[null,null,null,null,null,null,null,"P_Rg_zm",0.1,5,2,null,null,null,null,null,null,14,12,16]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,4,3,7.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.9,2,1,1,2,1,null,null,null,3.5,3,5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.5,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Vhv_v",0.9,1,1,1,2,1,null,null,null,3,0.25,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Veendikte maximaal 4 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,4,1,null,null,null,null,null,null,18,16,20]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,1,1,null,null,null,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms keileem beneden 30 m -NAP"]
[null,null,null,null,null,null,null,"P_Wdz_zf",1,2,1,null,null,null,null,null,null,3,2.5,3.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,4,1,null,null,null,null,null,null,18,16,20]
[45,13,null,6,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-0.25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,2,1,1,1,null,null,null,7,6,8]
[null,null,null,null,null,null,null,"P_Mg_zm",0.1,4,2,1,2,1,null,null,null,32,30,34]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.9,1,2,null,null,null,null,null,null,1,0.5,1.5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,14,10,24]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-5,-6,-3]
[null,null,null,null,null,null,null,"H_Rg_zm",0.8,2,1,null,null,null,null,null,null,1,0,2]
[null,null,null,null,null,null,null,"H_Rg_zg",0.1,3,2,1,3,1,null,null,null,15,13,18]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-5,-6,-3]
[]
[null,null,null,null,null,null,null,"H_Rg_zg",0.8,2,2,null,null,null,null,null,null,0,-1,1]
[null,null,null,null,null,null,null,"H_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,24,23,25]
[null,null,null,null,null,null,null,"H_Vhv_v",1,2,1,null,null,null,null,null,null,2.5,1.5,3]
[]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.4,1,2,null,null,null,null,null,null,4,3.5,5]
[null,null,null,null,null,null,null,"P_Gs_zg",0.3,5,2,1,1,1,null,null,null,30,20,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,2,2,null,null,null,null,null,null,6,5,13]
[47,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-13.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer variabele ondergrond, zie bijvoorbeeld sonderingen S40A00180 en S40B00460"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,1,1,1,1,1,null,null,null,-8,-10,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vuil zand en bevat sporadisch dun (dunner dan 0.5m dik) veenlaagje aan de basis"]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,1,2,1,2,1,null,null,null,0,-1,1]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,1,1,1,null,null,null,-7,-8,-3]
[null,null,null,null,null,null,null,"P_Rg_zf",0.1,3,1,1,3,1,null,null,null,35,33,37]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,1,1,1,1,null,null,null,-9.5,-10,-8]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,7,5,10]
[47,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S40B00945"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.1,1,2,1,2,1,null,null,null,-2,-5,3]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,4,1,1,2,1,null,null,null,37,35,40]
[null,null,null,null,null,null,null,"H_Rk_vk",0.3,1,1,1,2,1,null,null,null,-7.5,-8,-6.75]
[null,null,null,null,null,null,null,"H_Rg_zm",0.2,1,3,1,2,1,null,null,null,-2,-4,0]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,7.5,7,9]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,25,23.5,27]
[null,null,null,null,null,null,null,"H_Rk_vk",0.8,1,1,1,2,1,null,null,null,-8.75,-9.25,-8.5]
[null,null,null,null,null,null,null,"P_Ggs_zg",1,3,1,null,null,null,null,null,null,15,12,17]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,1,1,1,1,null,null,null,-5,-6,-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikke kleilaag"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,1.5,-1,4]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,null,null,null,null,null,null,-4,-6,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restgeulopvulling, bevat soms (grove) zandlagen dunner dan 1m"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,null,null,null,null,null,null,-10,-10.5,-9.75]
[48,3,null,null,"2a",1,null,"mv",null,null,null,null,null,null,null,null,null,-11.25]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,3,1,2,1,null,null,null,-7.25,-8,-6.5]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,3,1,2,1,null,null,null,-7,-7.25,-6]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,7,2,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandgrofte varieert tussen matig fijn en uiterst grof"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,1,null,null,null,null,null,null,-8.5,-9,-8]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,2,1,1,1,1,null,null,null,8,6,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zandgrofte varieert tussen matig fijn en uiterst grof"]
[48,7,null,null,"1e",1,null,"mv",null,null,null,null,null,null,null,null,null,-9.75]
[null,null,null,null,null,null,null,"P_Rg_zg",0.34,2,1,1,1,1,null,null,null,10,9,13]
[null,null,null,null,null,null,null,"P_Rbk_z&s",0.33,2,3,1,2,1,null,null,null,26,24,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dik pakket afgewisseld fijn zand en leemlagen"]
[null,null,null,null,null,null,null,"H_Rk_vk",0.1,1,2,1,2,1,null,null,null,-5.5,-6,-5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,25,22,28]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,2,1,1,1,1,null,null,null,8,7,9]
[]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,3,1,1,1,null,null,null,-6.5,-7.5,-5.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,2,null,null,null,null,null,null,-9,-10,-7]
[null,null,null,null,null,null,null,"H_Rk_k",0.7,1,1,null,null,null,null,null,null,-11.5,-12,-11]
[null,null,null,null,null,null,null,"P_Rg_zm",1,5,1,null,null,null,null,null,null,40,40,40]
[]
[null,null,null,null,null,null,null,"P_Ova_sd",0.3,3,1,1,1,1,null,null,null,3,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal aanwezig: kleipakket met zand en zandige intervallen, veenpakket aan de top"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,2,null,null,null,null,null,null,-1,-2,0]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,2,null,null,null,null,null,null,-1,-2,0]
[]
[null,null,null,null,null,null,null,"P_Ova_sd",0.05,3,1,1,1,1,null,null,null,5,3,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal aanwezig: kleipakket met zand en zandige intervallen, soms bovenin veen"]
[49,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-9]
[null,null,null,null,null,null,null,"P_Rg_zm",0.95,3,1,1,2,1,null,null,null,30,25,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat (dunner dan 2m) kleipakketten; Korrelgrootte wisselt sterk van fijn tot uiterst grof"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.8,1,1,1,1,1,null,null,null,-10,-11,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,null,null,null,null,null,null,-9.5,-10,-8]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.5,1,1,1,1,1,null,null,null,-11,-12,-10]
[49,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-11.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,null,null,null,null,null,null,-10.5,-11.5,-10]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.25,1,1,1,1,1,null,null,null,3,0,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holoceen dek in beekdal"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,2,2,1,2,1,null,null,null,11,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen"]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-2,-5,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Holoceen dek in beekdal"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Twello"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.9,2,2,1,1,1,null,null,null,7.5,4,9]
[50,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hierboven meestal tot 2m dik Antropogeen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,3,2,1,1,1,null,null,null,13,12,18]
[50,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Noordelijk deel segment langs stadsgebied dus tot 2m ophoging"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,3,null,null,null,null,null,null,-5,-6.5,-4]
[]
[null,null,null,null,null,null,null,"P_Ova_sd",0.95,3,1,1,1,1,null,null,null,7,5,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen; kleipakket met zand en zandige intervallen, veen aan de top"]
[50,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-7.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S33H00265 en S33H00221"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,1,null,null,null,null,null,null,-6,-6.5,-2]
[null,null,null,null,null,null,null,"P_Rg_zg",0.3,3,2,null,null,null,null,null,null,35,34,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bevat (dunner dan 3m) kleipakketten"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.1,3,1,1,1,1,null,null,null,3,2,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal aanwezig: kleipakket met zand en zandige intervallen, veen aan detop"]
[51,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dijklichaam volgt snelwegtrace A1 dus huidig maaiveld stuk hoger"]
[null,null,null,null,null,null,null,"H_Rk_ko",0.05,1,3,1,2,1,null,null,null,4,3,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vroeg-holocene kleiplug onderin beekdal"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.15,1,2,1,2,1,null,null,null,-2,-3,-1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,5,1,1,1,null,null,null,-0.5,-1,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vroeg-holocene beekdalopvulling"]
[]
[null,null,null,null,null,null,null,"P_Rg_zm",0.75,1,2,1,2,1,null,null,null,-2,-3,-1]
[null,null,null,null,null,null,null,"P_Rg_zg",0.1,2,2,1,1,1,null,null,null,10,9,11]
[]
[null,null,null,null,null,null,null,"P_Rg_zm",0.75,1,2,1,2,1,null,null,null,-2,-3,-1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,3,1,1,1,null,null,null,-4,-5,-3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.1,2,2,1,1,1,null,null,null,10,9,11]
[51,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dijklichaam volgt snelwegtrace A1 dus huidig maaiveld stuk hoger"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,2,2,1,2,1,null,null,null,11,9,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen"]
[51,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dijklichaam volgt snelwegtrace A1 dus huidig maaiveld stuk hoger"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,2,1,1,2,1,null,null,null,30,29,32]
[]
[null,null,null,null,null,null,null,"H_Vbv_v",0.7,1,1,0.5,2,1,1,1,1,0.5,0.25,0.75]
[52,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-4]
[null,null,null,null,null,null,null,"H_Vbv_v",0.05,1,3,1,3,1,null,null,null,-1,-1.25,-0.75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Alleen in zuidelijkste deel, maaiveld lager ~ +2m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,1,1,1,1,null,null,null,0.5,-1,1.25]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.1,1,4,null,null,null,null,null,null,0,-1,1]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Twello"]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,2,null,null,null,null,null,null,3,-0.5,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wiel- of restgeul opvulling"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Twello"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,1,1,1,2,1,null,null,null,1,-1,3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,2,1,1,3,1,null,null,null,32,30,38]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,1,0.8,1,2,null,null,null,-1,-2,0.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,2,1,1,2,1,null,null,null,11,9,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen; plaatselijk veen aan de top tot maximaal 2 m dik"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,1,1,1,1,null,null,null,-5,-5.5,-4.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.15,1,3,1,2,1,null,null,null,-2.5,-3.5,-2]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.3,1,6,null,null,null,null,null,null,-3,-4,-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vooral in zuidelijke helft van segment"]
[]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,2,1,1,1,null,null,null,-3.5,-4.5,-3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,2,1,1,1,1,null,null,null,2,0.5,4]
[null,null,null,null,null,null,null,"P_Ova_sd",0.6,2,1,1,2,1,null,null,null,7,5,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen; bevat soms zandlagen tot 2m dik, aan de top soms veen tot 1m dik"]
[52,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"S33G00132 en Sondering van Ger ws. S33G00220,221,222; maaiveld loopt op tot +12 mNAP tegen stuwwal in laatste paar honderd meter"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,2,1,2,1,null,null,null,-3,-4,-2]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,2,1,1,1,1,null,null,null,2,-2,4]
[]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.15,1,3,null,null,null,null,null,null,1.75,1.5,2.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rivierduintjes"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.2,2,1,1,2,1,null,null,null,12,11,14]
[]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,35,34,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal dunne (dunner dan 2m) kleilagen"]
[null,null,null,null,null,null,null,"H_Vbv_v",0.1,1,1,1,2,1,null,null,null,1,-0.5,1.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,2,1,1,2,1,null,null,null,12,11,14.5]
[53,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-4]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,38,36,40]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.2,1,3,null,null,null,null,null,null,0,-1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rivierduintjes,dekzandrug"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,38,37,40]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.2,1,3,null,null,null,null,null,null,-5,-6,-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rivierduintjes,dekzandrug"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,35,32,40]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,2,1,1,2,1,null,null,null,11,8,14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen-klei, bevat sporadisch dunne (dunner dan 50cm) veenlagen"]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.5,3,1,1,3,1,null,null,null,37,35,40]
[]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,13,11,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Zutphen-klei, bevat sporadisch dunne (dunner dan 50cm) veenlagen"]
[53,9,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-2]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,2,1,1,1,1,null,null,null,11,9,12]
[null,null,null,null,null,null,null,"P_Ova_sd",0.9,3,2,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kreftenheye-Twello-klei"]
[null,null,null,null,null,null,null,"P_Wdz_zf",0.6,1,2,1,2,1,null,null,null,2.25,1.5,3]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,24,17,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sporadisch dunne (dunner dan 50cm) kleilagen"]
[null,null,null,null,null,null,null,"H_Rk_k",0.15,1,2,1,1,1,null,null,null,0.75,0.5,1]
[null,null,null,null,null,null,null,"H_Rk_k",0.2,1,5,1,1,1,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"H_Vbv_v",0.5,1,1,1,2,1,null,null,null,2,0.75,3]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Gecombineerd Formaties van Kreftenheye, Urk en Appelscha"]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,2,1,1,1,null,null,null,0.5,0,1]
[null,null,null,null,null,null,null,"P_Gkl_kz",0.15,2,2,1,2,1,null,null,null,22,20,24]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-11.5,-12.5,-8.5]
[54,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-13]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,10,9,12]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,2,null,null,null,null,null,null,-10.5,-11,-10]
[54,4,4,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt grotendeels op hoge grond langs Niersdal"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,2,1,null,null,null,null,null,null,-10,-11,-1]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,0,-2.5,6]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,null,null,null,null,null,null,-10,-11,-9]
[]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,15,10,18]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,2,null,null,null,null,null,null,-11.5,-12,-11]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.15,1,1,null,null,null,null,null,null,-9,-9.5,-8.5]
[null,null,null,null,null,null,null,"P_Rg_zm",1,4,1,null,null,null,null,null,null,4,1,5]
[]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,2,0,6]
[null,null,null,null,null,null,null,"P_Ova_sd",1,6,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oosterhout"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,2,null,null,null,null,null,null,-7.5,-9,-6]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,5,1,1,2,1,null,null,null,30,28,32]
[null,null,null,null,null,null,null,"H_Rk_k",0.5,1,1,null,null,null,null,null,null,-12.25,-13,-10]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-12.25,-13,-10]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Breda-afzettingen, afwisseling tussen zand- en kleilagen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,1,1,1,2,1,null,null,null,2,0,4]
[]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Breda-afzettingen, afwisseling tussen zand- en kleilagen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,2,1,1,2,1,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.5,1,1,null,null,null,null,null,null,-11,-11.75,-9.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Breda-afzettingen, afwisseling tussen zand- en kleilagen"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,4,1,null,null,null,null,null,null,12,8,15]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.8,1,1,0.1,1,1,null,null,null,-10,-11,-9]
[]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,3,1,null,null,null,null,null,null,19,17.5,20.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,1,1,1,1,null,null,null,-13,-13.5,-10.5]
[null,null,null,null,null,null,null,"P_Wrd_zm",0.1,1,1,1,2,1,null,null,null,-12,-12.5,-10]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,3,2,null,null,null,null,null,null,19,17.5,20.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,0.95,1,1,null,null,null,-11.25,-11.5,-11]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Breda-afzettingen, afwisseling tussen zand- en kleilagen"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.3,1,1,1,2,1,null,null,null,-8,-10,-4]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Breda-afzettingen, afwisseling tussen zand- en kleilagen"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,1,-1,4]
[60,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt op terrasrand met plaatselijk hogere grond met zand vanaf het maaiveld"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,4,2,null,null,null,null,null,null,10,9,20]
[null,null,null,null,null,null,null,"H_Rk_k",0.4,1,1,0.1,1,2,null,null,null,-11.5,-12.5,-10.5]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,4,2,null,null,null,null,null,null,10,8,25]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,1,2,null,null,null,null,null,null,-12,-12.5,-8]
[]
[60,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Met plaatselijk hogere grond met zand vanaf het maaiveld"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,5,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Breda-afzettingen, afwisseling tussen zand- en kleilagen. "]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,-4,-6,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Voornamelijk grof, maar ook matig grof zand"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,1,1,null,null,null,null,null,null,-12.5,-13.5,-12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"02P002480_94 en 02P002480_95 voorbeeld van grote lokale variatie over 100 m in P_Rg_zm en P_Rg_zg. "]
[]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-4,-6,-1]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,1,0.15,1,1,null,null,null,-11,-12,-10.5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.4,3,1,null,null,null,null,null,null,20,15,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top van P_Rg_zm regelmatig met klei"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,1,0.3,1,1,null,null,null,-11.5,-12,-11]
[null,null,null,null,null,null,null,"P_Rg_zf",0.6,3,2,null,null,null,null,null,null,17,16,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top van P_Rg_zf regelmatig met klei"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,1,0.4,1,2,null,null,null,-12.25,-13.5,-11.75]
[null,null,null,null,null,null,null,"P_Rg_zm",0.85,3,2,null,null,null,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zm",0.6,1,2,null,null,null,null,null,null,-8,-9,-3]
[63,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt plaatselijk op hogere grond met zand vanaf het maaiveld"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,1,1,1,1,null,null,null,-13.5,-14,-10]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Breda-afzettingen, afwisseling tussen zand- en kleilagen. "]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,9,8,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[65,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-14.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de noordzijde kruist een beekdal (met beek) het segment. "]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,3,1,1,1,1,null,null,null,-4,-5,0]
[]
[null,null,null,null,null,null,null,"H_Rg_zm",1,2,1,null,null,null,null,null,null,-9,-12,-8]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,5,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,2,1,null,null,null,null,null,null,-12.5,-15,-11]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,5,1,1,2,1,null,null,null,8,7,9.5]
[66,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,1,1,2,1,null,null,null,9,8,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,2,null,null,null,null,null,null,9,8,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.6,5,1,1,1,1,null,null,null,11,10,14]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,5,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[67,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,1,0.5,1,1,null,null,null,-13.5,-15.5,-11.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.8,1,1,0.5,1,2,null,null,null,-14.5,-15.5,-12.5]
[null,null,null,null,null,null,null,"H_Rg_zm",0.8,1,1,1,2,1,null,null,null,-12,-13,-11]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.2,1,2,null,null,null,null,null,null,-9.5,-11,-8]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-2.5,-4,-1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,1,1,1,1,null,null,null,0,-1,1]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,3,1,1,2,1,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,3,2,null,null,null,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,1,1,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[67,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,1,null,null,null,null,null,null,-13.5,-15.5,-11.5]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,2,null,null,null,null,null,null,-14.5,-15.5,-12.5]
[null,null,null,null,null,null,null,"H_Rg_zm",1,2,1,null,null,null,null,null,null,-12,-13,-11]
[null,null,null,null,null,null,null,"H_Rg_zg",1,3,1,null,null,null,null,null,null,-6,-7,-5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,4,1,1,1,1,null,null,null,-3.5,-4.5,-2.5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,4,1,1,2,1,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,4,2,null,null,null,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,5,1,1,1,1,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,5,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.099999999999994,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,1,1,null,null,null,null,null,null,-14,-15,-12]
[null,null,null,null,null,null,null,"H_Rg_zm",0.4,1,2,1,1,1,null,null,null,-15,-15.5,-12]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,2,1,2,1,null,null,null,-14,-14.5,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-0.5,-4.5,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,1,1,1,1,null,null,null,0.5,0,3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,3,1,1,2,1,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,3,2,null,null,null,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,1,1,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.099999999999994,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,1,1,null,null,null,null,null,null,-10,-12,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,null,null,null,null,null,null,-14.5,-15,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-0.5,-4.5,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,1,1,1,1,null,null,null,0.5,0,3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,3,1,1,2,1,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,3,2,null,null,null,null,null,null,4,3,6]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,1,1,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.099999999999994,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,1,1,null,null,null,null,null,null,-10,-12,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,1,2,1,null,null,null,-14.5,-15,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-6,-8,-4.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,3,1,1,1,1,null,null,null,-4,-5,-3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,3,1,1,2,1,null,null,null,4,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,3,2,null,null,null,null,null,null,4,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,1,1,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.099999999999994,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,1,1,null,null,null,null,null,null,-10,-12,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,1,2,1,null,null,null,-14.5,-15,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-6,-8,-4.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,3,1,1,1,1,null,null,null,-4,-5,-3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,3,1,1,2,1,null,null,null,4,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,3,2,null,null,null,null,null,null,4,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,1,1,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.099999999999994,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16.5]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,1,1,null,null,null,null,null,null,-10.5,-12,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,1,2,1,null,null,null,-14.5,-15,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-6,-8,-4.5]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,3,1,1,1,1,null,null,null,-4,-5,-3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,3,1,1,2,1,null,null,null,4,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,3,2,null,null,null,null,null,null,4,3,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.4,4,1,1,1,1,null,null,null,6.5,6,10]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.099999999999994,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16.5]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,1,1,null,null,null,null,null,null,-10.5,-12,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,1,2,1,null,null,null,-14.5,-15,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-10,-10.5,-9]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,3,1,1,1,1,null,null,null,-8,-9,-6]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,3,1,1,2,1,null,null,null,-1,-2,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,3,2,null,null,null,null,null,null,-1,-2,0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal komen kleilagen voor van 1-2 m dik"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,4,1,1,1,1,null,null,null,1.5,1,3]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,4,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.099999999999994,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,1,null,null,null,null,null,null,-12,-13,-10]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,1,2,1,null,null,null,-15,-15.5,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-9.5,-10.5,-7]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,-5,-9,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de kleilaag komen regelmatig zandlagen voor"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,2,null,null,null,null,null,null,-1,-2,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,1,1,1,1,null,null,null,1.5,1,5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[68.2,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16.5]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.1,1,1,null,null,null,null,null,null,-10,-12,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,null,null,null,null,null,null,-14.5,-15.5,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-4,-6,-1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.95,3,1,1,1,1,null,null,null,8,1,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de kleilaag komen regelmatig onderling verbonden zandlagen voor van 1-2.5 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,3,2,null,null,null,null,null,null,40,40,40]
[]
[68.2,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-18]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-14.5,-15.5,-13.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer lokaal komt 1 m zand direct onder maaiveld voor"]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-9,-10,-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,8,3,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de kleilaag komen regelmatig onderling verbonden zandlagen voor van 1-2.5 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[68.2,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sondering S68.62+50 voorbeeld van Pleistocene klei met hoge conusweerstand (top Kiezelooliet)"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,1,null,null,null,null,null,null,-10,-12,-9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer lokaal komt 1 m zand direct onder maaiveld voor"]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.05,1,2,null,null,null,null,null,null,-10,-12,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,3,null,null,null,null,null,null,-14.5,-15.5,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-4,-9,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.95,3,1,1,1,1,null,null,null,8,1,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de kleilaag komen regelmatig onderling verbonden zandlagen voor van 1-2.5 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,3,2,null,null,null,null,null,null,40,40,40]
[]
[68.2,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-17]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-15,-15.5,-13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-6,-8,-5]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,-4,-4.5,5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[69,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,1,null,null,null,null,null,null,-12,-13,-10]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,1,2,1,null,null,null,-15,-15.5,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-8,-9,-7]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,-5,-7,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de kleilaag komen regelmatig zandlagen voor"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,2,null,null,null,null,null,null,-1,-2,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,1,1,1,1,null,null,null,1.5,1,5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[69,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-16.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,1,null,null,null,null,null,null,-12,-13,-10]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,1,2,1,null,null,null,-15,-15.5,-13.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-8,-9,-7]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,-5,-7,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de kleilaag komen regelmatig zandlagen voor"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,4,2,null,null,null,null,null,null,-1,-2,1]
[null,null,null,null,null,null,null,"P_Ova_sd",0.5,5,1,1,1,1,null,null,null,1.5,1,5]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,1,1,2,1,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,5,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kleilagen van enkele meters dik kunnen verspreid voorkomen"]
[]
[70,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-17.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,1,null,null,null,null,null,null,-10.5,-12,-9.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,null,null,null,null,null,null,-15.5,-16.5,-14.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-5,-8,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.95,3,1,1,1,1,null,null,null,5,-1,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de kleilaag komen regelmatig onderling verbonden zandlagen voor van 1-2.5 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,3,2,null,null,null,null,null,null,40,40,40]
[]
[70,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt op terrasrand, aan de rivierkant (buitendijks) ligt tot 7 m klei"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,null,null,null,null,null,null,-10.5,-12,-9.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,2,null,null,null,null,null,null,-15.5,-16.5,-14.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-5,-8,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.05,3,1,1,1,1,null,null,null,-2.5,-3,18]
[null,null,null,null,null,null,null,"P_Rg_zg",0.05,3,1,1,2,1,null,null,null,40,40,40]
[null,null,null,null,null,null,null,"P_Rg_zg",0.95,3,2,null,null,null,null,null,null,40,40,40]
[]
[70,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt op terrasrand, aan de rivierkant (buitendijks) ligt 2 tot 7 m klei"]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-15.5,-17.5,-14.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-5,-8,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[71,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-18.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,1,null,null,null,null,null,null,-11.5,-16,-10]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,null,null,null,null,null,null,-17.5,-18,-16]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-5,-8,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,1,1,1,null,null,null,40,40,40]
[]
[72,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt op terrasrand, plaatselijk 3 m hoogteverschil binnen- en buitendijks"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,null,null,null,null,null,null,-18.75,-19,-18]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-17.25,-17.5,-14.25]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-7,-8,-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[72,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-20]
[null,null,null,null,null,null,null,"P_Wrd_zm",1,1,1,null,null,null,null,null,null,-19,-19.25,-18]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,2,1,null,null,null,null,null,null,-18.75,-19,-18]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,2,2,null,null,null,null,null,null,-16,-17.5,-14.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"H_Rg_zg",1,3,1,null,null,null,null,null,null,-7,-8,-3]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[72,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19.25]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-18.25,-19.25,-17.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-10.5,-11.5,-9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[73,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt op terrasrand, plaatselijk 3 m hoogteverschil binnen- en buitendijks"]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-19,-20,-18]
[null,null,null,null,null,null,null,"H_Rg_zg",0.5,2,1,null,null,null,null,null,null,-15,-15.5,-14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"H_Rg_zg",0.5,2,2,null,null,null,null,null,null,-8,-14,-5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[73,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld varieert tussen 18 en 21 m NAP. 02P002480_185 voorbeeld dunne H_Rg_zm op H_Rg_zg (grindrijk) op Breda"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,1,1,1,1,null,null,null,-18,-18.5,-17]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,1,1,2,1,null,null,null,-14,-15,-13]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,null,null,null,null,null,null,-16,-16.5,-15]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-13,-15,-10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[73,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt tegen terrasrand"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-18,-18.5,-17]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,1,1,2,1,null,null,null,-14,-15,-13]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-16.5,-17,-15.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-6,-7,-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[73,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt op terrasrand, plaatselijk 3 m hoogteverschil binnen- en buitendijks"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-18,-18.5,-17]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,1,1,2,1,null,null,null,-14,-15,-10]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-16.5,-17,-15.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-6,-7,-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[73,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt bij terrasrand"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-16,-17,-15]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-13,-15,-12]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,28,24,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Korrelgrootte varieert van matig grof tot grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[73,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-20.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-19,-20,-15]
[null,null,null,null,null,null,null,"H_Rg_zf",1,2,1,null,null,null,null,null,null,-13.5,-15,-12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk kleiig"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,-5,-9,-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[73,7,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Langs de rand van het beekdal van de Swalm"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-17,-17,-15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,1,1,1,2,1,null,null,null,-5,-7,-2]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,2,1,1,1,null,null,null,-16,-16.5,-14]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,1,2,1,2,1,null,null,null,-5,-7,-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Stramproy"]
[]
[74,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kruist het beekdal van de Haelensche beek"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-17,-18.5,-17]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,1,1,2,1,null,null,null,-14,-15,-13]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-11,-12,-10.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-8,-11,-5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-2 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[74,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kruist het beekdal van de Haelensche beek"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-17,-18.5,-17]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,1,1,2,1,null,null,null,-14,-15,-13]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-11,-12,-10.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,20,18,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-2 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[74,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-20]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,1,null,null,null,null,null,null,-17,-19,-16]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,2,null,null,null,null,null,null,-20,-20,-20]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,2,1,1,2,1,1,1,1,-16.5,-18.5,-16]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,2,1,1,2,1,1,2,1,-14,-15,-13]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,2,2,null,null,null,null,null,null,-11,-12,-10.5]
[null,null,null,null,null,null,null,"H_Rg_zg",1,3,1,null,null,null,null,null,null,15,11,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-2 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[75,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ter plaatse van huidige uiterwaard maaiveld rond 17.5 m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.65,1,1,1,1,1,null,null,null,-18,-19,-17]
[null,null,null,null,null,null,null,"H_Rg_zf",0.65,1,1,1,2,1,null,null,null,-10,-11,-9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Siltig, kleiig 02P002480_198 voorbeeld"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,2,null,null,null,null,null,null,-10,-15,-8.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"02P002480_205 voorbeeld"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,18,16,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-2 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[75,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,1,null,null,null,null,null,null,-17,-18,-16.5]
[null,null,null,null,null,null,null,"H_Rg_zf",0.3,1,2,null,null,null,null,null,null,-16,-17,-15]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.8,2,1,null,null,null,null,null,null,-10,-13,-9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk tot 2 m veen"]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.2,2,2,null,null,null,null,null,null,-15,-16,-13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk tot 2 m veen"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,3,1,null,null,null,null,null,null,24,20,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[76,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19.5]
[null,null,null,null,null,null,null,"H_Rg_zf",0.3,1,1,1,1,1,null,null,null,-14,-16,-12]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,1,1,2,1,null,null,null,-10,-11,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,0.5,1,1,null,null,null,-10,-11,-9]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,0.5,1,2,null,null,null,-14,-15,-12]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,20,18,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[76.099999999999994,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eiland tussen Roertakken. Vlak langs Roer, maaiveld aanzienlijk lager"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-18,-19,-16]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,1,1,1,2,1,null,null,null,-14.5,-15.5,-12]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-14.5,-16,-10]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,29,20,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m, in ieder geval regelmatig in het bereik 9-12 m NAP"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[77,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Loopt langs zuidrand Roerdal. "]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,1,1,1,null,null,null,-18,-19,-16]
[null,null,null,null,null,null,null,"P_Rg_zf",0.5,1,1,1,2,1,null,null,null,-14.5,-15.5,-12]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-14.5,-16,-10]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,29,20,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m, in ieder geval regelmatig in het bereik 9-12 m NAP"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[77,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-19.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt veelal direct langs de Maas of grindgaten"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,1,null,null,null,null,null,null,-14.5,-16,-12]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,2,1,1,1,null,null,null,-17.5,-18.5,-17]
[null,null,null,null,null,null,null,"P_Rg_zf",0.35,1,2,1,2,1,null,null,null,-16,-16.5,-15]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,1,1,1,null,null,null,-16.5,-17.5,-15]
[null,null,null,null,null,null,null,"H_Rr_o&z",0.05,1,3,1,2,1,null,null,null,-10,-13,-9]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,32,28,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m, met name beneden de 12 m - NAP"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,3,1,null,null,null,null,null,null,40,40,40]
[]
[78,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Loopt plaatselijk langs terrasrand met meer dan 3 m hoogteverschil. Buitendijks opvulling grindgat"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.6,1,1,null,null,null,null,null,null,-18,-19.5,-15]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,2,null,null,null,null,null,null,-18,-19.5,-15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk veeninsluiting van 0.5-1 m dik"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,0,-3,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,25,20,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top komen regelmatig kleilagen voor van 1-4 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[78.099999999999994,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Loopt langs terrasrand met meer dan 3 m hoogteverschil"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.8,1,1,null,null,null,null,null,null,-19,-21,-18]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,2,null,null,null,null,null,null,-19,-22,-18]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,0,-3,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,25,20,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top komen regelmatig kleilagen voor van 1-4 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[79,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plaatselijk buitendijks grindgat opvulling"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.5,1,1,null,null,null,null,null,null,-20,-21.5,-16]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-20,-21.5,-16]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-3,-5,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,3,0,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top komen regelmatig kleilagen voor van 1-4 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[80,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Buitendijks opvulling grindgat in het westelijke deel"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,1,null,null,null,null,null,null,-18,-19.5,-15]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,null,null,null,null,null,null,-19,-20,-15]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,0,-3,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,15,10,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aan de top komen regelmatig kleilagen voor van 1-4 m"]
[null,null,null,null,null,null,null,"P_Rg_zf",1,4,1,null,null,null,null,null,null,40,40,40]
[]
[81,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt grotendeels op rand van ouder terras dat 1-2 m hoger ligt dan huidig terras. Plaatselijk buitendijks grindgat opvulling\n. Deze kenmerkt zich tot een zandige klei opvulling tot soms 12 m NAP. Bijvoorbeeld S60A00228,229,232,233"]
[null,null,null,null,null,null,null,"H_Rk_k",0.05,1,1,null,null,null,null,null,null,-22.5,-23.5,-19]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,2,null,null,null,null,null,null,-22.5,-23.5,-19]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-13,-15,-7]
[null,null,null,null,null,null,null,"P_Rg_zf",0.8,3,1,null,null,null,null,null,null,17,11,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Stramproy. Aan de top van de Stramproy (onder P_Rg_zg) komen soms kleilagen voor 1-2 m."]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,2,null,null,null,null,null,null,17,11,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Stramproy. Aan de top van de Stramproy (onder P_Rg_zg) komen soms kleilagen voor 1-2 m."]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer kleiige Fm van Kiezelooliet. Bevat ook fijne zandlagen"]
[]
[81,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-24.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ligt grotendeels op rand van ouder terras dat 1-2 m hoger ligt dan huidig terras. Plaatselijk buitendijks grindgat opvulling\n. Deze kenmerkt zich tot een zandige klei opvulling tot soms 12 m NAP. Bijvoorbeeld S60A00228,229,232,233"]
[null,null,null,null,null,null,null,"H_Rk_k",0.15,1,1,null,null,null,null,null,null,-21.5,-23.5,-18.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.85,1,2,null,null,null,null,null,null,-21.5,-23.5,-18.5]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-7,-9,-3]
[null,null,null,null,null,null,null,"P_Rg_zf",0.8,3,1,null,null,null,null,null,null,17,11,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Stramproy. Aan de top van de Stramproy (onder P_Rg_zg) komen soms kleilagen voor 1-2 m."]
[null,null,null,null,null,null,null,"P_Rg_zm",0.2,3,2,null,null,null,null,null,null,17,11,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Stramproy. Aan de top van de Stramproy (onder P_Rg_zg) komen soms kleilagen voor 1-2 m."]
[null,null,null,null,null,null,null,"P_Ova_sd",1,4,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zeer kleiige Fm van Kiezelooliet. Bevat ook fijne zandlagen"]
[]
[82,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-26.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Slingert rondom geulvormige laagte"]
[null,null,null,null,null,null,null,"H_Rg_zm",0.3,1,1,null,null,null,null,null,null,-24.5,-25.5,-24]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,2,null,null,null,null,null,null,-23.5,-24,-21]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-10,-12,-8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Rg_zm",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Verspreid komen regelmatig kleilagen voor vna 1-4 m dik"]
[]
[83.84,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-35]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-33.5,-34.5,-29]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-27,-29,-23]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Breda"]
[]
[83.84,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-33.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld loopt af van zuid naar noord van 35 tot 32.5 m ANP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.65,1,1,null,null,null,null,null,null,-31.5,-32.5,-31]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,2,null,null,null,null,null,null,-28,-31,-26]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-23,-25,-20]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Breda"]
[]
[83.84,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-31.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,1,null,null,null,null,null,null,-31,-32.5,-29]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-28,-29,-25]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-18,-20,-14]
[null,null,null,null,null,null,null,"P_Ova_sd",0.2,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Breda"]
[null,null,null,null,null,null,null,"P_Rg_zm",0.8,3,2,1,1,1,null,null,null,-5,-15,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kiezelooliet"]
[null,null,null,null,null,null,null,"P_Ova_sd",0.8,3,2,1,2,2,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Breda"]
[]
[83.84,4,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-30.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Loopt in noordelijk deel langs restgeul met maaiveld op 28 m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.2,1,1,null,null,null,null,null,null,-29.75,-30.25,-29]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.8,1,2,null,null,null,null,null,null,-27.5,-29,-24]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-10,-18,-5]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Stramproy. Bevat soms kleilagen van 1-2 m aan de top"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.3,3,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Stramproy. Bevat soms kleilagen van 1-2 m aan de top"]
[]
[83.84,5,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-29]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,1,null,null,null,null,null,null,-27,-28.5,-26]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.65,1,2,null,null,null,null,null,null,-25,-26,-23]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-13,-15,-8]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Stramproy. Bevat soms kleilagen van 1-2 m aan de top. Dieper kunnen ook onderbroken kleilagen voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.3,3,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Stramproy. Bevat soms kleilagen van 1-2 m aan de top. Dieper kunnen ook onderbroken kleilagen voorkomen"]
[]
[83.84,6,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld loopt af van zuid naar noord van 28.5 naar 27.5 m NAP. Zuidelijke deel ligt direct langs de Maas"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,1,null,null,null,null,null,null,-27,-28,-26]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,2,null,null,null,null,null,null,-24.5,-26,-23]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-11,-17,-8]
[null,null,null,null,null,null,null,"P_Rg_zm",0.7,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Stramproy. Bevat soms kleilagen van 1-2 m aan de top. Dieper kunnen ook onderbroken kleilagen voorkomen"]
[null,null,null,null,null,null,null,"P_Rg_zf",0.3,3,2,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fm. Van Stramproy. Bevat soms kleilagen van 1-2 m aan de top. Dieper kunnen ook onderbroken kleilagen voorkomen"]
[]
[85,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-34]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,null,null,null,null,null,null,-30,-32.5,-28.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loss"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,2,null,null,null,null,null,null,-28,-28.5,-26,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loss"]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-25,-27.5,-22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Breda"]
[]
[85,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-34]
[null,null,null,null,null,null,null,"H_Ro_z&k",1,1,1,null,null,null,null,null,null,-29,-31,-27.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loss"]
[null,null,null,null,null,null,null,"H_Rg_zg",1,2,1,null,null,null,null,null,null,-26,-28.5,-24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"In de zandlaag komen af en toe kleilagen voor van 0.5-1.5 m"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Formatie van Breda"]
[]
[86.87,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-38.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,1,null,null,null,null,null,null,-37.5,-38,-36]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,2,null,null,null,null,null,null,-34,-36,-32]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,3,1,1,1,null,null,null,-36.5,-38,-35]
[null,null,null,null,null,null,null,"H_Rk_k",0.3,1,3,1,2,1,null,null,null,-34,-36,-32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stijve klei"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,4,null,null,null,null,null,null,-31,-32,-30]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-28,-30,-23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rupel met daaronder Tongeren"]
[]
[86.87,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld rondom plas langs Veldjensweg lokaal 34,35 m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,1,null,null,null,null,null,null,-36,-36.5,-35]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,2,null,null,null,null,null,null,-34,-35,-33]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,4,null,null,null,null,null,null,-31,-33,-30]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-26,-28,-24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rupel met daaronder Tongeren"]
[]
[88,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-41]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,null,null,null,null,null,null,-38,-39.5,-37]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,3,null,null,null,null,null,null,-36,-39,-33]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-29,-31,-26,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vrijwel overal Rupel klei met daaronder Tongeren en daaronder kalksteen. Soms onder Tongeren nog Landen klei"]
[]
[89,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-42.5]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.7,1,1,null,null,null,null,null,null,-40,-41.5,-39]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.3,1,3,null,null,null,null,null,null,-38,-39,-35]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-31,-33,-29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vrijwel overal Tongeren klei met daaronder kalksteen"]
[]
[90,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-44.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal binnendijks opgehoogd tot 48 m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.4,1,1,null,null,null,null,null,null,-43.5,-44,-42,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.55000000000000004,1,2,null,null,null,null,null,null,-41.5,-42,-40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,-37,-40,-34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.8,2,1,null,null,null,null,null,null,-35,-36,-32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.2,2,2,null,null,null,null,null,null,-31,-32,-30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kalksteen, verkit zandsteen en klei"]
[]
[90,2,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-45,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top waarschijnlijk sterk geroerd"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,1,null,null,null,null,null,null,-44,-44.5,-42.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,2,null,null,null,null,null,null,-42,-42.5,-40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,-37,-40,-34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-35,-36,-33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kalksteen, verkit zandsteen en klei"]
[]
[90,3,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-47]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.45,1,1,null,null,null,null,null,null,-46,-46.5,-45,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.5,1,2,null,null,null,null,null,null,-42.5,-45,-40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,-39,-40,-38,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-38,-40,-36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kalksteen, verkit zandsteen en klei"]
[]
[91,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-43,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maaiveld varieert tussen ongeveer 42 en 44 m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,null,null,null,null,null,null,-41,-42,-40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,-36,-40,-35]
[null,null,null,null,null,null,null,"P_Rg_zg",0.7,2,1,null,null,null,null,null,null,-33,-34,-31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.3,2,2,null,null,null,null,null,null,-35,-36,-34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms Tongeren klei aan de top, daaronder kalksteen"]
[]
[92,1,null,null,"2c",1,null,"mv",null,null,null,null,null,null,null,null,null,-44.25]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.95,1,1,null,null,null,null,null,null,-42,-42.75,-40.75]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,-37.25,-40.75,-35]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-35,-36,-33]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Soms Tongeren klei aan de top, daaronder kalksteen"]
[]
[93,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-44.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lokaal binnendijks opgehoogd tot 49 m NAP"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.35,1,1,null,null,null,null,null,null,-43.5,-44,-42]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.6,1,2,null,null,null,null,null,null,-41,-42,-40]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.05,1,3,null,null,null,null,null,null,-37,-40,-34]
[null,null,null,null,null,null,null,"P_Rg_zg",0.4,2,1,null,null,null,null,null,null,-34,-35,-32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.6,2,2,null,null,null,null,null,null,-30,-32,-29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kalksteen, verkit zandsteen en klei"]
[]
[94,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-48]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,null,null,null,null,null,null,-46,-47,-44]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,2,null,null,null,null,null,null,-43,-44,-42]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,2,1,null,null,null,null,null,null,-40,-42,-39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Rg_zg",0.5,2,2,null,null,null,null,null,null,-37,-39,-33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kalksteen, verkit zandsteen en klei"]
[]
[95,1,null,null,null,1,null,"mv",null,null,null,null,null,null,null,null,null,-49]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.9,1,1,null,null,null,null,null,null,-46,-47,-44,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bestaat deels uit verspoelde loess"]
[null,null,null,null,null,null,null,"H_Ro_z&k",0.1,1,2,null,null,null,null,null,null,-43,-44,-42]
[null,null,null,null,null,null,null,"P_Rg_zg",1,2,1,null,null,null,null,null,null,-41,-42,-36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Eenheid bestaat met name uit grind"]
[null,null,null,null,null,null,null,"P_Ova_sd",1,3,1,null,null,null,null,null,null,40,40,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kalksteen, verkit zandsteen en klei"]

{"sheet":"unit descr.","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"sedimentaire facieseenheden","index":2,"n_rows":52,"n_cols":5,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
["P_Rg_zs","Pfsf",null,"Tcsm","H_Mg_zm"]
["P_Rg_zm","Pfsm",null,"Tcss","H_Mg_zf"]
["P_Rg_zg","Pfsc",null,"Tcsf","H_Mg_zk"]
["P_Rk_k&s","Pvcs",null,"Tfss","H_Mp_zf"]
["P_Wls_s","Pasi",null,"Tccs","H_Mr_kz"]
["P_Rbk_z&s","Pvss",null,"Tfsc","H_Mkw_k&z"]
["P_Rbk_zm","Pvsm",null,"Tfcc","H_Mp_k"]
["P_Wdz_zf","Pasf",null,"Tfco","H_Mp_ko"]
["P_Wrd_zm","Pasm",null,"Lfco","H_Ml_ko"]
["P_Gkl_kz","Pgcs",null,"Ecsm","H_Eg_zm"]
["P_Gs_zg","Pgsc",null,"Eccs","H_Eg_k&z"]
["P_Om_k","Pgcc",null,"Fcsc","H_Rg_zg"]
["P_Om_zf","Pgsf",null,"Fcsm","H_Rg_zm"]
["P_Ggs_zg","Pgip",null,"Fcsf","H_Rg_zf"]
["P_Mg_zk","Ptsc",null,"Fcos","H_Rr_o&z"]
["P_Mg_zm","Ptsm",null,"Fpsc","H_Ro_k&z"]
["P_Mp_k","Ptcc",null,"Fpcc","H_Rk_k"]
["P_Ova_sd","Pxlp",null,"Fbcd Fbpd","H_Rk_k&v"]
["H_Rg_zf","Fcsf",null,"Fbco","H_Rk_ko"]
["H_Rg_zm","Fcsm",null,"Fbpc","H_Rk_vk"]
["H_Rg_zg","Fcsc",null,"Shpp","H_Vhv_v"]
["H_Eg_k&z","Eccs",null,"Sbpp","H_Vbv_v"]
["H_Eg_zm","Ecsm",null,"Rssm/Rssc","H_Ova_zm"]
["H_Rk_k","Fpcc",null,"Rssf","H_Ova_zf"]
["H_Ro_k&z","Fpsc",null,"Aaop","H_Aa_ht"]
["H_Rk_ko","Fbco",null,"Ptsm","P_Mg_zm"]
["H_Rk_vk","Fbpc",null,"Ptsc","P_Mg_zk"]
["H_Rk_k&v","FbcdFbpd",null,"Ptcc","P_Mp_k"]
["H_Rr_o&z","Fcos",null,"Pfsc","P_Rg_zg"]
["H_Mp_k","Tfcc",null,"Pfsm","P_Rg_zm"]
["H_Mp_ko","Tfco",null,"Pfsf","P_Rg_zs"]
["H_Mkw_k&z","Tfsc",null,"Pvcs","P_Rk_k&s"]
["H_Mp_zf","Tfss",null,"Pvsm","P_Rbk_zm"]
["H_Mg_zk","Tcsf",null,"Pvss","P_Rbk_z&s"]
["H_Mg_zf","Tcss",null,"Pasm","P_Wrd_zm"]
["H_Mg_zm","Tcsm",null,"Pasf","P_Wdz_zf"]
["H_Mr_kz","Tccs",null,"Pasi","P_Wls_s"]
["H_Ml_ko","Lfco",null,"Pgsc","P_Gs_zg"]
["H_Vhv_v","Shpp",null,"Pgip","P_Ggs_zg"]
["H_Vbv_v","Sbpp",null,"Pgcs","P_Gkl_kz"]
["H_Ova_zm","Rssc/Rssm",null,"Pgsf","P_Om_zf"]
["H_Ova_zf","Rssf",null,"Pgcc","P_Om_k"]
["H_Aa_ht","Aaop",null,"Pxlp","P_Ova_sd"]
[]
[]
[]
[]
[]
[]
[]
[]
["END","END"]

{"sheet":"Global application layer types","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Items","index":4,"n_rows":31,"n_cols":2,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["ITEMS"]
["Segment ID","Iseg"]
["Global Scenario Type","GScT"]
["ID global senario","Igsc"]
["P global scenario","Pgsc"]
[]
["Sedimentary Facies Unit","SFU"]
["P sedimentary facies unit","Psfu"]
["position sedimentary facies unit","Tsfu"]
["correlated sedimentary facies unit","Csfu"]
["Depth basis representative sedimentary facies unit","Hsfr"]
["Depth basis minimum sedimentary facies unit","Hsfi"]
["Depth basis maximum sedimentary facies unit","Hsfa"]
[]
[]
["sedimentary Facies Subunit","SFS"]
["P sedimentary facies subunit","Psfs"]
["position sedimentary facies subunit","Tsfs"]
[]
["Global Application Layer","GAL"]
["P global application layer","Pgal"]
["position global application layer","Tgal"]
[]
[]
[]
[]
[]
["application layer","AL"]
[null,"Pal"]
[null,"Tal"]
["Remarks application layer","Ral"]

{"sheet":"GLobal appl layers out","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"TOut","index":6,"n_rows":17,"n_cols":25,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[null,"segment_id","index","probability","grondtypes",null,null,null,null,null,null,null,null,null,null,"toplevels"]
[null,33,1,1.26E-2,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 4H_Vhv_v"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,null,4,4.5,6.5,8.5,9,13,24,25,40]
[null,null,2,2.9399999999999999E-2,"mv"," 3H_Mp_k"," 4H_Vhv_v"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,null,null,4,6.5,8.5,9,13,24,25,40]
[null,null,3,2.9399999999999999E-2,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 5H_Vhv_v"," 6H_Mp_k"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,4,4.5,6.5,7.5,8.5,9,13,24,25,40]
[null,null,4,6.8599999999999994E-2,"mv"," 3H_Mp_k"," 5H_Vhv_v"," 6H_Mp_k"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,null,4,6.5,7.5,8.5,9,13,24,25,40]
[null,null,5,5.4000000000000003E-3,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 4H_Vhv_v"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,null,4,4.5,6.5,8.5,9,13,24,25,40]
[null,null,6,1.26E-2,"mv"," 3H_Mp_k"," 4H_Vhv_v"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,null,null,4,6.5,8.5,9,13,24,25,40]
[null,null,7,1.26E-2,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 5H_Vhv_v"," 6H_Mp_k"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,4,4.5,6.5,7.5,8.5,9,13,24,25,40]
[null,null,8,2.9399999999999999E-2,"mv"," 3H_Mp_k"," 5H_Vhv_v"," 6H_Mp_k"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 11P_Ova_sd"," 12P_Mg_zm",null,null,4,6.5,7.5,8.5,9,13,24,25,40]
[null,null,9,5.04E-2,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 4H_Vhv_v"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,null,4,4.5,6.5,8.5,9,13,24,40]
[null,null,10,0.1176,"mv"," 3H_Mp_k"," 4H_Vhv_v"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,null,null,4,6.5,8.5,9,13,24,40]
[null,null,11,0.1176,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 5H_Vhv_v"," 6H_Mp_k"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,4,4.5,6.5,7.5,8.5,9,13,24,40]
[null,null,12,0.27439999999999998,"mv"," 3H_Mp_k"," 5H_Vhv_v"," 6H_Mp_k"," 7H_Vbv_v"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,null,4,6.5,7.5,8.5,9,13,24,40]
[null,null,13,2.1600000000000001E-2,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 4H_Vhv_v"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,null,4,4.5,6.5,8.5,9,13,24,40]
[null,null,14,5.04E-2,"mv"," 3H_Mp_k"," 4H_Vhv_v"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,null,null,4,6.5,8.5,9,13,24,40]
[null,null,15,5.04E-2,"mv"," 1H_Mp_k"," 2H_Mkw_z&k"," 5H_Vhv_v"," 6H_Mp_k"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,4,4.5,6.5,7.5,8.5,9,13,24,40]
[null,null,16,0.1176,"mv"," 3H_Mp_k"," 5H_Vhv_v"," 6H_Mp_k"," 8H_Mp_k"," 9P_Wdz_zf"," 10P_Rg_zm"," 13P_Mg_zm",null,null,null,4,6.5,7.5,8.5,9,13,24,40]