\input{PackagesAndCommands}

\begin{document}
\begin{Form}
\def\arraystretch{1.2}

%%%%%%%%%%%%%%%%%%%%%%%%%%%
\chapter*{Test Document DAM UI}

\section*{Algemeen}
Dit document beschrijft de test procedure van het programma DAM. 
De tester zal aan de hand van dit document een test uitvoeren. 
De test die beschreven wordt in dit document is een functionele test. 
De inhoudelijke test wordt door middel van verificatie sommen uitgevoerd, 
en wordt in een ander document beschreven.	

\textbf{Let op! De test in dit document moet uitgevoerd worden voor de opties Engels en Nederlands.}			

\section*{Algemene gegevens}

\def\arraystretch{1.5}

\begin{tabular}[t]{ll}
Versie programma:	     & \TextField[name=Versie, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Naam tester:           & \TextField[name=NaamTester, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Datum:                 & \TextField[name=Datum, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Image:                 & \TextField[name=Image, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Platform:              & \TextField[name=Platform, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Decimal:               & \TextField[name=Decimal, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Resolutie:             & \TextField[name=Resolutie, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Kleurenschema:         & \TextField[name=Kleurenschema, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Taal operating system: & \TextField[name=Taal, width=80mm, height=3mm, color=black, bordercolor=black, value={}]{} \\
Printers:              & \TextField[multiline, name=Printers, width=80mm, height=10mm, color=black, bordercolor=black, value={}]{} \\
\end{tabular}

\vspace{15mm}

Opmerkingen tester:

\TextField[multiline, name=OpmerkingenTester, width=\textwidth, height=5cm, color=black, bordercolor=black, value={}]{}

\def\arraystretch{1}

\tableofcontents

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\chapter{DAM -- Installation}

\BeginTable
\multicolumn{3}{l}{\underline{Open DAM zonder de Common files te hebben geinstalleerd.}} \\
\quad Krijg je een correcte foutmelding? & \ChoiceAnswer & \AddComment \\
\EmptyRow
\\
\Instructions{Installeer de common files} \\
\EmptyRow
\underline{Kan het programma correct worden geinstalleerd?} & \ChoiceAnswer & \AddComment \\
\EmptyRow
\\
\Instructions{Open DAM} \\
\EmptyRow
\\
\underline{Wordt een melding getoond over .NET Desktop Runtime?} & \ChoiceAnswer & \AddComment \\
\EmptyRow
\\
\Instructions{Klik op Yes en installeer .NET Desktop Runtime} \\
\Instructions{Deinstalleer de common files} \\
\EmptyRow
\multicolumn{3}{l}{\underline{Open DAM nadat de common files zijn gedeinstalleerd}} \\
\quad Krijg je een correcte foutmelding? & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Werken de volgende knoppen correct?}} \\
\quad Yes & \ChoiceAnswer & \AddComment \\
\quad No & \ChoiceAnswer & \AddComment \\
\quad Abort & \ChoiceAnswer & \AddComment \\
\EmptyRow
\underline{Kom je op de correcte webpagina uit waar je de common files kan} & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\underline{downloaden nadat je op Yes hebt gedrukt?}} \\ 
\EmptyRow
\\
\Instructions{Installeer de common files opnieuw en voeg een licentie toe} \\
\EmptyRow
\underline{Kun je invoerfiles gemaakt met een oude versie openen?} & \ChoiceAnswer & \AddComment \\
\underline{Is de shortcut voor DAM zichtbaar op de desktop en werkt deze?} & \ChoiceAnswer & \AddComment \\
\underline{Wordt het correcte splashscreen getoond bij het opstarten van DAM?} & \ChoiceAnswer & \AddComment \\
\EmptyRow
\\
\multicolumn{3}{l}{\underline{Is de juridische informatie correct op de volgende plekken?}} \\
\quad Setup EULA & \ChoiceAnswer & \AddComment \\
\quad Splash screen & \ChoiceAnswer & \AddComment \\
\quad About box & \ChoiceAnswer & \AddComment \\
\quad Disclaimer dialog & \ChoiceAnswer & \AddComment \\
\EndTable

\chapter{DAM -- Toolbar}

\BeginTable
\underline{Elke knop heeft een hint} & \ChoiceAnswer & \AddComment \\
\EmptyRow
\underline{Werken de in de menu's genoemde accelerator keys?} &  & \AddComment \\
\quad Ctrl+N: New (Nieuw) & \ChoiceAnswer & \AddComment \\
\quad Ctrl+O: Open (Openen) & \ChoiceAnswer & \AddComment \\
\quad Ctrl+S: Save (Opslaan) & \ChoiceAnswer & \AddComment \\
\quad F12: Save as (Opslaan als) & \ChoiceAnswer & \AddComment \\
\quad Alt+F4: Exit (Afsluiten) & \ChoiceAnswer & \AddComment \\
\quad Ctrl+Z: Undo (Ongedaan maken) & \ChoiceAnswer & \AddComment \\
\quad Ctrl+Y: Redo (Opnieuw) & \ChoiceAnswer & \AddComment \\
\quad Delete: Delete (Verwijderen) & \ChoiceAnswer & \AddComment \\
\quad Ctrl+Shift+R: Reset (Herstel) & \ChoiceAnswer & \AddComment \\
\quad F9: Run (Start) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Knoppen-Correcte hint en werking}} \\
\quad New (Nieuw) & \ChoiceAnswer & \AddComment \\
\quad Open (Openen) & \ChoiceAnswer & \AddComment \\
\quad Save (Opslaan) & \ChoiceAnswer & \AddComment \\
\quad Undo (Ongedaan maken) & \ChoiceAnswer & \AddComment \\
\quad Redo (Opnieuw) & \ChoiceAnswer & \AddComment \\
\quad Run (Start) & \ChoiceAnswer & \AddComment \\
\quad Abort (Afbreken) & \ChoiceAnswer & \AddComment \\
\quad Reset (Herstel) & \ChoiceAnswer & \AddComment \\
\quad Calculation type (Berekeningstype) & \ChoiceAnswer & \AddComment \\
\quad Analysis type (Analyse type) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\underline{Programma kan meerdere keren tegelijk worden gestart} & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Werkt de Close-button:}} \\
\quad Wordt het scherm gesloten als er geen wijzigingen zijn aangebracht? & \ChoiceAnswer & \AddComment \\
\quad Verschijnt er een vraag als er iets gewijzigd is? & \ChoiceAnswer & \AddComment \\
\EndTable

\chapter{DAM -- Menubar}

\section{DAM -- File menu (Bestand menu)}

\BeginTable
\multicolumn{3}{l}{\underline{File - New (Bestand - Nieuw)}} \\
\quad Wordt er, bij wijziging van invoer, gevraagd "Save changes"? & \ChoiceAnswer & \AddComment \\
\quad Zijn calculation types Design (Ontwerp) en DamLive Configuration (DamLive Configuratie) aanwezig? & \ChoiceAnswer & \AddComment \\
\quad Kan je Design (Ontwerp) selecteren? & \ChoiceAnswer & \AddComment \\
\quad Kan je DamLive Configuration selecteren? & \ChoiceAnswer & \AddComment \\
\quad Kan je een DAM datasource file (DAM databron bestand) selecteren? & \ChoiceAnswer & \AddComment \\
\quad Wordt er automatisch een DAM project file (DAM project bestand) geselecteerd? & \ChoiceAnswer & \AddComment \\
\quad Is Sensor configuration file (Sensor gegevens bestand) disabled bij een Design calculation? & \ChoiceAnswer & \AddComment \\
\quad Kan je een Sensor configuration file selecteren voor een DamLive Configuration calculation? & \ChoiceAnswer & \AddComment \\
\quad Kan je een dikering (dijkring) selecteren? & \ChoiceAnswer & \AddComment \\
\quad Werkt de Projection (Projectie) knop? & \ChoiceAnswer & \AddComment \\
\quad Accepteert DAM UI stix files als input? & \ChoiceAnswer & \AddComment \\
\quad Accepteert DAM UI sti files \textbf{niet} als input? & \ChoiceAnswer & \AddComment \\
\quad Werkt de Cancel knop? & \ChoiceAnswer & \AddComment \\
\quad Werkt de Ok knop? & \ChoiceAnswer & \AddComment \\
\quad Leest DAM de data in? & \ChoiceAnswer & \AddComment \\
\quad Is de tabvolgorde correct? & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{File - New - Projection (Bestand - Nieuw - Projectie)}} \\
\multicolumn{3}{l}{\quad Projection type:} \\
\quad \quad Kan je kiezen tussen Projected en Geographic? & \ChoiceAnswer & \AddComment \\
\quad \quad Kan je iets selecteren uit de dropdown voor de Major Category? & \ChoiceAnswer & \AddComment \\
\quad \quad Kan je iets selecteren uit de dropdown voor de Minor Category? & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad From EPGS code:} \\
\quad \quad Kan je het nummer aanpassen met de pijltjes knoppen? & \ChoiceAnswer & \AddComment \\
\quad \quad Kan je een nummer intypen? & \ChoiceAnswer & \AddComment \\
\quad \quad Werkt de Find knop? & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad From ESRI or Proj4 string:} \\
\quad \quad Kan je ESRI (otheriwse Proj4) aan- en uitvinken? & \ChoiceAnswer & \AddComment \\
\quad \quad Werkt de Parse knop? & \ChoiceAnswer & \AddComment \\
\quad Werkt de apply knop? & \ChoiceAnswer & \AddComment \\
\quad Werkt de OK knop? & \ChoiceAnswer & \AddComment \\
\quad Werkt de Cancel knop? & \ChoiceAnswer & \AddComment \\
\quad Is de tabvolgorde correct? & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{File – Open (Bestand - Openen)}} \\
\quad Bestand aanklikken & \ChoiceAnswer & \AddComment \\
\quad Naam intypen & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad File type} \\
\quad \quad damx & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Open button:} \\
\quad \quad Vanaf harde schijf & \ChoiceAnswer & \AddComment \\
\quad \quad Vanaf netwerk schijf & \ChoiceAnswer & \AddComment \\
\quad \quad Vanaf read only netwerk schijf & \ChoiceAnswer & \AddComment \\
\quad Cancel & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{File – Save (Bestand - Opslaan)}} \\
\quad Naar harde schijf & \ChoiceAnswer & \AddComment \\
\quad Naar netwerk schijf & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{File – Save As (Bestand - Opslaan als)}} \\
\quad Bestand aanklikken & \ChoiceAnswer & \AddComment \\
\quad Naam intypen & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Save button:} \\
\quad \quad Naar harde schijf & \ChoiceAnswer & \AddComment \\
\quad \quad Naar netwerk schijf & \ChoiceAnswer & \AddComment \\
\quad Cancel & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{File – Export - Surfacelines (Bestand - Exporteren - Ontworpen maaiveldlijnen), beschikbaar bij Design, na gerekend te hebben}} \\
\quad Maken/selecteren uitvoer directory & \ChoiceAnswer & \AddComment \\
\quad Naam intypen voor nieuwe directory & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Ok button:} \\
\quad \quad Naar harde schijf & \ChoiceAnswer & \AddComment \\
\quad \quad Naar netwerk schijf & \ChoiceAnswer & \AddComment \\
\quad \quad Naar readonly netwerk schijf (mag niet lukken) & \ChoiceAnswer & \AddComment \\
\quad Cancel & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{File – Last used project }} \\
\quad Project 1 & \ChoiceAnswer & \AddComment \\
\quad Project 2 & \ChoiceAnswer & \AddComment \\
\quad Project 3 & \ChoiceAnswer & \AddComment \\
\quad Project 4 & \ChoiceAnswer & \AddComment \\
\quad Project 5 & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{File – Exit (Bestand - Afsluiten)}} \\
\quad Wordt er, bij wijziging van invoer, gevraagd “Save changes?” & \ChoiceAnswer & \AddComment \\
\EndTable

\section{DAM -- Edit menu (Bewerken menu)}

\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Undo (Ongedaan maken) & \ChoiceAnswer & \AddComment \\
\quad Redo (Opnieuw) & \ChoiceAnswer & \AddComment \\
\quad Delete (Verwijderen) & \ChoiceAnswer & \AddComment \\
\quad Clear Selection (Wis selectie) & \ChoiceAnswer & \AddComment \\
\EndTable

\section{DAM -- View menu (Beeld menu)}

\BeginTable
\multicolumn{3}{l}{\underline{Opent het juiste tab bij het klikken van de volgende opties?}} \\
\quad Reset (Herstel) & \ChoiceAnswer & \AddComment \\
\quad Cross section (Dwarsdoorsnede) & \ChoiceAnswer & \AddComment \\
\quad Image (Afbeelding) & \ChoiceAnswer & \AddComment \\
\quad Map (Kaart) & \ChoiceAnswer & \AddComment \\
\quad Navigator & \ChoiceAnswer & \AddComment \\
\quad Properties (Eigenschappen) & \ChoiceAnswer & \AddComment \\
\quad Validation messages (Validatie) & \ChoiceAnswer & \AddComment \\
\quad Log & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Voor een Design calculation:} \\
\quad \quad Tables (Materials + Locations + Design Calculations) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Voor een DamLive Configuration calculation:} \\
\quad \quad Tables (Materials + Locations + Sensor configuration + Sensor group configuration + Sensor location data) & \ChoiceAnswer & \AddComment \\
\EndTable

\section{DAM -- Calculation menu (Berekening menu)}

\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Run (Start) & \ChoiceAnswer & \AddComment \\
\quad Abort (Afbreken) & \ChoiceAnswer & \AddComment \\
\quad Clear results (Verwijder resultaten) & \ChoiceAnswer & \AddComment \\
\quad Options (Opties) & \ChoiceAnswer & \AddComment \\
\EndTable

\section{DAM -- Tools menu (Gereedschap menu)}

\BeginTable
\multicolumn{3}{l}{\underline{Options–General (Opties-Algemeen): Kun je iets selecteren bij:}} \\
\quad Start up - Initial project (Opstarten - Start-project) & \ChoiceAnswer & \AddComment \\
\quad Language - Language (Taal - taal) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Multi Core - Number of cores (Gebruik Processoren - Aantal processoren)} \\
\quad \quad Min: 1 & \ChoiceAnswer & \AddComment \\
\quad \quad Max: aanwezig aantal cpu's & \ChoiceAnswer & \AddComment \\
\quad Is de tabvolgorde correct? & \ChoiceAnswer & \AddComment \\
\quad Werkt de OK knop? & \ChoiceAnswer & \AddComment \\
\quad Werkt de Cancel knop? & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Options-Units (Opties-Eenheden): Kun je iets selecteren bij:}} \\
\quad Numbers - Fraction (Getallen - Fracties) & \ChoiceAnswer & \AddComment \\
\quad Geometry - Length (Geometrie - Lengte) & \ChoiceAnswer & \AddComment \\
\quad Geometry - Tiny length (Geometrie - Kleine lengte) & \ChoiceAnswer & \AddComment \\
\quad Geometry - Angle (Geometrie - Hoek) & \ChoiceAnswer & \AddComment \\
\quad Weight and forces - Weight (Gewicht en krachten - (Volumiek) gewicht) & \ChoiceAnswer & \AddComment \\
\quad Weight and forces - Pressure per length (Gewicht en krachten - Druk per lengte) & \ChoiceAnswer & \AddComment \\
\quad Weight and forces - Pressure (Gewicht en krachten - Druk) & \ChoiceAnswer & \AddComment \\
\quad Discharges - Permeability (Afvoer - Doorlatendheid) & \ChoiceAnswer & \AddComment \\
\quad Is de tabvolgorde correct? & \ChoiceAnswer & \AddComment \\
\quad Werkt de OK knop? & \ChoiceAnswer & \AddComment \\
\quad Werkt de Cancel knop? & \ChoiceAnswer & \AddComment \\
\EmptyRow
\underline{Units (Eenheden) (zie Options - Units): wordt de juiste tab getoond?} & \ChoiceAnswer & \AddComment \\
\EndTable

\section{DAM -- Help menu}

\BeginTable
\underline{Manual (Gebruikershandleiding) - Word je doorverwezen naar de juiste pagina?} & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{About (Info) – Werken de volgende knoppen:}} \\
\quad Disclaimer & \ChoiceAnswer & \AddComment \\
\quad Ok & \ChoiceAnswer & \AddComment \\
\quad Cancel (Annuleren) & \ChoiceAnswer & \AddComment \\
\quad Is de tabvolgorde correct? & \ChoiceAnswer & \AddComment \\
\EndTable

\chapter{DAM -- Navigator}

\BeginTable
\multicolumn{3}{l}{\underline{Rechtermuisknop voor geselecteerde locaties:}} \\
\quad \quad Show item in map & \ChoiceAnswer & \AddComment \\
\EmptyRow
\quad Is het mogelijk om de checkboxen in de "Run" ("Berekening") tab te selecteren en deselecteren? & \ChoiceAnswer & \AddComment \\
\quad Is het mogelijk om items in en uit te klappen? & \ChoiceAnswer & \AddComment \\
\quad Wordt de informatie in het Properties (Eigenschappen) venster gesynchroniseerd als je op een locatie klikt? & \ChoiceAnswer & \AddComment \\
\Instructions{Klik met de rechtermuisknop op de headers Name en Run (Naam en Berekening)} \\
\multicolumn{3}{l}{\underline{Werken de volgende opties?}} \\
\quad Column Chooser & \ChoiceAnswer & \AddComment \\
\quad Best Fit & \ChoiceAnswer & \AddComment \\
\quad Best Fit (All columns) & \ChoiceAnswer & \AddComment \\
\quad Layout & \ChoiceAnswer & \AddComment \\
\EndTable

\chapter{DAM -- Map (Kaart)}

\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Selection (Selectie) & \ChoiceAnswer & \AddComment \\
\quad Zoom to extents (Zoom naar alle kaartlagen) & \ChoiceAnswer & \AddComment \\
\quad Zoom to data (Zoom naar gegevens) & \ChoiceAnswer & \AddComment \\
\quad Zoom to (Zoom tot geselecteerde data op de kaart) & \ChoiceAnswer & \AddComment \\
\quad Zoom rectangle (Zoom naar rechthoek) & \ChoiceAnswer & \AddComment \\
\quad Show legend (Toon legenda) & \ChoiceAnswer & \AddComment \\
\quad Open layer from file (Openen laag van bestand) & \ChoiceAnswer & \AddComment \\
\quad Export layers (Exporteer kaartlagen) & \ChoiceAnswer & \AddComment \\
\quad Save map (Slaat de kaart zoals nu zichtbaar als afbeelding op) & \ChoiceAnswer & \AddComment \\
\quad Select web layer (Selecteer achtergrondkaart) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Hebben de volgende knoppen een correcte hint als je eroverheen hovert?}} \\
\quad Selection (Selectie) & \ChoiceAnswer & \AddComment \\
\quad Zoom to extents (Zoom naar alle kaartlagen) & \ChoiceAnswer & \AddComment \\
\quad Zoom to data (Zoom naar gegevens) & \ChoiceAnswer & \AddComment \\
\quad Zoom to (Zoom tot geselecteerde data op de kaart) & \ChoiceAnswer & \AddComment \\
\quad Zoom rectangle (Zoom naar rechthoek) & \ChoiceAnswer & \AddComment \\
\quad Show legend (Toon legenda) & \ChoiceAnswer & \AddComment \\
\quad Open layer from file (Openen laag van bestand) & \ChoiceAnswer & \AddComment \\
\quad Export layers (Exporteer kaartlagen) & \ChoiceAnswer & \AddComment \\
\quad Save map (Slaat de kaart zoals nu zichtbaar als afbeelding op) & \ChoiceAnswer & \AddComment \\
\quad Select web layer (Selecteer achtergrondkaart) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Rechtermuisknop - Show legend (Toon legenda) & \ChoiceAnswer & \AddComment \\
\quad Rechtermuisknop - Clear selection (Wis selectie) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\underline{Map - Legend (Kaart - Legenda)}} \\
\quad Is het mogelijk om items in en uit te klappen? & \ChoiceAnswer & \AddComment \\
\quad Is het mogelijk om items aan en uit te vinken? & \ChoiceAnswer & \AddComment \\
\EndTable

\chapter{DAM -- Cross section (Dwarsdoorsnede)}

\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Selection (Selectie) & \ChoiceAnswer & \AddComment \\
\quad Pan (Verschuif) & \ChoiceAnswer & \AddComment \\
\quad Zoom to extents (Zoom naar limieten en behoud aspect ratio) & \ChoiceAnswer & \AddComment \\
\quad Zooms to extents and reset aspect ratio (Zoom naar limieten en herstel aspect ratio) & \ChoiceAnswer & \AddComment \\
\quad Zooms by rectangle (Zoom per rechthoek) & \ChoiceAnswer & \AddComment \\
\quad Options (Opties) & \ChoiceAnswer & \AddComment \\
\quad Dropdown menu met de volgende opties: & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad \quad Stability inside (Binnenwaartse stabiliteit)} \\
\multicolumn{3}{l}{\quad \quad Stability outside (Buitenwaartse stabiliteit)} \\
\multicolumn{3}{l}{\quad \quad Piping} \\
\quad Profile name (wordt getoond) & \ChoiceAnswer & \AddComment \\
\quad Previous soil profile & \ChoiceAnswer & \AddComment \\
\quad Next soil profile & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Hebben de volgende knoppen een correcte hint als je eroverheen hovert?}} \\
\quad Selection (Selectie) & \ChoiceAnswer & \AddComment \\
\quad Pan (Verschuif) & \ChoiceAnswer & \AddComment \\
\quad Zoom to extents (Zoom naar limieten en behoud aspect ratio) & \ChoiceAnswer & \AddComment \\
\quad Zooms to extents and reset aspect ratio (Zoom naar limieten en herstel aspect ratio) & \ChoiceAnswer & \AddComment \\
\quad Zooms by rectangle (Zoom per rechthoek) & \ChoiceAnswer & \AddComment \\
\quad Options (Opties) & \ChoiceAnswer & \AddComment \\
\quad Previous soil profile & \ChoiceAnswer & \AddComment \\
\quad Next soil profile & \ChoiceAnswer & \AddComment \\
\quad Percentage & \ChoiceAnswer & \AddComment \\
\EmptyRow
\Instructions{Klik op Options (Opties)} \\
\multicolumn{3}{l}{\underline{Editor options (Editor opties) - Kun je iets aanvinken bij:}} \\
\quad Checkbox Visible (Zichtbaar) & \ChoiceAnswer & \AddComment \\
\quad Checkbox Label visible (Label zichtbaar) & \ChoiceAnswer & \AddComment \\
\quad Show grid (Toon raster) & \ChoiceAnswer & \AddComment \\
\quad Snap to grid (Uitlijnen op raster) & \ChoiceAnswer & \AddComment \\
\quad Snap to angle (Uitlijnen op hoek) & \ChoiceAnswer & \AddComment \\
\quad Snap grid distance (Uitlijn raster afstand) & \ChoiceAnswer & \AddComment \\
\EndTable

\chapter{DAM - Input}

\section{DAM -- Stability Modulus}
\subsection{DAM -- Properties -- Location Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Identification (Identificatie) - Is het volgende aanwezig en disabled?}} \\
\quad Dike (Kering) & \ChoiceAnswer & \AddComment \\
\quad Name (Naam) & \ChoiceAnswer & \AddComment \\
\quad X location (X (RD)) & \ChoiceAnswer & \AddComment \\
\quad Y location (Y (RD)) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Load (Belasting) - Kun je iets invullen bij: }} \\
\quad Traffic load (Verkeersbelasting) & \ChoiceAnswer & \AddComment \\
\quad Degree of consolidation (Consolidatiegraad) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Calculation (Berekening) - Kun je iets invullen bij:}} \\
\multicolumn{3}{l}{\quad PL-Line creation (Generatie WSP):} \\
\quad \quad Expert Knowledge (Expert kennis) & \ChoiceAnswer & \AddComment \\
\quad \quad Expert knowledge linear in dike (Expertkennis (lineair in dijk)) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Zone type (Zonerings type):} \\
\quad \quad No zones (Geen zones) & \ChoiceAnswer & \AddComment \\
\quad \quad Forbidden zones (Verboden zone) & \ChoiceAnswer & \AddComment \\
\quad Minimum circle depth (Minimale cirkel diepte) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Design (Ontwerp) - Kun je iets invullen bij:}} \\
\quad Dike emb. Material (Ophoogmateriaal dijk) & \ChoiceAnswer & \AddComment \\
\quad Shoulder emb. Material (Ophoogmateriaal berm) & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth slope (Berm ontwikkelings ratio) & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth delta X (Berm stap grootte) & \ChoiceAnswer & \AddComment \\
\quad Slope adaption delta X (Talud stapgrootte) & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Properties -- Location scenarios Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\multicolumn{3}{l}{\quad Filter columns (Filter kolommen)} \\
\quad \quad All (Alles) & \ChoiceAnswer & \AddComment \\
\quad \quad Inside stability (Binnenstabiliteit) & \ChoiceAnswer & \AddComment \\
\quad \quad Piping & \ChoiceAnswer & \AddComment \\
\quad \quad PL line schematization (PL line schematisatie) & \ChoiceAnswer & \AddComment \\
\quad Copy (Kopiëren) & \ChoiceAnswer & \AddComment \\
\quad Paste (Plakken) & \ChoiceAnswer & \AddComment \\
\quad Fits columns (Aanpassen) & \ChoiceAnswer & \AddComment \\
\quad Edit (Wijzig) & \ChoiceAnswer & \AddComment \\
\quad Edit unit (Wijzig eenheid) & \ChoiceAnswer & \AddComment \\
\quad Export (Tabel Exporteren) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Hebben de volgende knoppen een correcte hint als je eroverheen hovert?}} \\
\quad Filter columns (Filter kolommen) & \ChoiceAnswer & \AddComment \\
\quad Copy (Kopiëren) & \ChoiceAnswer & \AddComment \\
\quad Paste (Plakken) & \ChoiceAnswer & \AddComment \\
\quad Fits columns (Aanpassen) & \ChoiceAnswer & \AddComment \\
\quad Edit (Wijzig) & \ChoiceAnswer & \AddComment \\
\quad Edit unit (Wijzig eenheid) & \ChoiceAnswer & \AddComment \\
\quad Export (Tabel Exporteren) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Kun je iets invullen bij de volgende kolommen:}} \\
\quad River level (Buitenwaterstand) & \ChoiceAnswer & \AddComment \\
\quad River level low (Lage buitenwaterstand) & \ChoiceAnswer & \AddComment \\
\quad Dike table height (DTH) & \ChoiceAnswer & \AddComment \\
\quad Polder level (Polderpeil) & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion piping (Criterium opdrijven bij piping) & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion stability (Criterium opdrijven bij stabiliteit) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (river) (PL1-buitenkruin offset) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (polder) (PL1-binnenkruin offset) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder base (polder) (PL1-Insteek binnenberm offset) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below toe of dike (polder) (PL1-binnenteen offset) & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset below middle of dike crest (Gebruik PL1-kruin midden offset) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below middle of dike crest (PL1-kruin midden offset) & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset factor below shoulder crest inside (Gebruik PL1-offset factor kruin binnenberm) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder crest inside (PL1-offset kruin binnenberm) & \ChoiceAnswer & \AddComment \\
\quad Head PL2 (Stijghoogte PL2) & \ChoiceAnswer & \AddComment \\
\quad Head PL3 (Stijghoogte PL3) & \ChoiceAnswer & \AddComment \\
\quad Head PL4 (Stijghoogte PL4) & \ChoiceAnswer & \AddComment \\
\quad Required safety factor stability inner slope (Vereiste veiligheidsfactor binnenwaartse stabiliteit) & \ChoiceAnswer & \AddComment \\
\quad Required safety factor stability outer slope (Vereiste veiligheidsfactor buitenwaartse stabiliteit) & \ChoiceAnswer & \AddComment \\
\quad Required safety factor piping (Vereiste veiligheidsfactor piping) & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Properties -- Surface line Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad \quad Copy (Kopiëren) & \ChoiceAnswer & \AddComment \\
\quad \quad Fits columns (Aanpassen) & \ChoiceAnswer & \AddComment \\
\quad \quad Edit unit (Wijzig eenheid) & \ChoiceAnswer & \AddComment \\
\quad \quad Export (Tabel Exporteren) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\underline{Hebben de volgende knoppen een correcte hint als je eroverheen hovert?}} \\
\quad \quad Copy (Kopiëren) & \ChoiceAnswer & \AddComment \\
\quad \quad Fits columns (Aanpassen) & \ChoiceAnswer & \AddComment \\
\quad \quad Edit unit (Wijzig eenheid) & \ChoiceAnswer & \AddComment \\
\quad \quad Export (Exporteren) & \ChoiceAnswer & \AddComment \\
\quad Zijn de X en Z waardes disabled? & \ChoiceAnswer & \AddComment \\
\quad Kan je iets anders selecteren voor de Characteristic points (Karakteristiek punt)? & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Properties -- Calculation Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Input (Invoer)}} \\
\multicolumn{3}{l}{\quad Zijn de volgende opties aanwezig en disabled?} \\
\quad \quad Location (Locatie) & \ChoiceAnswer & \AddComment \\
\quad \quad Profile Name (Profielnaam) & \ChoiceAnswer & \AddComment \\
\quad \quad Stability Model (Stabiliteitsmodel) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Kun je iets invullen bij:} \\
\quad \quad Scenario Name (Scenarionaam) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Results (Resultaten)}} \\
\multicolumn{3}{l}{\quad Zijn de volgende opties aanwezig en disabled?} \\
\quad \quad Safety factor (Stabiliteitsfactor) & \ChoiceAnswer & \AddComment \\
\quad \quad Calculation result (Berekenings resultaat) & \ChoiceAnswer & \AddComment \\
\quad \quad Number of Iterations (Aantal iteraties) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Evaluation (Evaluatie)}} \\
\multicolumn{3}{l}{\quad Kun je het volgende selecteren?} \\
\quad \quad Accepted (Goedgekeurd) & \ChoiceAnswer & \AddComment \\
\quad \quad Rejected (Afgekeurd) & \ChoiceAnswer & \AddComment \\
\quad \quad Not evaluated (Niet getoetst) & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Werkt de volgende knop?} \\
\quad \quad Open calculation & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Kun je iets invullen bij:} \\
\quad \quad Notes (Opmerkingen) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\EndTable

\subsection{DAM -- Tables -- Materials Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Add (Toevoegen) & \ChoiceAnswer & \AddComment \\
\quad Delete (Verwijderen) & \ChoiceAnswer & \AddComment \\
\quad Copy (Kopiëren) & \ChoiceAnswer & \AddComment \\
\quad Paste (Plakken) & \ChoiceAnswer & \AddComment \\
\quad Fits columns (Aanpassen) & \ChoiceAnswer & \AddComment \\
\quad Edit (Wijzig) & \ChoiceAnswer & \AddComment \\
\quad Edit Unit (Wijzig eenheid) & \ChoiceAnswer & \AddComment \\
\quad Export (Tabel Exporteren) & \ChoiceAnswer & \AddComment \\
\quad Item selection & \ChoiceAnswer & \AddComment \\
\quad \quad All (Alles) & \ChoiceAnswer & \AddComment \\
\quad \quad Macrostability (Macrostabiliteit) & \ChoiceAnswer & \AddComment \\
\quad \quad Piping & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij All?}} \\
\quad Name (Naam) & \ChoiceAnswer & \AddComment \\
\quad Color (Kleur) & \ChoiceAnswer & \AddComment \\
\quad Soil type (Type ondergrond) & \ChoiceAnswer & \AddComment \\
\quad Saturated unit weight (Verzadigd gewicht) & \ChoiceAnswer & \AddComment \\
\quad Unsaturated unit weight (Onverzadigd gewicht) & \ChoiceAnswer & \AddComment \\
\quad Cohesion (Cohesie) & \ChoiceAnswer & \AddComment \\
\quad Friction angle (Wrijvingshoek) & \ChoiceAnswer & \AddComment \\
\quad Diameter D70 (D70) & \ChoiceAnswer & \AddComment \\
\quad Permeability X (Doorlatendheid) & \ChoiceAnswer & \AddComment \\
\quad Shear strength model (Schuifsterkte model) & \ChoiceAnswer & \AddComment \\
\quad Sigma-Tau table name & \ChoiceAnswer & \AddComment \\
\quad Strength increase exp (Sterkte toename exp) & \ChoiceAnswer & \AddComment \\
\quad Ratio Su/Pc (Schuifsterkte ratio S) & \ChoiceAnswer & \AddComment \\
\quad POP & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Macrostability (Macrostabiliteit)?}} \\
\quad Name (Naam) & \ChoiceAnswer & \AddComment \\
\quad Color (Kleur) & \ChoiceAnswer & \AddComment \\
\quad Soil type (Type ondergrond) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Piping?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Color & \ChoiceAnswer & \AddComment \\
\quad Soil type & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Item selection: All - Kun je iets invullen bij de volgende kolommen?}} \\
\quad Name (Naam) & \ChoiceAnswer & \AddComment \\
\quad Color (Kleur) & \ChoiceAnswer & \AddComment \\
\quad Soil type (Type ondergrond) & \ChoiceAnswer & \AddComment \\
\quad \quad Sand (Zand) & \ChoiceAnswer & \AddComment \\
\quad \quad Peat (Veen) & \ChoiceAnswer & \AddComment \\
\quad \quad Loam (Leem) & \ChoiceAnswer & \AddComment \\
\quad \quad Clay (Klei) & \ChoiceAnswer & \AddComment \\
\quad \quad Gravel (Grind) & \ChoiceAnswer & \AddComment \\
\quad Saturated unit weight (Verzadigd gewicht) & \ChoiceAnswer & \AddComment \\
\quad Unsaturated unit weight (Onverzadigd gewicht) & \ChoiceAnswer & \AddComment \\
\quad Cohesion (Cohesie) & \ChoiceAnswer & \AddComment \\
\quad Friction angle (Wrijvingshoek) & \ChoiceAnswer & \AddComment \\
\quad Diameter D70 (D70) & \ChoiceAnswer & \AddComment \\
\quad Permeability X (Doorlatendheid) & \ChoiceAnswer & \AddComment \\
\quad Shear strength model (Schuifsterkte model) & \ChoiceAnswer & \AddComment \\
\quad \quad Mohr-Coulomb & \ChoiceAnswer & \AddComment \\
\quad \quad SHANSEP & \ChoiceAnswer & \AddComment \\
\quad \quad Sigma-Tau table & \ChoiceAnswer & \AddComment \\
\quad POP & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Tables -- Locations Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Copy & \ChoiceAnswer & \AddComment \\
\quad Paste & \ChoiceAnswer & \AddComment \\
\quad Fits columns & \ChoiceAnswer & \AddComment \\
\quad Edit & \ChoiceAnswer & \AddComment \\
\quad Edit unit & \ChoiceAnswer & \AddComment \\
\quad Export & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Item selection} \\
\quad \quad All & \ChoiceAnswer & \AddComment \\
\quad \quad Main items & \ChoiceAnswer & \AddComment \\
\quad \quad Dike & \ChoiceAnswer & \AddComment \\
\quad \quad Water levels & \ChoiceAnswer & \AddComment \\
\quad \quad Design & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Main items?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad X location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Y location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Zone type & \ChoiceAnswer & \AddComment \\
\quad Forbidden Zone Factor [-] & \ChoiceAnswer & \AddComment \\
\quad Dike emb. material & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Dike?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Segment & \ChoiceAnswer & \AddComment \\
\quad Description & \ChoiceAnswer & \AddComment \\
\quad Traffic load [kN/m³] & \ChoiceAnswer & \AddComment \\
\quad Degree of consolidation [\%] & \ChoiceAnswer & \AddComment \\
\quad Dike & \ChoiceAnswer & \AddComment \\
\quad Minimum circle depth [m] & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Water levels?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL3 [-] & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL4 [-] & \ChoiceAnswer & \AddComment \\
\quad Penetration length [m] & \ChoiceAnswer & \AddComment \\
\quad Slope damping factor & \ChoiceAnswer & \AddComment \\
\quad PL-Line creation [-] & \ChoiceAnswer & \AddComment \\
\quad Intrusion vertical water pressure & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Design?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Shoulder emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth slope [-] & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Slope adaption delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Redesign dike height & \ChoiceAnswer & \AddComment \\
\quad Redesign dike shoulder & \ChoiceAnswer & \AddComment \\
\quad Stability design method & \ChoiceAnswer & \AddComment \\
\quad Start value for design of slope & \ChoiceAnswer & \AddComment \\
\quad End value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Step value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Use new width crest & \ChoiceAnswer & \AddComment \\
\quad New width crest & \ChoiceAnswer & \AddComment \\
\quad Use new slope inside & \ChoiceAnswer & \AddComment \\
\quad New slope inside & \ChoiceAnswer & \AddComment \\
\quad Use new slope outside & \ChoiceAnswer & \AddComment \\
\quad New slope outside & \ChoiceAnswer & \AddComment \\
\quad Use new top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use the value for new allowed height of shoulder as fraction of dike height & \ChoiceAnswer & \AddComment \\
\quad New allowed height shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad New allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad Use new definition ditch & \ChoiceAnswer & \AddComment \\
\quad New width ditch bottom & \ChoiceAnswer & \AddComment \\
\quad New slope ditch & \ChoiceAnswer & \AddComment \\
\quad New depth ditch & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Item selection: All - Name -Kun je iets invullen bij de volgende kolommen?}} \\
\quad River Level & \ChoiceAnswer & \AddComment \\
\quad River level low & \ChoiceAnswer & \AddComment \\
\quad Dike table height & \ChoiceAnswer & \AddComment \\
\quad Polder level & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion piping & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion stability & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (river) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (polder) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder base (polder) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below toe of dike (polder) & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset below middle of dike crest & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below middle of dike crest & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset factor below shoulder crest inside & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder crest inside & \ChoiceAnswer & \AddComment \\
\quad Head PL2 & \ChoiceAnswer & \AddComment \\
\quad Head PL3 & \ChoiceAnswer & \AddComment \\
\quad Head PL4 & \ChoiceAnswer & \AddComment \\
\quad Required safety factor stability inner slope & \ChoiceAnswer & \AddComment \\
\quad Required safety factor outer slope & \ChoiceAnswer & \AddComment \\
\quad Required safety factor piping & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Item selection: All - Kun je iets invullen bij de volgende kolommen:}} \\
\quad Y location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad X location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Segment & \ChoiceAnswer & \AddComment \\
\quad Description & \ChoiceAnswer & \AddComment \\
\quad Traffic load [kN/m³] & \ChoiceAnswer & \AddComment \\
\quad Degree of consolidation [\%] & \ChoiceAnswer & \AddComment \\
\quad Dike & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL3 [-] & \ChoiceAnswer & \AddComment \\
\quad Distance to Entrypoint [m] & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL4 [-] & \ChoiceAnswer & \AddComment \\
\quad Penetration length [m] & \ChoiceAnswer & \AddComment \\
\quad Slope damping factor & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad PL-Line creation [-]} \\
\quad \quad Expert Knowledge & \ChoiceAnswer & \AddComment \\
\quad \quad Expert knowledge linear in dike & \ChoiceAnswer & \AddComment \\
\quad Minimum circle depth [m] & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Zone type} \\
\quad \quad No zones & \ChoiceAnswer & \AddComment \\
\quad \quad Forbidden zones & \ChoiceAnswer & \AddComment \\
\quad Forbidden zone factor [-] & \ChoiceAnswer & \AddComment \\
\quad Dike emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth slope [-] & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Slope adaption delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Redesign dike height & \ChoiceAnswer & \AddComment \\
\quad Redesign dike shoulder & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Stability design method} \\
\quad \quad Optimized slope and shoulder adaption & \ChoiceAnswer & \AddComment \\
\quad \quad Slope adaption before shoulder adaption & \ChoiceAnswer & \AddComment \\
\quad Start value for design of slope & \ChoiceAnswer & \AddComment \\
\quad End value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Step value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Use new width crest & \ChoiceAnswer & \AddComment \\
\quad New width crest & \ChoiceAnswer & \AddComment \\
\quad Use new slope inside & \ChoiceAnswer & \AddComment \\
\quad New slope inside & \ChoiceAnswer & \AddComment \\
\quad Use new slope outside & \ChoiceAnswer & \AddComment \\
\quad New slope outside & \ChoiceAnswer & \AddComment \\
\quad Use new top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use the value for new allowed height of shoulder as fraction of dike height & \ChoiceAnswer & \AddComment \\
\quad New allowed height shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad New allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad Use new definition ditch & \ChoiceAnswer & \AddComment \\
\quad New width ditch bottom & \ChoiceAnswer & \AddComment \\
\quad New slope ditch & \ChoiceAnswer & \AddComment \\
\quad New depth ditch & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Intrusion vertical water pressure} \\
\quad \quad DAM Standard & \ChoiceAnswer & \AddComment \\
\quad \quad Linear & \ChoiceAnswer & \AddComment \\
\quad \quad Full hydrostatic & \ChoiceAnswer & \AddComment \\
\quad \quad Hydrostatic & \ChoiceAnswer & \AddComment \\
\quad \quad Semi time dependent & \ChoiceAnswer & \AddComment \\
\quad Surface line & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Validation messages Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen?}} \\
\quad Severity & \ChoiceAnswer & \AddComment \\
\quad Message & \ChoiceAnswer & \AddComment \\
\quad Subject & \ChoiceAnswer & \AddComment \\
\quad Repair & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Log Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen?}} \\
\quad Message & \ChoiceAnswer & \AddComment \\
\quad Subject & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{Analysis type}
\BeginTable
\Instructions{Open de tutorial en selecteer Adapt geometry voor Analysis type.} \\
\quad Is de aangepaste geometrie hetzelfde als in release 19.1.2? & \ChoiceAnswer & \AddComment \\
\EndTable

\section{DAM -- Piping Modulus}
\subsection{DAM -- Properties -- Location Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Klopt de volgende informatie: }} \\
\quad Dike & \ChoiceAnswer & \AddComment \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad X location (RDS) & \ChoiceAnswer & \AddComment \\
\quad Y location (RDS) & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Load - Kun je iets invullen bij: }} \\
\quad Traffic load & \ChoiceAnswer & \AddComment \\
\quad Degree of consolidation & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Calculation - Kun je iets invullen bij:}} \\
\multicolumn{3}{l}{\quad PL-Line creation:} \\
\quad \quad Expert Knowledge & \ChoiceAnswer & \AddComment \\
\quad \quad Expert knowledge linear in dike & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Zone type:} \\
\quad \quad No zones & \ChoiceAnswer & \AddComment \\
\quad \quad Forbidden zones & \ChoiceAnswer & \AddComment \\
\quad Minimum circle depth & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Design - Kun je iets invullen bij:}} \\
\quad Dike emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth slope & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth delta X & \ChoiceAnswer & \AddComment \\
\quad Slope adaption delta X & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Properties -- Location scenarios Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\multicolumn{3}{l}{\quad Filter columns} \\
\quad \quad All & \ChoiceAnswer & \AddComment \\
\quad \quad Inside stability & \ChoiceAnswer & \AddComment \\
\quad \quad Piping & \ChoiceAnswer & \AddComment \\
\quad \quad PL line schematization & \ChoiceAnswer & \AddComment \\
\quad Copy & \ChoiceAnswer & \AddComment \\
\quad Paste & \ChoiceAnswer & \AddComment \\
\quad Fits columns & \ChoiceAnswer & \AddComment \\
\quad Edit & \ChoiceAnswer & \AddComment \\
\quad Edit unit & \ChoiceAnswer & \AddComment \\
\quad Export & \ChoiceAnswer & \AddComment \\
\EmptyRow
\EmptyRow
\multicolumn{3}{l}{\underline{Zijn de volgende kolommen aanwezig:}} \\
\quad ID Location Scenario & \ChoiceAnswer & \AddComment \\
\quad River level [m] & \ChoiceAnswer & \AddComment \\
\quad River level low [m] & \ChoiceAnswer & \AddComment \\
\quad Dike table height [m] & \ChoiceAnswer & \AddComment \\
\quad Polder level [m] & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion piping & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion stability & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (river) [m] & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (polder) [m] & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder base (polder) [m] & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below toe of dike (polder) [m] & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset below middle of dike crest [-] & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below middle of dike crest [m] & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset factor below shoulder crest inside [-] & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder crest inside [÷] & \ChoiceAnswer & \AddComment \\
\quad Head PL2 [m] & \ChoiceAnswer & \AddComment \\
\quad Head PL3 [m] & \ChoiceAnswer & \AddComment \\
\quad Head PL4 [m] & \ChoiceAnswer & \AddComment \\
\quad Required safety factor stability inner slope & \ChoiceAnswer & \AddComment \\
\quad Required safety factor stability outer slope & \ChoiceAnswer & \AddComment \\
\quad Required safety factor piping & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Properties -- Surface line Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Copy & \ChoiceAnswer & \AddComment \\
\quad Fits columns & \ChoiceAnswer & \AddComment \\
\quad Edit Unit & \ChoiceAnswer & \AddComment \\
\quad Export & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Characteristic point - Kun je kiezen uit de volgende opties?}} \\
\quad Surface level outside  & \ChoiceAnswer & \AddComment \\
\quad Dike toe at river & \ChoiceAnswer & \AddComment \\
\quad Shoulder crest outside & \ChoiceAnswer & \AddComment \\
\quad Shoulder base outside & \ChoiceAnswer & \AddComment \\
\quad Dike crest at river & \ChoiceAnswer & \AddComment \\
\quad Traffic load outside & \ChoiceAnswer & \AddComment \\
\quad Traffic load inside & \ChoiceAnswer & \AddComment \\
\quad Dike crest at polder & \ChoiceAnswer & \AddComment \\
\quad Shoulder base inside & \ChoiceAnswer & \AddComment \\
\quad Shoulder crest inside & \ChoiceAnswer & \AddComment \\
\quad Dike toe at polder & \ChoiceAnswer & \AddComment \\
\quad Ditch dike side & \ChoiceAnswer & \AddComment \\
\quad Bottom ditch dike side & \ChoiceAnswer & \AddComment \\
\quad Bottom ditch polder side & \ChoiceAnswer & \AddComment \\
\quad Ditch polder side & \ChoiceAnswer & \AddComment \\
\quad Surface level inside & \ChoiceAnswer & \AddComment \\
\quad None & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Properties -- Calculation Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Input}} \\
\multicolumn{3}{l}{\quad Zijn de volgende opties aanwezig en disabled?} \\
\quad \quad Location & \ChoiceAnswer & \AddComment \\
\quad \quad Profile name & \ChoiceAnswer & \AddComment \\
\quad \quad Stability model & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Input - Kun je iets invullen bij: }} \\
\quad Scenario Name & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Results}} \\
\multicolumn{3}{l}{\quad Zijn de volgende opties aanwezig en disabled?} \\
\quad \quad Safety factor & \ChoiceAnswer & \AddComment \\
\quad \quad Calculation result & \ChoiceAnswer & \AddComment \\
\quad \quad Number of iterations & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Evaluation - Kun je het volgende selecteren:}} \\
\quad Accepted & \ChoiceAnswer & \AddComment \\
\quad Rejected & \ChoiceAnswer & \AddComment \\
\quad Not evaluated & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Evaluation - Kun je iets invullen bij }} \\
\quad Notes & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Tables -- Materials Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Add & \ChoiceAnswer & \AddComment \\
\quad Delete & \ChoiceAnswer & \AddComment \\
\quad Copy & \ChoiceAnswer & \AddComment \\
\quad Paste & \ChoiceAnswer & \AddComment \\
\quad Fits columns & \ChoiceAnswer & \AddComment \\
\quad Edit & \ChoiceAnswer & \AddComment \\
\quad Edit Unit & \ChoiceAnswer & \AddComment \\
\quad Export & \ChoiceAnswer & \AddComment \\
\quad Item selection & \ChoiceAnswer & \AddComment \\
\quad \quad All & \ChoiceAnswer & \AddComment \\
\quad \quad Macrostability & \ChoiceAnswer & \AddComment \\
\quad \quad Piping & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij All?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Color & \ChoiceAnswer & \AddComment \\
\quad Soil type & \ChoiceAnswer & \AddComment \\
\quad Saturated unit weight & \ChoiceAnswer & \AddComment \\
\quad Unsaturated unit weight & \ChoiceAnswer & \AddComment \\
\quad Cohesion & \ChoiceAnswer & \AddComment \\
\quad Friction angle & \ChoiceAnswer & \AddComment \\
\quad Diameter D70 & \ChoiceAnswer & \AddComment \\
\quad Permeability X & \ChoiceAnswer & \AddComment \\
\quad Shear strength model & \ChoiceAnswer & \AddComment \\
\quad Strength increase exp & \ChoiceAnswer & \AddComment \\
\quad Ratio Su/Pc & \ChoiceAnswer & \AddComment \\
\quad POP & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Macrostability?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Color & \ChoiceAnswer & \AddComment \\
\quad Soil type & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Piping?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Color & \ChoiceAnswer & \AddComment \\
\quad Soil type & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Item selection - All: Kun je iets invullen bij de volgende kolommen?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Color & \ChoiceAnswer & \AddComment \\
\quad Soil type & \ChoiceAnswer & \AddComment \\
\quad \quad Sand & \ChoiceAnswer & \AddComment \\
\quad \quad Peat & \ChoiceAnswer & \AddComment \\
\quad \quad Loam & \ChoiceAnswer & \AddComment \\
\quad \quad Clay & \ChoiceAnswer & \AddComment \\
\quad \quad Gravel & \ChoiceAnswer & \AddComment \\
\quad Saturated unit weight & \ChoiceAnswer & \AddComment \\
\quad Unsaturated unit weight & \ChoiceAnswer & \AddComment \\
\quad Cohesion & \ChoiceAnswer & \AddComment \\
\quad Friction angle & \ChoiceAnswer & \AddComment \\
\quad Diameter D70 & \ChoiceAnswer & \AddComment \\
\quad Permeability X & \ChoiceAnswer & \AddComment \\
\quad Shear strength model & \ChoiceAnswer & \AddComment \\
\quad \quad None & \ChoiceAnswer & \AddComment \\
\quad \quad C phi & \ChoiceAnswer & \AddComment \\
\quad \quad Stress table & \ChoiceAnswer & \AddComment \\
\quad \quad Pseudo values & \ChoiceAnswer & \AddComment \\
\quad \quad Su measured & \ChoiceAnswer & \AddComment \\
\quad \quad Su calculated & \ChoiceAnswer & \AddComment \\
\quad \quad Su gradient & \ChoiceAnswer & \AddComment \\
\quad \quad Su calculated with yield & \ChoiceAnswer & \AddComment \\
\quad \quad C phi or Su calculated & \ChoiceAnswer & \AddComment \\\
\quad POP & \ChoiceAnswer & \AddComment \\
\EmptyRow

\EndTable

\subsection{DAM -- Tables -- Locations Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Copy & \ChoiceAnswer & \AddComment \\
\quad Paste & \ChoiceAnswer & \AddComment \\
\quad Fits columns & \ChoiceAnswer & \AddComment \\
\quad Edit & \ChoiceAnswer & \AddComment \\
\quad Edit Unit & \ChoiceAnswer & \AddComment \\
\quad Export & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Item selection} \\
\quad \quad All & \ChoiceAnswer & \AddComment \\
\quad \quad Main items & \ChoiceAnswer & \AddComment \\
\quad \quad Dike & \ChoiceAnswer & \AddComment \\
\quad \quad Water levels & \ChoiceAnswer & \AddComment \\
\quad \quad Design & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Main items?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Y location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad X location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Zone type & \ChoiceAnswer & \AddComment \\
\quad Forbidden zone factor [-] & \ChoiceAnswer & \AddComment \\
\quad Dike emb. material & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Dike?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Dike & \ChoiceAnswer & \AddComment \\
\quad Segment & \ChoiceAnswer & \AddComment \\
\quad Description & \ChoiceAnswer & \AddComment \\
\quad Traffic load [kN/m³] & \ChoiceAnswer & \AddComment \\
\quad Degree of consolidation [\%] & \ChoiceAnswer & \AddComment \\
\quad Minimum circle depth [m] & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Water levels?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL3 [-] & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL4 [-] & \ChoiceAnswer & \AddComment \\
\quad Penetration length [m] & \ChoiceAnswer & \AddComment \\
\quad Slope damping factor & \ChoiceAnswer & \AddComment \\
\quad PL-Line creation [-] & \ChoiceAnswer & \AddComment \\
\quad Intrusion vertical water pressure & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen bij Design?}} \\
\quad Name & \ChoiceAnswer & \AddComment \\
\quad Shoulder emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth slope [-] & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Slope adaption delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Redesign dike height & \ChoiceAnswer & \AddComment \\
\quad Redesign dike shoulder & \ChoiceAnswer & \AddComment \\
\quad Stability design method & \ChoiceAnswer & \AddComment \\
\quad Start value for design of slope & \ChoiceAnswer & \AddComment \\
\quad End value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Step value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Use new width crest & \ChoiceAnswer & \AddComment \\
\quad New width crest & \ChoiceAnswer & \AddComment \\
\quad Use new slope inside & \ChoiceAnswer & \AddComment \\
\quad New slope inside & \ChoiceAnswer & \AddComment \\
\quad Use new slope outside & \ChoiceAnswer & \AddComment \\
\quad New slope outside & \ChoiceAnswer & \AddComment \\
\quad Use new top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use the value for new allowed height of shoulder as fraction of dike height & \ChoiceAnswer & \AddComment \\
\quad New allowed height shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad New allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad Use new definition ditch & \ChoiceAnswer & \AddComment \\
\quad New width ditch bottom & \ChoiceAnswer & \AddComment \\
\quad New slope ditch & \ChoiceAnswer & \AddComment \\
\quad New depth ditch & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Item selection: All - Name -Kun je iets invullen bij de volgende kolommen?}} \\
\quad River level & \ChoiceAnswer & \AddComment \\
\quad River level low & \ChoiceAnswer & \AddComment \\
\quad Dike table height & \ChoiceAnswer & \AddComment \\
\quad Polder level & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion piping & \ChoiceAnswer & \AddComment \\
\quad Uplift criterion stability & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (river) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below top dike (polder) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder base (polder) & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below toe of dike (polder) & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset below middle of dike crest & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below middle of dike crest & \ChoiceAnswer & \AddComment \\
\quad Use PL1 offset factor below shoulder crest inside & \ChoiceAnswer & \AddComment \\
\quad PL1 offset below shoulder crest inside & \ChoiceAnswer & \AddComment \\
\quad Head PL2 & \ChoiceAnswer & \AddComment \\
\quad Head PL3 & \ChoiceAnswer & \AddComment \\
\quad Head PL4 & \ChoiceAnswer & \AddComment \\
\quad Required safety factor stability inner slope & \ChoiceAnswer & \AddComment \\
\quad Required safety factor stability outer slope & \ChoiceAnswer & \AddComment \\
\quad Required safety factor piping & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Item selection: All - Kun je iets invullen bij de volgende kolommen:}} \\
\quad X location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Y location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Dike & \ChoiceAnswer & \AddComment \\
\quad Segment & \ChoiceAnswer & \AddComment \\
\quad Description & \ChoiceAnswer & \AddComment \\
\quad Traffic load [kN/m³] & \ChoiceAnswer & \AddComment \\
\quad Degree of consolidation [\%] & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL3 [-] & \ChoiceAnswer & \AddComment \\
\quad Damping factor PL4 [-] & \ChoiceAnswer & \AddComment \\
\quad Distance to Entrypoint [m] & \ChoiceAnswer & \AddComment \\
\quad Penetration length [m] & \ChoiceAnswer & \AddComment \\
\quad Slope damping factor & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad PL-Line creation [-]} \\
\quad \quad Expert Knowledge & \ChoiceAnswer & \AddComment \\
\quad \quad Expert knowledge linear in dike & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Intrusion vertical water pressure} \\
\quad \quad DAM Standard & \ChoiceAnswer & \AddComment \\
\quad \quad Linear & \ChoiceAnswer & \AddComment \\
\quad \quad Full hydrostatic & \ChoiceAnswer & \AddComment \\
\quad \quad Hydrostatic & \ChoiceAnswer & \AddComment \\
\quad \quad Semi time dependent & \ChoiceAnswer & \AddComment \\
\quad Minimum circle depth [m] & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Zone type} \\
\quad \quad No zones & \ChoiceAnswer & \AddComment \\
\quad \quad Forbidden zones & \ChoiceAnswer & \AddComment \\
\quad Forbidden zone factor [-] & \ChoiceAnswer & \AddComment \\
\quad Dike emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder emb. material & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth slope [-] & \ChoiceAnswer & \AddComment \\
\quad Shoulder growth delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Slope adaption delta X [m] & \ChoiceAnswer & \AddComment \\
\quad Redesign dike height & \ChoiceAnswer & \AddComment \\
\quad Redesign dike shoulder & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Stability design method} \\
\quad \quad Optimized slope and shoulder adaption & \ChoiceAnswer & \AddComment \\
\quad \quad Slope adaption before shoulder adaption & \ChoiceAnswer & \AddComment \\
\quad Start value for design of slope & \ChoiceAnswer & \AddComment \\
\quad End value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Step value for design of slope & \ChoiceAnswer & \AddComment \\
\quad Use new width crest & \ChoiceAnswer & \AddComment \\
\quad New width crest & \ChoiceAnswer & \AddComment \\
\quad Use new slope inside & \ChoiceAnswer & \AddComment \\
\quad New slope inside & \ChoiceAnswer & \AddComment \\
\quad Use new slope outside & \ChoiceAnswer & \AddComment \\
\quad New slope outside & \ChoiceAnswer & \AddComment \\
\quad Use new top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New top slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad New base slope shoulder & \ChoiceAnswer & \AddComment \\
\quad Use the value for new allowed height of shoulder as fraction of dike height & \ChoiceAnswer & \AddComment \\
\quad New allowed height shoulder & \ChoiceAnswer & \AddComment \\
\quad Use new allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad New allowed distance toe-ditch & \ChoiceAnswer & \AddComment \\
\quad Use new definition ditch & \ChoiceAnswer & \AddComment \\
\quad New width ditch bottom & \ChoiceAnswer & \AddComment \\
\quad New slope ditch & \ChoiceAnswer & \AddComment \\
\quad New depth ditch & \ChoiceAnswer & \AddComment \\
\quad Surface line & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Validation messages Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen?}} \\
\quad Severity & \ChoiceAnswer & \AddComment \\
\quad Message & \ChoiceAnswer & \AddComment \\
\quad Subject & \ChoiceAnswer & \AddComment \\
\quad Repair & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Log Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen?}} \\
\quad Message & \ChoiceAnswer & \AddComment \\
\quad Subject & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{Analysis type}
\BeginTable
\Instructions{Open de tutorial en selecteer Adapt geometry voor Analysis type.} \\
\quad Is de aangepaste geometrie hetzelfde als in release 19.1.2? & \ChoiceAnswer & \AddComment \\
\EndTable

\chapter{DAM -- Calculation \& Results}
\section{DAM -- Piping Modulus}
\subsection{DAM -- Tables -- Design calculations Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Copy & \ChoiceAnswer & \AddComment \\
\quad Paste & \ChoiceAnswer & \AddComment \\
\quad Fits columns & \ChoiceAnswer & \AddComment \\
\quad Edit & \ChoiceAnswer & \AddComment \\
\quad Edit Unit & \ChoiceAnswer & \AddComment \\
\quad Export & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen?}} \\
\quad Location & \ChoiceAnswer & \AddComment \\
\quad Scenario & \ChoiceAnswer & \AddComment \\
\quad Calculation result & \ChoiceAnswer & \AddComment \\
\quad X location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Y location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Analysis & \ChoiceAnswer & \AddComment \\
\quad Uplift & \ChoiceAnswer & \AddComment \\
\quad Profile Name & \ChoiceAnswer & \AddComment \\
\quad Profile probability [÷] & \ChoiceAnswer & \AddComment \\
\quad Stability model [-] & \ChoiceAnswer & \AddComment \\
\quad Safety factor [-] & \ChoiceAnswer & \AddComment \\
\quad Shoulder height [m] & \ChoiceAnswer & \AddComment \\
\quad X Bottom new slope [m] & \ChoiceAnswer & \AddComment \\
\quad Z Bottom new slope [m] & \ChoiceAnswer & \AddComment \\
\quad Required safety factor [-] & \ChoiceAnswer & \AddComment \\
\quad River level & \ChoiceAnswer & \AddComment \\
\quad River level low & \ChoiceAnswer & \AddComment \\
\quad Dike table height & \ChoiceAnswer & \AddComment \\
\quad Slope damping factor & \ChoiceAnswer & \AddComment \\
\quad Dike length [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 uplift [-] & \ChoiceAnswer & \AddComment \\
\quad PL3 head adjusted [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 location uplift (X-local) [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 location uplift (X-global) [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 location uplift (Y-global) [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift [-] & \ChoiceAnswer & \AddComment \\
\quad PL4 head adjusted [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift (X-local) [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift (X-global) [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift (Y-global) [m] & \ChoiceAnswer & \AddComment \\
\quad Entry point piping X local [m] & \ChoiceAnswer & \AddComment \\
\quad Entry point piping X global [m] & \ChoiceAnswer & \AddComment \\
\quad Entry point piping Y global [m] & \ChoiceAnswer & \AddComment \\
\quad Exit point piping X local [m] & \ChoiceAnswer & \AddComment \\
\quad Exit point piping X global [m] & \ChoiceAnswer & \AddComment \\
\quad Exit point piping Y global [m] & \ChoiceAnswer & \AddComment \\
\quad Seepage length piping [m] & \ChoiceAnswer & \AddComment \\
\quad Uplift safety factor [-] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion DeltaHc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion reduced DeltaHc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Uplift safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Uplift hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Uplift DeltaHc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Heave safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Heave hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Heave gradient (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Piping safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Piping hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Effective stress exit point(WBI) [kN/m²] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion CCreep (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Result message & \ChoiceAnswer & \AddComment \\
\quad Exception message & \ChoiceAnswer & \AddComment \\
\quad Notes & \ChoiceAnswer & \AddComment \\
\quad Number of iterations & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Evaluation}\\
\quad \quad Accepted & \ChoiceAnswer & \AddComment \\
\quad \quad Rejected & \ChoiceAnswer & \AddComment \\
\quad \quad Not evaluated & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- 2D geometry}
\BeginTable
\Instructions{Open de tutorial.} \\
\quad Kan je de berekening uitvoeren als No adaptation geselecteerd is? & \ChoiceAnswer & \AddComment \\
\quad Is na berekening een resultaat cirkel aanwezig in de Cross section tab? & \ChoiceAnswer & \AddComment \\
\quad Is na berekening een stix file aanwezig in de berekenings directory? & \ChoiceAnswer & \AddComment \\
\EndTable

\section{DAM -- Stability Modulus}
\subsection{DAM -- Tables -- Design calculations Tab}
\BeginTable
\multicolumn{3}{l}{\underline{Werken de volgende knoppen?}} \\
\quad Copy & \ChoiceAnswer & \AddComment \\
\quad Paste & \ChoiceAnswer & \AddComment \\
\quad Fits columns & \ChoiceAnswer & \AddComment \\
\quad Edit & \ChoiceAnswer & \AddComment \\
\quad Edit unit & \ChoiceAnswer & \AddComment \\
\quad Export & \ChoiceAnswer & \AddComment \\
\EmptyRow
\multicolumn{3}{l}{\underline{Zie je de volgende kolommen?}} \\
\quad Location & \ChoiceAnswer & \AddComment \\
\quad Scenario & \ChoiceAnswer & \AddComment \\
\quad Calculation result & \ChoiceAnswer & \AddComment \\
\quad X location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Y location (RDS) [m] & \ChoiceAnswer & \AddComment \\
\quad Analysis & \ChoiceAnswer & \AddComment \\
\quad Uplift & \ChoiceAnswer & \AddComment \\
\quad Profile Name & \ChoiceAnswer & \AddComment \\
\quad Profile Probability [÷] & \ChoiceAnswer & \AddComment \\
\quad Stability Model [-] & \ChoiceAnswer & \AddComment \\
\quad Safety factor [-] & \ChoiceAnswer & \AddComment \\
\quad Shoulder height [m] & \ChoiceAnswer & \AddComment \\
\quad X Bottom new slope [m] & \ChoiceAnswer & \AddComment \\
\quad Z Bottom new slope [m] & \ChoiceAnswer & \AddComment \\
\quad Required safety factor [-] & \ChoiceAnswer & \AddComment \\
\quad River level & \ChoiceAnswer & \AddComment \\
\quad River level low & \ChoiceAnswer & \AddComment \\
\quad Dike table height & \ChoiceAnswer & \AddComment \\
\quad Slope damping factor & \ChoiceAnswer & \AddComment \\
\quad Dike length [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 uplift [-] & \ChoiceAnswer & \AddComment \\
\quad PL3 head adjusted [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 location uplift (X-local) [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 location uplift (X-global) [m] & \ChoiceAnswer & \AddComment \\
\quad PL3 location uplift (Y-global) [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift [-] & \ChoiceAnswer & \AddComment \\
\quad PL4 head adjusted [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift (X-local) [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift (X-global) [m] & \ChoiceAnswer & \AddComment \\
\quad PL4 uplift (Y-global) [m] & \ChoiceAnswer & \AddComment \\
\quad Entry point piping X local [m] & \ChoiceAnswer & \AddComment \\
\quad Entry point piping X global [m] & \ChoiceAnswer & \AddComment \\
\quad Entry point piping Y global [m] & \ChoiceAnswer & \AddComment \\
\quad Exit point piping X local [m] & \ChoiceAnswer & \AddComment \\
\quad Exit point piping X global [m] & \ChoiceAnswer & \AddComment \\
\quad Exit point piping Y global [m] & \ChoiceAnswer & \AddComment \\
\quad Seepage length piping [m] & \ChoiceAnswer & \AddComment \\
\quad Uplift safety factor [-] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion DeltaHc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion reduced DeltaHc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Uplift safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Uplift hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Uplift DeltaHc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Heave safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Heave hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Heave gradient (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Piping safety factor (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Piping hc (WBI) [m] & \ChoiceAnswer & \AddComment \\
\quad Effective stress exit point(WBI) [kN/m²] & \ChoiceAnswer & \AddComment \\
\quad Backward erosion CCreep (WBI) [-] & \ChoiceAnswer & \AddComment \\
\quad Result message & \ChoiceAnswer & \AddComment \\
\quad Exception message & \ChoiceAnswer & \AddComment \\
\quad Notes & \ChoiceAnswer & \AddComment \\
\quad Number of iterations & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\quad Evaluation} \\
\quad \quad Accepted & \ChoiceAnswer & \AddComment \\
\quad \quad Rejected & \ChoiceAnswer & \AddComment \\
\quad \quad Not evaluated & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Waternet creator}
\BeginTable
\Instructions{Open TestWaternet\_v24\_1DProfile.damx van /trunk/test/TestDataForTestDocument/WaternetCreator, bereken en open de gecreëerde stix bestanden in D-Stability.} \\
\multicolumn{3}{l}{\underline{Worden de juiste waternet lines gemaakt zoals beschreven in de handleiding voor de volgende opties:}} \\
\quad DAM Standard & \ChoiceAnswer & \AddComment \\
\quad Full hydrostatic & \ChoiceAnswer & \AddComment \\
\quad Hydrostatic & \ChoiceAnswer & \AddComment \\
\quad Linear & \ChoiceAnswer & \AddComment \\
\quad Semi time dependent & \ChoiceAnswer & \AddComment \\
\Instructions{Ga naar tab Tables - Design Calculations, selecteer profiel SoilProfile\_TwoInbetweenAquifers van locatie SemiTimeDependent en klik op Open calculation onder Properties} \\
\multicolumn{3}{l}{\underline{Zijn de labels van de waternet lines en headlines als volgt:}} \\
\quad \quad Phreatic line (PL 1) & \ChoiceAnswer & \AddComment \\
\quad \quad Headline 2 (PL 2) & \ChoiceAnswer & \AddComment \\
\quad \quad Headline 3 (PL 3) & \ChoiceAnswer & \AddComment \\
\quad \quad Headline 4 (PL 4) & \ChoiceAnswer & \AddComment \\
\quad \quad Waternet line in-between aquifer top (1) & \ChoiceAnswer & \AddComment \\
\quad \quad Waternet line in-between aquifer bottom (1) & \ChoiceAnswer & \AddComment \\
\quad \quad Waternet line in-between aquifer top (2) & \AddComment & \AddComment \\
\quad \quad Waternet line in-between aquifer bottom (2) & \ChoiceAnswer & \AddComment \\
\quad \quad Penetration zone lower aquifer & \ChoiceAnswer & \AddComment \\
\quad \quad Waternet line lower aquifer & \ChoiceAnswer & \AddComment \\
\quad Zijn er 2 waternet lines boven en onder de tussen aquifer lagen? & \ChoiceAnswer & \AddComment \\
\multicolumn{3}{l}{\underline{Zijn de coördinaten van de waternet line die geassocieerd is met de phreatic line als volgt:}} \\
\quad 0;-9.999 & \ChoiceAnswer & \AddComment \\
\quad 31.329;-9.999 & \ChoiceAnswer & \AddComment \\
\Instructions{Open TestWaternet\_v24\_1DProfile.damx van /trunk/test/TestDataForTestDocument/WaternetCreator en voer de berekening uit. Open de stix file voor SoilProfile\_NoInbetweenAquifer.} \\
\quad Bevat het waternet geen waternet lines verbonden aan PL 4 voor de hoogste zandlaag (in de dijk)? & \ChoiceAnswer & \AddComment \\
\quad Bevat het waternet 2 waternet lines verbonden aan PL 4 voor de tweede zandlaag? & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Stix File Writer}
\subsubsection{Input stix file}
\BeginTable
\Instructions{Open de tutorial.} \\
\quad Wordt een input stix file gemaakt na een Bishop berekening? & \ChoiceAnswer & \AddComment \\
\quad \quad Heeft deze input stix file een grid onder het Calculate menu in D-Stability? & \ChoiceAnswer & \AddComment \\
\quad \quad Is de safety factor na berekening in D-Stability niet altijd hetzelfde als in DAM? & \ChoiceAnswer & \AddComment \\
\quad Wordt \textbf{geen} input stix file gemaakt na een Uplift-Van berekening met Calculation grid als Search Method? & \ChoiceAnswer & \AddComment \\
\quad Wordt een input stix file gemaakt na een Uplift-Van berekening met Bee Swarm als Search Method? & \ChoiceAnswer & \AddComment \\
\quad \quad Is de safety factor na berekening in D-Stabilit niet altijd hetzelfde als in DAM? & \ChoiceAnswer & \AddComment \\
\EndTable
\subsubsection{Results stix file}
\BeginTable
\Instructions{Open Actualisatie.damx van /trunk/src/Dam/Deltares.Dam.IntegrationTests/TestData/StabilityOutside1DProfileTest en voer een berekening uit. Open vervolgens de gecreëerde stix file in D-Stability.} \\
\quad Bevat de stix file de 2D geometrie, waternet lines en berekenings grid? & \ChoiceAnswer & \AddComment \\
\quad Heeft de stix file de juiste sigma tau tabellen? & \ChoiceAnswer & \AddComment \\
\quad Hebben de soils/materialen de juiste shear stress mode toegekend? & \ChoiceAnswer & \AddComment \\
\quad Kun je de berekening in D-Stability uitvoeren? & \ChoiceAnswer & \AddComment \\
\quad Is de berekende safety factor hetzelfde als in DAM? & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- 2D geometry}
\BeginTable
\Instructions{Open de tutorial.} \\
\quad Kan je de berekening uitvoeren als No adaptation geselecteerd is? & \ChoiceAnswer & \AddComment \\
\quad Is na berekening een resultaat cirkel aanwezig in de Cross section tab? & \ChoiceAnswer & \AddComment \\
\quad Is na berekening een stix file aanwezig in de berekenings directory? & \ChoiceAnswer & \AddComment \\
\EndTable

\subsection{DAM -- Results}
\BeginTable
\Instructions{Open de tutorial.} \\
\quad Is de slip circle zichtbaar in de cross section tab na een berekening met Bishop? & \ChoiceAnswer & \AddComment \\
\quad Is een dubbele slip circle zichtbaar in de cross section tab na een berekening met Uplift-Van? & \ChoiceAnswer & \AddComment \\
\EndTable

\BeginTable
\Instructions{Open de tutorial. Selecteer alle locaties, Stability inside, Bishop, Automatic grid en No adaptation. Voer de berekening uit.} \\
\quad Is een resultaat beschikbaar voor alle locaties en scenarios (DWP\_10 wordt uitgevoerd voor 3 scenario's)? & \ChoiceAnswer & \AddComment \\
\EndTable

\end{Form}
\end{document}
