\chapter{Calculation}\label{sec:USCalculation}

There a different calculations possible, depending on the type of the project.

\section{Perform Design calculation - No adaption}\label{sec:USCalculationDesignNoAdaption}
It should be possible to make a calculation in a Design project based on the input parameters. 
The most important outcome of the calculation are the safety factors.

\section{Perform Design calculation - With adaption}\label{sec:USCalculationDesignWithAdaption}
It should be possible to make calculations in a Design project with adaption of the geometry of the dike,
if the calculated safety factor is lower than the required safety factor. 
The adaptation must have the options to increase the crest, change the angle of the slope, 
create a berm or a combination of these options according to given settings.

\section{Perform Calamity calculation}\label{sec:USCalculationCalamity}
It should be possible to make a calculation in a Calamity project. 
After importing a time series of water levels the safety factors will be calculated for all locations and for all time steps.

