\chapter{Create Project}\label{sec:USOpenProject}

The user can create a project by defining different sources, see \autoref{sec:USDataFormat} and \autoref{sec:USDataCombi}

\section{Create Design project}\label{sec:USCreateDesignProject}
When the data sources are correctly defined, the user should be able to create a Design project. 
If the creation fails a log should display the problems encountered.
This project can be used to perform a calculation of safety factors in different locations. \newline
It is also possible to make a calculation where the user defines a required safety factor.
When this value is not met with the initial calculation, then a new surfaceline is determined, 
which will result in a safety factor that complies to the required value. 

\section{Create Calamity project}\label{sec:USCreateCalamityProject}
When the data sources are correctly defined the user should be able to create a Calamity project.
If the creation fails a log should display the problems encountered.
This project can be used to perform a calculation of safety factors during a certain amount of time. 
A time series of waterlevels has to be provided for this calculation.

\section{DAMLive configuration}\label{sec:USDAMLiveConfiguration}
When the data sources are correctly defined and a separate configuration file for the sensor data is provided, 
the user should be able to create a DamLive configuration. 
If the creation fails a log should display the problems encountered.
This configuration can be used in DamLive, 
which will be part of an operational system, 
assessing in real-time the condition of the dikes in the specified locations. 
An example of such an operational system is FEWS.


