Index: DamClients/DamUI/trunk/doc/DAM UI - Functional Design/DataCombination.tex
===================================================================
diff -u -r2077 -r2082
--- DamClients/DamUI/trunk/doc/DAM UI - Functional Design/DataCombination.tex	(.../DataCombination.tex)	(revision 2077)
+++ DamClients/DamUI/trunk/doc/DAM UI - Functional Design/DataCombination.tex	(.../DataCombination.tex)	(revision 2082)
@@ -1,16 +1,16 @@
 \chapter{Data combination}\label{sec:USDataCombi}
 
-\section{REQ Data.Generation.Geometry}\label{sec:REQDataGenerationGeometry}
-The \ProgramName can combine a surface line with a subsoil scenario. The result is a geometry, usable for the failure mechanism Macrostability. 
+\section{Data extraction}\label{sec:DataExtraction}
 
-
-\section{Location}\label{sec:location}
 The locations are described with a name and RD-coordinates; a point element in GIS files.
 Each location is connected to a crosssection; a line element in GIS files.
 
 The combination of data from GIS files is made based on these point and line elements.\\
 If the input data is available in a GIS file with line elements the data is collected at the intersection of the crosssection with the line element, see \autoref{fig:GISLine}.
 
+When a parameter is available in a line shape, \ProgramName will check, during import of data, if the cross section of a location intersects the shapefile of the parameter. When so, this parameter is connected to this location.
+If a cross section intersects more than one line of the shapefile, no parameters is connected at all and a message is given that this location is not imported.
+
 \begin{figure}[H]
 	\centering
 		\includegraphics[width=0.7\textwidth]{pictures/GISLine.png}
@@ -29,6 +29,10 @@
 
 If the inputdata is not available in GIS files, all input data can be linked to each location via a table (csv-format).
 
+\section{GeoemetryGeneration}\label{sec:GeometryGeneration}
+
+The \ProgramName can combine a surface line with a subsoil scenario. The result is a geometry, usable for the failure mechanism Macrostability. 
+
 \section{Subsoil}
 The subsoil model is made up of the following elements:
 \begin{itemize}
