Index: dam engine/trunk/doc/Dam Engine - Technical Design/DAM Engine - Technical Design.tex
===================================================================
diff -u -r220 -r333
--- dam engine/trunk/doc/Dam Engine - Technical Design/DAM Engine - Technical Design.tex	(.../DAM Engine - Technical Design.tex)	(revision 220)
+++ dam engine/trunk/doc/Dam Engine - Technical Design/DAM Engine - Technical Design.tex	(.../DAM Engine - Technical Design.tex)	(revision 333)
@@ -369,7 +369,7 @@
 Within DAM we have 3 types of scenarios:
 \begin{itemize}
 	\item Subsoil scenario
-	\item Load scenario
+	\item Design scenario
 	\item Regional scenario
 \end{itemize}
 
@@ -378,8 +378,8 @@
 Used as part of the stochastic subsoil schematization. 
 A subsoil scenario defines a possible 1D- or 2D-profile that applies to a certain location.
 
-\subsection{Load scenario}
-\label{sec:LoadScenario}
+\subsection{Design scenario}
+\label{sec:DesignScenario}
 Used for Design calculation. 
 In a design calculation a new surfaceline is designed for a location, based on a target failure factor (e.g. due to new requirements), or load (e.g. a higher waterlevel).
 
@@ -417,15 +417,15 @@
 \paragraph*{SoilSegment}
 A soil segment contains the subsoil data for a specific failure mechanism.
 \paragraph*{SurfaceLine}
-A surfaceline describes the dike profile in a specific location. In the Design calculation it can also be the new dike profile, which can meet design criteria in a specific load scenario.
+A surfaceline describes the dike profile in a specific location. In the Design calculation it can also be the new dike profile, which can meet design criteria in a specific design scenario.
 \paragraph*{WaternetOptions}
 The options that support the creation of a waternet in a specific location.
 \paragraph*{DesignOptions}
 The options that will be used in the Design calculation (e.g.\ how to design a shoulder when needed).
 \paragraph*{SensorData}
 The sensor data can be used to define a waternet based on live sensor data. This sensor data holds information about ID and location of the sensor. The actual sensor readings are defined as timeseries readings for each sensor in each location.
-\paragraph*{LoadScenario}
-Used for Design calculation. A load scenario contains the following items:
+\paragraph*{DesignScenario}
+Used for Design calculation. A design scenario contains the following items:
 \begin{itemize}
 	\item Riverlevel low
 	\item Riverlevel high
